Version 7.2
     - Port Mirroring support
     - IPM support
     - New bridge support (RFC2674)
Version 7.1
     - Accton support were added
     - Strataswitch support was added
     - Bug fixing
Version 7.0
     - Multivendor support
Version 6.4
     - Support of 8900
Version 6.3
     - Support of M2400 (generic version)
Version 6.2
     - Support of M2400 (non-generic version)
Version 6.1.1

   1. Bugs fixing.

   2. New features:

     - Support for Apollo-Pro 2 (Apollo Giga)
     - HPOV support using HPOVPlugIn kit

     - Uninstall
     - Install search default files and directory for Java interpreter / browser
       etc..
     - Install new look
     - Setup applications to change installed attributes without reinstall the
       system

     - Initial Screen new look.
     - Option key for configuration options and for trap monitor
     - RADLAN homepage reference from applet.
     - Cascade Window button to arrange screens
     - Quick open of “Edit Device List” Screen” using CTRL + D
     - DNS search. You can call device’s zoom by name or by IP address

     - When a trap arrive the ConfigMaster will beep, you can stop the beeping
     - Trap's can be saved to a file <ConfigMaster dir>/Nms/Configuration/traps.dat
     - The number of traps appearing on screen is limited and can be
       configured. If more traps arrive, the oldest are written to a file.
       The number of traps in this file is limited and configurable as well.
     - Double Click on a trap in the traps screen, will bring the zoom of the
       sending device.

     - Many shortcut buttons on zoom toolbar (Ports and VLANs parameters and
       statistics etc.)
     - Improved look for the devices on the zoom
     - In case off  “RE failure” or “Power Supply Failure” a beep and an error
       will arouse
     - Double click on a port for the port parameters screen
     - Double click on a VLAN button for the VLAN parameters screen
     - Multiple ports adding to a VLAN

     - Graph's sample time and presentation units
     - Button to show/hide Graph’s control panel
     - Click on graph item presents its value and name
     - New attractive colors for graph items
     - New Graph Type – STACKING AREA
     - Counters list is now alphabetical sorted

     - Keyboard support for toolbars (CTRL-U = update, ESC = cancel etc.
       see help topic “Shortcuts” or buttons ToolTips for further information)
     - Table keys (indexes) freeze when scrolling
     - Table allows multi line selection and group actions
     - Tables cell can now show multi line data
     - SHIFT - mouse = right click on port
     - Improved automatic correction and leading in text fields for IP, IPX etc.

     - New features and  look for FILE menu screens, including external TFTP
       support and progress bar
     - Changes that require device reset for taking place are
       invoking a reset dialog automatically (Send Configuration
       to device , Update Device Software and Device tuning)
     - Device Reset - Notify the user when device is up
     - Polling Configuration – improved screen, more options
     - Device Configuration – S-416 is now named S-164
     - Port Parameters – now called port properties and includes important
       new information.
     - Threshold Table – now under ALARM menu. Improved layout for insert
     - Refresh Version – new option under SERVICES menu. Checks if the
       device’s GRE version is the same as handled by this current zoom.
       If not, offers to close current zoom and reopen with proper version.
     - New look (with tabs) fhe following screens:
       device tuning, global parameters and port properties

     - Enhanced TFTP
     - No file association for help on NT
     - Screens titles show the device name or IP and changes automatically
       if device’s name is changed in General Parameters screen
     - Errors now contain a prefix with time and date


Version 6.0 released: 14/12/1998

   Features:
     - A new application that support SNMP TFTP etc.
     - Support for APOLLO-PRO version 2 and above


