
      	D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter

	Installation for NetWare Server v4.10, v4.11, v4.2
                  

 Contents
 --------
    - Compatibility List
    - Getting Started
       - First time installation from the install menu
       - The other time installation from the install menu
       - Modifying an existing NetWare 4.x Server

 Compatibility List
 ------------------
      Because this driver  follows  Novell  ODI  Driver Specification
      version 3.31, the NetWare version 4.10 NetWare server must be
      patched to work with this driver. The servers of NetWare version
      4.11 and above do not need to be patched. The patching method is
      described as below:

       1. Copy LOADER.EXE and LSWAP.EXE to the NetWare 4.10 server
          directory.

       2. Execute LSWAP.EXE at MS-DOS prompt from server directory.

          Usage: LSWAP [loaderFilePath [serverFilePath]]
                 Default loaderFilePath = C:\NWSERVER\LOADER.EXE
                 Default serverFilePath = C:\NWSERVER\SERVER.EXE

        PS. Both LSWAP.EXE and LOADER.EXE files provide by Novell.

       ****************************************************************
       Note: This ODI update is for English only.
       ****************************************************************

       Before installing, make sure the following items have been
       completed.

       410PTx.EXE (Where "x" is 6 or higher) must be installed on
       NetWare v4.10 file servers prior to installing ODI driver.
       Without this patch the following message may be displayed
       when NBI.NLM loads.

       "Warning: This version of NetWare does not support protected mode
       BIOS accesses. Without a loader patch some PCI drivers may fail."

 Getting Started
 ---------------
    First time installation from the install menu
    ---------------------------------------------
       1. Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

       2. Execute "LOAD INSTALL" after booting up.  Type,
          : LOAD INSTALL

       3. Select "Driver Options", -> "Configure network drivers", and
          -> "Select a driver".

       4. Press <Insert> key to install an unlisted driver.

       5. Please insert released driver CD into CD-ROM drive.

       6. Press <F3> to specify a different <PATH>. <PATH> is a directory
          which includes both DLH5X.LAN and DLH5X.LDI

          Ex. <CD drive>:\NETWARE\32BITLAN

       7. Select an adapter which you want to install.	
          example:
		Suppose your adapter is DFE-550TX, you should
	  	select "DLH5X.LAN D-Link DFE-550TX FAST Ethernet 10/100 Adapter".
          
       8. Specify "SLOT", "Media and Line Speed" and "Node Address"
          if necessary.

       9. Select "Save parameters and load driver" after configuring
          adapter setting.

       10. NetWare server will load/bind driver automatically.


    The other time installation from the install menu
    -------------------------------------------------
        1. Start the NetWare Server.

           > CD \NWSERVER
           > SERVER

        2. Execute "LOAD INSTALL" after booting up.  Type,
           : LOAD INSTALL

        3. Select "Driver Options", -> "Configure network drivers", and
           -> "Select a driver".

        4. Select an adapter which you want to install in Select a driver windows.
	   example:
		Suppose your adapter is DFE-550TX, you should
	  	select "DLH5X.LAN D-Link DFE-550TX FAST Ethernet 10/100 Adapter".

        5. Specify "SLOT", "Media and Line Speed" and "Node Address"
           if necessary.

        6. Select "Save parameters and load driver" after configuring adpter
           setting.

        7. NetWare server will load/bind driver automatically.


    Modifying an existing NetWare 4.x Server
    ----------------------------------------
        1. Make a sub-directory NLMS.OLD under NWSERVER directory.

           Ex. >MD \NWSERVER\NLMs.OLD

        2. Save NBI.NLM, MSM.NLM and ETHERTSM.NLM to NLMS.OLD
           sub-directory. (v4.10, v4.11 server only)

	3. Get NLM files from NOVELL website and put them in floppy disk.

        4. Please insert release driver CD into CD-ROM drive.

        5. Copy all provided NLM and LAN files into your dos directory
           which include SERVER.EXE. (v4.10, v4.11 server only)

            Ex. >COPY <Floppy drive>:\NETWARE\32BITLAN\NBI.NLM      C:\NWSERVER
                >COPY <Floppy drive>:\NETWARE\32BITLAN\MSM.NLM      C:\NWSERVER
                >COPY <Floppy drive>:\NETWARE\32BITLAN\ETHERTSM.NLM C:\NWSERVER
                >COPY <CD drive>:\NETWARE\32BITLAN\DLH5X.LAN   C:\NWSERVER
                >COPY <CD drive>:\NETWARE\32BITLAN\DLH5X.LDI   C:\NWSERVER

           <PATH> here is the directory where support NLMs and
           DLH5X.LAN reside.

        6. Start the NetWare Server.

            > CD \NWSERVER
            > SERVER

        7. From the Novell Server side, execute "LOAD INSTALL".  Type:
           :LOAD INSTALL
           Select <NCF files options>
           Select <Edit AUTOEXEC.NCF file>

        8. Add below item into the server's AUTOEXEC.NCF file.

           LOAD C:\NWSERVER\NBI.NLM
           LOAD C:\NWSERVER\MSM.NLM
           LOAD C:\NWSERVER\ETHERTSM.NLM

           LOAD C:\NWSERVER\DLH5X SLOT=1 FRAME=Ethernet_802.3
                NAME=DLH5X_1_E83
           BIND IPX DLH5X_1_E83 NET=xxxx

           LOAD C:\NWSERVER\DLH5X SLOT=1 FRAME=Ethernet_802.2
                NAME=DLH5X_1_E82
           BIND IPX DLH5X_1_E82 NET=xxxx

           LOAD C:\NWSERVER\DLH5X SLOT=1 FRAME=Ethernet_II
                NAME=DLH5X_1_EII
           BIND IPX DLH5X_1_EII NET=xxxx

           LOAD C:\NWSERVER\DLH5X SLOT=1 FRAME=Ethernet_SNAP
                NAME=DLH5X_1_ESP
           BIND IPX DLH5X_1_ESP NET=xxxx

        9. Restart the server again.


       Parameters supported by the DLH5X.LAN driver
       ---------------------------------------------
       SLOT     1      - Forces the driver to search for the specified board

       AUTOSENSE       - This keyword configures the adapter to conduct
                         NWay Auto-negotiation to determine the network
                         speed and the duplex mode of the network connection.
			 (Not support on DFE-550FX 100Mbps Fiber-optics Adapter)

       10MBPSHD        - Force driver to 10Mbps half duplex mode.
			 (Not support on DFE-550FX 100Mbps Fiber-optics Adapter)

       10MBPSFD        - Force driver to 10Mbps full duplex mode.
			 (Not support on DFE-550FX 100Mbps Fiber-optics Adapter)

       100MBPSHD       - Force driver to 100Mbps half duplex mode.

       100MBPSFD       - Force driver to 100Mbps full duplex mode.

       