
      	D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter
           
          NetWare Drivers Installation Overview

 Contents
 --------
    - Introduction
    - User's Guide

 Introduction
 ------------
    The PCI Family NetWare driver programs provided in this diskette.
    For installation information for various systems, please refer to the
    appropriate text file listed below.  These files are included in this
    diskette.

        File                Description
    ------------    ------------------------------------------------
    DOSODI.TXT      NetWare DOS Client installation document
    NW4XX.TXT       NetWare 4.x Server installation document
    NW5.TXT	    NetWare 5.0 Server installation document
    NW6.TXT	    NetWare 6 Server installation document
    CLIENT32.TXT    Client32 for DOS/Windows 3.1x installation document
    

 User's Guide
 ------------
    This guide lists the available NET.CFG keywords for the ODI device
    drivers. Most of these keywords are optional and use respective
    default values.

    Parameters supported by the NET.CFG for DLH5X.COM driver
    ---------------------------------------------------------
       Protocol IPX
       Bind #1

       Link Driver DLH5X
       frame Ethernet_802.3
      ;frame Ethernet_802.2
      ;frame Ethernet_II
      ;frame Ethernet_SNAP

       Protocol IPX 00 Ethernet_802.3
      ;Protocol IPX E0 Ethernet_802.2
      ;Protocol IPX 8137 Ethernet_II
      ;Protocol IPX 8137 Ethernet_SNAP

      ;NOTE:The following keywords are for DFE-550TX,DFE-580TX and DFE-530TXS		
      ;Optional driver keywords:
      ;----------------------------------------------------------------------
       AUTOSENSE          ;Autosense media type
      ;10MBPSHD           ;Force the driver to 10Mbps half duplex mode.
      ;10MBPSFD           ;Force the driver to 10Mbps full duplex mode.
      ;100MBPSHD          ;Force the driver to 100Mbps half duplex mode.
      ;100MBPSFD          ;Force the driver to 100Mbps full duplex mode.
      

      ;NOTE:The following keywords are for DFE-550FX only.		
      ;Optional driver keywords:
      ;----------------------------------------------------------------------
      ;100MBPSHD          ;Force the driver to 100Mbps half duplex mode.
       100MBPSFD          ;Force the driver to 100Mbps full duplex mode.
      
