
        D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter 
		Installation

	NetWare Client 32 for DOS/Windows 3.1x

 Contents
 ========
    - Getting Started
      - Client 32 for DOSWIN

 Getting Started
 ===============

   Client 32 for DOS/Windows 3.1x
   ------------------------------

     Method 1: Install Driver During Install
               Novell NetWare Client 32 for DOS/Windows 3.1x
     -------------------------------------------------------

    1. In DOS environment, run "INSTALL" command.

    2. Follow the installation steps of Novell NetWare Client 32.

    3. In "Select a LAN Driver Type" window, select "32-bit" LAN drivers.

    4. In "32-Bit Network Board Drivers" window, select
       "USER SPECIFIED 32 BIT DRIVER".

    5. In "Insert The Driver Disk" window, input the path
       where the LAN driver and .LDI file locate:
          ex. <CD drive>:\NETWARE\32BITLAN, if CD-ROM is used.

    6. Select the desired parameters, eg. SLOT number....
       and continue the installation procedure.

    7. In MS Windows environment, run "SETUP" command.

    8. In "ODI Driver Selection" window, select "32 bit" mode
       and "other Boards".

    9. Enter the path and filename of the ODI driver in "ODI Driver Path"
       window.

   10. Follow the installation setps of Novell NetWare Client 32.

       After the installation, a STARTNET.BAT batch file will be created.
       Please check the STARTNET.BAT file contains the right parameters.

       Content of STARTNET.BAT (for 32-bit LAN driver)
       -----------------------------------------------
       SET NWLANGUAGE=ENGLISH
       C:\NOVELL\DOSCLNT\NIOS.EXE
       LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
       LOAD C:\NOVELL\CLIENT32\CMSM.NLM
       LOAD C:\NOVELL\CLIENT32\ETHERTSM.NLM
       LOAD C:\NOVELL\CLIENT32\DLH5X.LAN FRAME=ETHERNET_802.2 SLOT=??
       LOAD C:\NOVELL\CLIENT32\DLH5X.LAN FRAME=ETHERNET_802.3 SLOT=??
       LOAD C:\NOVELL\CLIENT32\DLH5X.LAN FRAME=ETHERNET_II    SLOT=??
       LOAD C:\NOVELL\CLIENT32\DLH5X.LAN FRAME=ETHERNET_SNAP  SLOT=??
       LOAD C:\NOVELL\CLIENT32\IPX.NLM           <-- Binding driver
       LOAD C:\NOVELL\CLIENT32\CLIENT32.NLM      <-- Finding server


       Content of STARTNET.BAT (for 16-bit DOS driver)
       -----------------------------------------------
       SET NWLANGUAGE=ENGLISH
       C:\NOVELL\CLIENT32\NIOS.EXE
       C:\NOVELL\CLIENT32\LSL.COM
       C:\NOVELL\CLIENT32\N16ODI.COM
       C:\NOVELL\CLIENT32\NESL.COM
       C:\NOVELL\CLIENT32\DLH5X.COM
       LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
       LOAD C:\NOVELL\CLIENT32\PC32MLID.LAN
       LOAD C:\NOVELL\CLIENT32\TCPIP.NLM
       LOAD C:\NOVELL\CLIENT32\IPX.NLM           <-- Binding driver
       LOAD C:\NOVELL\CLIENT32\CLIENT32.NLM      <-- Finding server


       Content of NET.CFG
       ------------------
        Link Driver DLH5X
                Frame Ethernet_802.2
                Frame Ethernet_802.3
                Frame Ethernet_II
                Frame Ethernet_SNAP

        NetWare DOS Requester
                FIRST NETWORK DRIVE = F
                NETWARE PROTOCOL = NDS BIND



     NOTE: You can run the NetWare client installation program for each
           workstation type from the CLIENT directory under SYS:PUBLIC or
           directly from the CD-ROM.


     Method 2: Install Driver After Novell NetWare Client 32 for
               DOS/Windows 3.1x is Installed
     -----------------------------------------------------------

       Copy the LAN driver and LDI file to the \Novell\Client32 directory,
       and use text editor to edit STARTNET.BAT file directly.


     TroubleShooting
     ---------------
        If you experience the warning messages displayed when STARTNET.BAT
        is executed, "Command Line Parameter Prompt for DLH5X" then
        follow the instructions as below:

          Change
          LOAD C:\NOVELL\CLIENT32\DLH5X.LAN FRAME=ETHERNET_802.3
          to
          LOAD C:\NOVELL\CLIENT32\DLH5X.LAN FRAME=ETHERNET_802.3 SLOT=1
          in STARTNET.BAT, where SLOT must be the correct value as found
          by driver.
