
        D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter 

 	Packet Driver Installation for IPX SHELL


 Getting Started
 ---------------
    There are two methods for running the IPX SHELL program. They are
    described below.

    METHOD 1:
    ---------
        - If the DLH5X.SYS program is used, the following statement
          must be included in your CONFIG.SYS file:

                DEVICE = DLH5X.SYS [/option] <packet_int_no>

          <packet_int_no> is the software interrupt vector number used
                          by the packet driver program. This can be from
                          96 to 128.

          /d              Delay Initial - The driver program will not
                                          initialize the network interface
                                          card until the packet driver
                                          program is accessed by its upper
                                          layer program.

          /w              The /w parameter is for use only in the Windows
                                          environment.

          See \PKTDRV\README.TXT for addition parameters


        - Modify the content of AUTOEXEC.BAT to add DPDIPX statement:

                >DPDIPX
                >NETX
                ><change to last driver>
                >LOGIN <username>

    METHOD 2:
    ---------
        - If the DLH5X.COM program is used, follow these steps:

        - Execute DLH5X.COM by typing:

                >DLH5X [/option] <packet_int_no>
                >DPDIPX
                >NETX
                ><change to last driver>
                >LOGIN <username>

          <packet_int_no> is the software interrupt vector number used
                          by the packet driver program. This can be
                          from 96 to 128.

          /d              Delay Initial - The driver program will not
                          initialize the network interface card until
                          the packet driver program is accessed by its
                          upper layer program.

          /w              The -w parameter is for use only in the Windows
                          environment.

          See \PKTDRV\README.TXT for addition parameters

