
        D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter 

 	Packet Driver Installation for WinSock


 Getting Started
 ---------------

    Loading driver via two methods :

    METHOD 1:
    ---------
    - If the DLH5X.SYS program is used, the following statement must be
      included in your CONFIG.SYS file:

      DEVICE = DLH5X.SYS [/option] <packet_int_no>

      See \PKTDRV\README.TXT for addition parameters

      You can place this line anywhere in the CONFIG.SYS file.

    METHOD 2:
    ---------
    - If the DLH5X.COM program is used, follow these steps:

    - Execute DLH5X.COM by typing:

          >DLH5X [/option] <packet_int_no>

      See \PKTDRV\README.TXT for addition parameters

    The Secondry Step:

    - In order to run winsock under Windows enhanced mode correctly,
      you need to get "WINPKT.COM" program which can be getten from
      Internet file server sites.

      Execute "WINPKT.COM" as following:

      >WINPKT <packet_int_no>

      The "<packet_int_no>" is software interrupt number used by

      packet driver.

      This number must be the same as driver's parameters.


    - After you run winsock under Windows environment ,
      just set correct "Packet Vector" value.

    - Winsock associated programs can be ready to used.

      See also winsock distributions INSTALL.DOC file

    Examples:

      > DLH5X.COM 0x62

      > WINPKT 0x62

      Run Windows , winsock applications.


