
	D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter
		Installation for Windows XP

 Getting Started
 ---------------

    The Windows XP installation CD is needed to complete this
    installation.

    Installation Procedure under Windows XP 
    ---------------------------------------

    The following steps helps you install driver for your adapter:

     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows XP will find new hardware, and
        "Add new hardware wizard" will appear.

     5. Insert the driver diskette/CD into floppy/CDROM drive.

     6. Follow the instruction and the wizard will help you
        complete the installation.


 Driver keywords
 ---------------
     - Open 'Device Manager' in "Start" -> "Control Pannel" -> "System"
       Select "Hardware" and click "Device Manager".
       Double click the adapter, like "D-Link DFE-550TX ..." etc.
       Select "Advanced" tag.

       802.1Q/1P VLAN       You can enable it for VLAN group.
       tagging              Default: Disabled

       Connection Type      Specify the connection type for the adapter.
                            Default: Auto-Negotiation
                            (for DFE-550FX default setting is 100Base-FX
                             Full Duplex)

       GVRP                 Support GVRP and will active after 802.1Q/1P
                            VLAN tagging enable.
                            Default: Enabled

       Network Address      You can set the Ethernet address for your
                            adapter. It is not recommended to use this
                            keyword. As you know two or more adapter in
                            the same network with same Ethernet address
                            will cause a little problem.

                            When using this keyword you need to input
                            exactly 6 bytes of Ethernet address using
                            one of the following format:

				xx-xx-xx-xx-xx-xx                                                                   
                            OR                                                                                      
				xxxxxxxxxxxx                                                                        
                                                                                                                    
                            Default: read address from adapter ROM.                                                 

       VLAN ID              This value will active after 802.1Q/1P VLAN
                            tagging enable.

 	   