
	D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter
	  Installation for Windows Server 2003


 Getting Started
 ---------------

    Windows Server 2003 Driver Installation Procedure
    --------------------------------------------------------

     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows Server 2003 will find new hardware, Check "install 
        from a list or specific location (Advance)", click Next.
     
     5. Select "Search for the best driver in these locations" and 
        Check "Search removable media (floppy, CD-ROM...)", click Next.
        (Make sure that the installation disk or CD-ROM is already placed
        suitiably in floppy drive or CD drive.)
        
     6. System might show a messagebox about that this hardware has not 
        passed Windows Logo testing to verify its compatibility with this
        version of Windows, please select "Continue Anyway" to finish the 
        installation.
     
     7. After finishing the installation, there should be a new
        'Local Area Connection' will appear and the LAN card should work now.
   
 Trouble Shooting
 ----------------

    1. Everything is OK in Device Manager, but the network adapter still
       doesn't function properly. Please make sure that your Computer
       name is different from others in the same network.  You can change
       your Computer name in

       "My Computer" -> Press right key of you mouse and select "Properties"->
       "Computer Name" -> "Change" icon.

    2. Everything appears to be OK but the network adapter still doesn't
       function properly. Please make sure that the adapter is properly
       connected to a network device (ex: HUB) and the "connection type"
       for this adapter set to "Auto-negotiation" or the correct
       media type. You can check it in "My Computer" -> press right key of
       your mouse and select "properties"->"Hardware""Device Manager"
       ->"Network Adapter" -> "Properties" icons. Select "Advanced" item.


    Driver keywords:
    ----------------

       Open "Device Manager" -> "Network Adapter" -> "Properties" ->
       Double click the adapter, like "D-Link DFE-550TX ..." etc.
       Select "Advanced" item.

       802.1Q/1P VLAN       You can enable it for VLAN group.
       tagging              Default: Disabled

       Connection Type      Specify the connection type for the adapter.
                            Default: Auto-Negotiation

       GVRP                 Support GVRP and will active after 802.1Q/1p
                            VLAN tagging enable.
                            Default: Enabled

       Network Address      You can set the Ethernet address for your
                            adapter. It is not recommended to use this
                            keyword. As you know two or more adapter in
                            the same network with same Ethernet address
                            will cause a little problem.

                            When using this keyword you need to input
                            exactly 6 bytes of Ethernet address using
                            one of the following format:

				xx-xx-xx-xx-xx-xx
                            OR
				xxxxxxxxxxxx

                            Default: read address from adapter ROM.

       VLAN ID              This value will active after 802.1Q/1p VLAN
                            tagging enable.


