
        D-Link DFE-550TX 10/100 Adapter Installation
                   for WIN/TCP PathWay Access


 Getting Started
 ---------------
    - Install Win/TCP Pathway Access

    - Copy the DLH5X.DOS file into your C:\LANMAN directory.

    - Change to the C:\LANMAN directory, and create a PROTOCOL.INI text
      file with the following statements:

                [DLH5X]
                drivername = DLH5X$

    - Add the following statements to your CONFIG.SYS file:

                device=c:\lanman\DLH5X.DOS

    - Add the following statements to your AUTOEXEC.BAT file:

                ndis
                winbind
                wintcp

    - Reboot and Win/TCP Pathway should be active.