Windows 98

Installation:
-------------
Follow these steps to install the D-Link DFE-690TXD CardBus PC Card's 
driver:

    1. Start your PC, then insert the D-Link DFE-690TXD CardBus PC Card
       into an available PC Card slot in your PC .

    2. After starting Windows 98, the D-Link DFE-690TXD CardBus PC Card 
       will be detected automatically, then the Add New Hardware Wizard
       window appears.

    3. Insert the D-Link DFE-690TXD CardBus PC Card Installation disk
       into CDROM drive, then click the Next button.

    4. Select the "Search for the best driver for your device(Recommended)"
       ,radio button, then click the Next button.

    5. Select the "CDROM drives", then click the Next button.
       Windows 98 will start to search CDROM drive for network driver,
       and Windows displays the message:

            "D-Link DFE-690TXD CardBus PC Card"

    6. Click the Next button, then the Windows 98 starts to copy the
       D-Link DFE-690TXD CardBus PC Card driver to the user's hard disk.

    7. Click Finish button,
       then the Win98 starts to copy the D-Link DFE-690TXD CardBus PC Card
       driver to the user's hard disk.

    8. Restart your computer.
