Windows 2000 
    
Installation:
=============
Follow these steps to install the D-Link DFE-690TXD CardBus PC Card's 
driver:

    1. Start your PC, then insert the D-Link DFE-690TXD CardBus PC Card
       into an available PC Card slot in your PC .

    2. After starting Windows 2000, the D-Link DFE-690TXD CardBus PC Card 
       will be detected automatically, then the Found New Hardware Wizard
       window appears.

    3. Insert the D-Link DFE-690TXD CardBus PC Card Installation disk
       into CDROM drive, then click the Next button.

    4. Select the "Search for a suitable driver for my device(recommended)"
       , radio button, then click the Next button.

    5. Select the "CDROM drives" in Loacte Driver Files window,
       then click the Next button.

    6. Windows 2000 will start to search CDROM drive for network driver,
       and found a driver for this device:
            "D-Link DFE-690TXD CardBus PC Card"

       Click the Next button to install the driver.

    7. Click the Yes button, when "Digital Signature Not Found" to continue
       with the installation.

    8. Windows 2000 will start to copy the D-Link DFE-690TXD CardBus PC 
       Card driver to the user's hard disk.

    9. Click Finish button.
