Notes to the Windows XP users during the driver installation on Windows XP:

<1> Run the SETUP.EXE on CD if it does not auto-run.
<2> Please do NOT plug the DSL-200 onto your machine until you are asked to do so.

<3> In the Select ISP window, select the ISP appropriate for your account and then click Next. For example, select "PPPoA for Australia" for Australia or "PPPoA for NZ" for NZ.

<4> When you install the driver on Windows XP, you will see a few warning message windows that say: 

"The software you are installing for this hardware...  has not passed Windows XP logo testing..."

Do not worry about it.
Simply click on "Continue Anyway" button to continue with the driver installation process.
        
The reason for this message is because Our DSL-200 v1.11.0007Q driver is not built into Windows XP yet.

<5> During the installaton process, Windows XP will install three different parts of the DSL-200 driver, simply continue/follow the steps.

Whenever you see any warning messages, simply click on "Continue Anyway" button to continue/complete the installation process.

<6> When the installation is done, you will find "D-Link Dial-Up PPP Connection" icon on your Desktop. You need to double-click on it to enter your Username and Password as given to you by your ADSL service provider. Click on "Dial" to connect.

For further information, you could visit
http://www.dlink.com.au/
TECH SUPPORT > Tech Resources




