
IMPORTANT:
==========
*Please do NOT connect DSL-200 to your computer until you are asked to do so.
*You need to do the driver installation first.


For Windows XP users:
=====================
Before you install the driver on your Windows XP, you must install at least the "Windows XP Service Pack 1" first.

"Windows XP Service Pack 1" (or later) is provided by Microsoft.
"Windows XP Service Pack 1" fixes isochronous USB transfers over the USB bus. 
The first version of Windows XP has this problem. 
This problem leads to unreliable transfer over the USB connection. 
This can be seen as AAL5 errors, poor FTP throughput, missed EOC messages, and line stability if EOC messages are missed. Microsoft has released a QFE to address these issues.


For all Windows users, the driver installation steps are:
=========================================================
<1> Please do NOT plug the DSL-200 onto your computer until you are asked to do so.
<2> Run the START.EXE on CD if it does not auto-run.
<3> Select "Install Driver"
<4> Select "Next" to continue.
<5> In the "Select Service Provider" window, select the connection type appropriate for your account and then click "Next".

For example, 
select "PPPoA for Australia" for most Australian account; 
select "PPPoA for New Zealand" for most NZ account. 
Check with your ADSL service provider if unsure. There are additional useful information which you can read in the QUick Installation Guide and User's Guide.

<6> Follow the prompt for the rest of the installation. When the installation is done, you will find for example "D-Link PPPoA Connection" icon on your Desktop. 

<7> Double-click on the icon to enter your PPPoA Username and Password as given to you by your ADSL service provider. Click on "Dial" to connect.

<8> For further information, please refer to your ADSL service provider's document,
or you could visit
http://www.dlink.com.au/
TECH SUPPORT > Downloads section.