[Message]

Error                                =      "Error"
Warning                          =      "Warning"
Information                     =      "Information"
OK                                  =      "OK"
Cancel                              =      "Cancel"
Retry                                =      "Retry"

ErrorNoCard                   =       "No Ethernet Adapter found! Please check your network connections."
ErrorLAN                       =        "PC Ethernet cable is not properly connected. Please check the cable connection and make sure the router is powered on."
ErrorDHCP                     =       "Problem found on connecting to the gateway, do you want to change your IP settings to DHCP Client? DCC requires this function to continue."
ErrorDiscover                  =       "Utility can't discover the Device. Please check the cable connection and make sure the router is powered on."
ErrorPassword                =        "Your router password has been changed from factory default, please enter your current password below to progress."
ErrorForgetPSW               =        "Please push the reset button to reload from factory default."  
;ErrorDoSet                     =        "Cannot connect your router. Please check hardware again."
ErrorDoGet                     =        "Problem occurred when accessing to the internet. Please contact to your ISP for support."

ErrorEmptyUsername     =       "Please fill the entire field!"
ErrorEmptyPassword      =       "Please fill the entire field!"
ErrorRetypePassword     =       "Password is not identical!" 
ErrorIllegalIP                     =       "Invalid Address! Please specify a value between 1 and 223."
ErrorLoopbackIP             =       "IP addresses starting with 127 are not valid because they are reserved for loop back addresses. Please specify some other valid value between 1 and 223."
ErrorSubnetMaskIP         =       "You entered an invalid subnet mask. The subnet mask has to be contiguous. Please enter a valid mask."

ErrorEmptySSID             =      "Please fill the entire field!"
;ErrorWEP64                    =      "WEP64 can be entered as 5 ascii or 10 hexadecimal characters."
ErrorWEP64                    =      "The WEP key should be 5 ASCII digits"
;ErrorWEP128                    =     "WEP128 can be entered as 13 ascii or 26 hexadecimal characters."
ErrorWEP128                    =     "The WEP key should be 13 ASCII digits"
ErrorWPAPSKLength     =      "The Passphrase must be between 8 and 63 characters." 

MSGDisableProxy          =      "Proxy server for your LAN has been disabled."

[String]
Str_Label_PSW                =        "Password:  "
Str_Label_ForgetPSW          =        "[Forgotten your password]"
Str_PPTP                                   =  "PPTP  (for Europe use only)  "
Str_L2TP                                   =  "L2TP  (for specific ISPs use only)  "
Str_BigPond                              =   "BigPond Cable  (for Australia use only)  "
Str_AutoSelect               =        "Auto Select" 
Str_Disable                  =        "Disable"
Str_WPA                      ="WPA-PSK / WPA2-PSK"

[Default]

SSID                               =       "default"
Channel                           =       "6"
RouterIP                          =       "192.168.0.1"
AppTitle                          =       "D-Link Click'n'Connect"
MsgTitle                          =       "D-Link"
WEP128                            =       "No"
ManualPath                        ="Manual\\DIR-635_manual_ww.pdf"
QIGPath                           ="QIG\\DIR-635_QIG_ww.pdf"
ModelName                         ="DIR-635_A1"

 
 