DSM-330 Firmware Update Procedure
=================================

To do the update, please follow the below steps in order:

1. Unzip the update.bin file and save it to the root folder of a USB thumb drive/flash drive.
 
2. Power on the DSM-330 and press the Setup button on the remote to display the main setup menu.
 
3. Insert the USB thumb drive/flash drive with the update.bin file in the DSM-330's USB slot.
 
4. Press the following numeric sequence on the remote while at the main setup menu: 2828464631
 
5. There is no feedback for the number presses, but if done correctly, you will see an update message appear.
 
6. During this update there will be no feedback registered on the interface and should take about 10 minutes to complete.

7. You will see a completion message when the update has finished. After the message has appeared, remove power from the device for a few seconds or hold the power button for 5 seconds, then turn it back on.

8. The DSM-330 is now updated and running the latest firmware.