In order to upgrade the firmware to Version 2.10B01T01.AU.B.20071129_WEB, you must first load firmware version FIRST_AU_DVA-G3340S_singleimage_kernel_fs_V2.10B01T01.AU.B.20070529 then after that load firmware version SECOND_AU_DVA-G3340S_singleimage_kernel_fs_V2.10B01T01.AU.B.20071129.

Please ensure that you factory reset the DVA-G3340S to factory defaults after the firmware has been updated to the lastest.
Please note that you will then need to re-configure the DVA-G3340S as factory reset will clear all settings.

