$Version: HM0-0-4$                                                              ^
$Id: cli_help_msg.txt,v 1.168 2009/01/09 20:47:08 steve-lee Exp $       ^
$Source: /home/cvs/projects/source/syscon/sharedsyscon/cli/help/cli_help_msg.txt,v $^
@1~{---------------------------------------------------------------------------}^
{Operating Modes                                                               }^
{                                                                              }^
{Configuration <co>             Enter system configuration mode                }^
{Diagnostic <diag>              Enter system diagnostics mode                  }^
{Maintain <mai>                 Enter system maintenance mode                  }^
{Monitor <mo>                   Enter system monitor mode                      }^
--------------------------------------------------------------------------------^
Operating Modes                                                                 ^
                                                                                ^
Configuration <co>                                                              ^
     Enter system configuration mode.       <Example: company# co>              ^
                                                                                ^
Diagnostic <diag>                                                               ^
     Enter system diagnostics mode.         <Example: company# diag>            ^
                                                                                ^
Maintain <mai>                                                                  ^
     Enter system maintenance mode.         <Example: company# mai>             ^
                                                                                ^
Monitor <mo>                                                                    ^
     Enter system monitor mode.             <Example: company# mo>              ^
                                                                                ^
@10~{--------------------------------------------------------------------------}^
{Configuration Commands:        Configuration mode of operations               }^
{                                                                              }^
{new                            Add a new entity.                              }^
{set                            Set an attribute values of the current entity. }^
{delete                         Delete an existing entity.                     }^
{                                                                              }^
{add                            Add a 'tablized' numbers/entity under a        }^
{                               directory.                                     }^
{                                                                              }^
{remove                         Remove a 'tablized' numbers/entities under a   }^
{                               directory.                                     }^
{                                                                              }^
{change                         Change properties of certain 'tablized'        }^
{                               entities.                                      }^
{                                                                              }^
{remove                         Remove a card configuration from a slot.       }^
{                                                                              }^
{replace                        Replace a card configuration in a slot with    }^
{                               that of the card in the slot.                  }^
{                                                                              }^
{map                            Map channels of a DigitalInterface into a      }^
{                               ChannelGroup.                                  }^
{                                                                              }^
{submit                         Submit the configuration changes.              }^
{discard                        Discard the configuration changes.             }^
{time                           Set the time.                                  }^
{                               config-TimeServer-1# time 02/21/03/15:45:51    }^
{logout                         Logout the session.                            }^
{setfactory                     Set configuration to factory default.          }^
{systemuptime                   Display in days,hrs,mins,secs since powerup.   }^
{                                                                              }^
--------------------------------------------------------------------------------^
Configuration Commands:         Configuration mode of operations                ^
                                                                                ^
New                                                                             ^
     Add a new entity.                                                          ^
             <Example: config-GateWay-1# new CASSignalingGroup 2>               ^
                                                                                ^
Set                                                                             ^
     Set an attribute values of the current entity.                             ^
             <Example: config-MasterChassis-1# set name "Tenor">                ^
     Set an attribute values of the current entity to "Not Set".                ^
             <Example: config-MasterChassis-1# set name "">                     ^
                                                                                ^
Delete                                                                          ^
     Delete an existing entity.                                                 ^
             <Example: config-GateWay-1# del CASSignalingGroup 2>               ^
                                                                                ^
Add                                                                             ^
     Add a 'tablized' numbers/entities under a directory.                       ^
             <Example: config-NumberDirectories-1# add 2225555>                 ^
                                                                                ^
Remove                                                                          ^
     Remove a 'tablized' numbers/entities under a directory.                    ^
             <Example: config-NumberDirectories-1# rem 2225555>                 ^
                                                                                ^
Change                                                                          ^
     Change properties of certain 'tablized' entities.                          ^
             <Example: config-HopoffNumberDirectory-1# change 1 p 3337777>      ^
                                                                                ^
Remove                                                                          ^
     Remove a card configuration from a slot.                                   ^
             <Example: config-MasterChassis-1-SLot-1# remove>                   ^
                                                                                ^
Replace                                                                         ^
     Replace a card configuration with that of the card in the slot.            ^
             <Example: config-MasterChassis-1-SLot-1# replace>                  ^
                                                                                ^
Map                                                                             ^
     Map channels of a DigitalInterface into a ChannelGroup.                    ^
             <Example: config-DigitalInterface-1# map +6..10 cg 1>              ^
                                                                                ^
Submit                                                                          ^
     Submit the configuration changes.                                          ^
             <Example: config* sub>                                             ^
                                                                                ^
Discard                                                                         ^
     Discard the configuration changes.                                         ^
             <Example: config* disca>                                           ^
                                                                                ^
Time                                                                            ^
     Display or set system time.                                                ^
             <Example: config-TimeServer-1# time 04/05/01/15:45:00>             ^
                                                                                ^
Date                                                                            ^
     Display system date and time.                                              ^
             <Example: Quintum# date                                            ^
                                                                                ^
Alarm                                                                           ^
     Display all kinds of alarms on the system based on next argument.          ^
             <Example: Quintum# alarm                                           ^
                                                                                ^
LastCall                                                                        ^
     Display the last call that is finished on the system.                      ^
             <Example: Quintum-MasterChassis-1# lastcall                        ^
                                                                                ^
Logout                                                                          ^
     Logout the session.                                                        ^
             <Example: config# logout>                                          ^
                                                                                ^
Setfactory                                                                      ^
     Set configuration to factory default.                                      ^
             <Example: config# setfactory>                                      ^
                                                                                ^
Systemuptime                                                                    ^
     Show the time in Days, Hrs, Mins and Secs since the unit is up powerup.    ^
             <Example: config# systemuptime>                                    ^
                                                                                ^
@12~{--------------------------------------------------------------------------}^
{Time                          -a config command used to display or set the    }^
{                               time of a Tenor chassis.                       }^
{                                                                              }^
--------------------------------------------------------------------------------^
Time                           -a config command used to display or set the time^
                                of a Tenor chassis.        OR                   ^
                                A command from TimeServer prompt to reset the   ^
                                Tenor for a new software release to be loaded.  ^
                                This is a forced reboot.                        ^
                                                                                ^
                                                                                ^
@13~{--------------------------------------------------------------------------}^
{new                           -a config command to add a new entity.          }^
{                                                                              }^
--------------------------------------------------------------------------------^
new                            -a config command to add a new entity.           ^
                                                                                ^
     Example one shows how to create a new ChannelGroup SL12DV1DI1.             ^
             Example 1: config# new cg SL12DV1DI1                               ^
                                                                                ^
@14~{--------------------------------------------------------------------------}^
{set                           -a config command to set an attribute values of }^
{                                the current entity.                           }^
{                                                                              }^
--------------------------------------------------------------------------------^
set                            -a config command to set an attribute values of }^
                                the current entity.                             ^
                                                                                ^
     Example one shows how to set Primary Clock Source to Line.                 ^
             Example 1: config-MasterChassis-1# set pcs 1                       ^
                                                                                ^
@15~{--------------------------------------------------------------------------}^
{delete                        -a config command to delete an existing entity. }^
{                                                                              }^
--------------------------------------------------------------------------------^
delete                         -a config command to delete an existing entity.  ^
                                                                                ^
     Example one shows how to delete existing ChannelGroup 2.                   ^
             Example 1: config# del cg 2                                        ^
                                                                                ^
@20~{--------------------------------------------------------------------------}^
{Maintenance                    Perform maintenance operations.                }^
{                                                                              }^
{Password <passw>               Used to change password.                       }^
{Reset <reset>                  Used to reset MasterChassis; this command is   }^
{                               used under MasterChassis level only.           }^
{Timesync <timesync>            Used to retrieve the current time from a time  }^
{                               server and display the time on the screen.     }^
{                                                                              }^
--------------------------------------------------------------------------------^
Maintenance                     Perform maintenance operations.                 ^
                                                                                ^
Password                                                                        ^
     Used to change password.                                                   ^
             <Example: maintain# password>                                      ^
                                                                                ^
Reset                                                                           ^
     Used to reset MasterChassis. This command can only be executed under       ^
     MasterChassis level. Type "yes" to accept the reset.                       ^
             <Example: maintain-MasterChassis-1# reset>                         ^
                                                                                ^
Timesync                                                                        ^
     Used to retrieve the current time from a time server and display the time  ^
     on the screen.                                                             ^
     This command will display the time of the SNTP server pointed out by the   ^
     timeserver configuration.                                                  ^
             <Example: config#timesync -a                                       ^
     This command will display the time of the SNTP server pointed out by the   ^
     timeserver primaryIP address and time offset and sets the time on the Tenor^
             <Example: maintain#timesync -i <time_server_ip utcoffset>          ^
     This command will display the time of the SNTP whose ip and offset are     ^
     specified in the command.                                                  ^
     Shown in the example with an clock offset of 6hrs 15mts lag                ^
             <Example: maintain#timesync -a ipa.ipa.ipa.ipa -6:15               ^
                                                                                ^
Disconnect                                                                      ^
     Used to disconnect a call specified by a call id. A call id can be found   ^
     by executing a Calls command under the Monitor mode.                       ^
                                                                                ^
              <Example: maitain#disconnect <callid>>                            ^
                                                                                ^
@21~{--------------------------------------------------------------------------}^
{AutoSwitch                    -a diagnostic command used to show autoswitch   }^
{                               status or toggling between manual autoswitch   }^
{                               and automatic switching.                       }^
{    Syntax: Diag# as s|m                                                      }^
{            Where    s - for status and                                       }^
{                       m - for toggling manual allowed state.                 }^
{                                                                              }^
--------------------------------------------------------------------------------^
AutoSwitch                     -a diagnostic command used to show autoswitch    ^
                                status or toggling between manual autoswitch and^
                                automatic switching.                            ^
                                                                                ^
     Example one shows how to display autoswitch status.                        ^
             Example 1: diagnostic# as s                                        ^
                                                                                ^
     Example two shows how to manually toggle autoswitch.                       ^
             Example 2: diagnostic# as m                                        ^
                                                                                ^
@22~{--------------------------------------------------------------------------}^
{SetFactory                    -a config command used to reset configuration to}^
{                               Factory Default <except EthernetInterface>.    }^
{                                                                              }^
--------------------------------------------------------------------------------^
SetFactory                     -a config command used to set configuration to   ^
                                Factory Default <except EthernetInterface>.     ^
                                                                                ^
     Example one shows how to reset a Tenor to factory default settings.        ^
             Example 1: config# setfactory                                      ^
                                                                                ^
@23~{--------------------------------------------------------------------------}^
{Reset                         -a maint command used to reset a Tenor unit;    }^
{                               this is be used under MasterChassis level only.}^
{                                                                              }^
--------------------------------------------------------------------------------^
Reset                          -a maint command used to reset a Tenor unit;     ^
                                this is be used under MasterChassis level only. ^
                                Type "yes" to accept the reset command.         ^
                                                                                ^
     Example one shows how to reset a Tenor unit   .                            ^
             Example 1: maintain-MasterChassis-1# reset                         ^
                                                                                ^
@24~{--------------------------------------------------------------------------}^
{Timesync                       -a config/maint command used to retrieve the   }^
{                                current time from a time server and display   }^
{                                the sync statistics on the screen.            }^
--------------------------------------------------------------------------------^
Timesync                                                                        ^
                                -a config/maint command used to retrieve the    ^
                                 current time from a time server and display the^
                                 sync statistics on the screen.                 ^
                                                                                ^
      Example one shows how to adjust the current time from a time server       ^
      ip 131.216.18.4 when this device is lagging behind the server by 6 hrs    ^
             Example 1: maintain#timesync -a 131.216.18.4 -6:00                 ^
                                                                                ^
      Example two shows how to display the time sync statistics from a time     ^
      server ip 130.126.24.53 when this device is 5 hrs 30mts ahead.            ^
             Example 2: maintain#timesync -i 130.126.24.53 5:30                 ^
      The four possible timesync commands are                                   ^
             maintain#timesync -i                                               ^
             config#  timesync -i 130.126.24.53 5:30                            ^
             maintain#timesync -a                                               ^
             maintain#timesync -a 130.126.24.53 -5:15                           ^
                                                                                ^
@25~{--------------------------------------------------------------------------}^
{Disconnect                     -a maint command used to disconnect a call.    }^
--------------------------------------------------------------------------------^
Disconnect                                                                      ^
                                -a maint command used to disconnect a call      ^
                                 specified by a call id. A call id can be found ^
                                 by executing the Calls command under Monitor   ^
                                 Mode.                                          ^
                                                                                ^
      Example one shows how to disconnect a call with call id, <11>.            ^
             Example 1: maintain#disconnect 11                                  ^
                                                                                ^
@30~{--------------------------------------------------------------------------}^
{Monitor                       -Monitor the networks and all system components,}^
{                               including chassis, software components, trace  }^
{                               files, alarms, and CDR.                        }^
{                                                                              }^
{Alarm                         -Display active alarms and alarm history for an }^
{                               entity.                                        }^
{                                                                              }^
{Calls                         -Monitor the active calls on each chassis line  }^
{                               and channel.                                   }^
{                                                                              }^
{Status                        -Display status of certain entities.            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Monitor                        -Monitor the networks and all system components, ^
                                including chassis, software components, trace   ^
                                files, alarms, and CDR.                         ^
                                                                                ^
Alarm                          -Display active alarms and alarm history for an  ^
                                entity. This is supported from all modes.       ^
                                                                                ^
     Example one shows how to display all active alarms.                        ^
             Example 1: monitor-DigitalInterface-1# alarm a                     ^
                                                                                ^
Calls                          -Monitor the active calls on each chassis line   ^
                                and channel.                                    ^
                                                                                ^
     Example one shows all active calls on DigitalInterface 1.                  ^
             Example 1: monitor-DigitalInterface-1# calls                       ^
                                                                                ^
Status                         -Display status of certain entities.             ^
                                                                                ^
     Example one shows how monitor status of slot 5.                            ^
             Example 1: monitor-SLot-5# status                                  ^
                                                                                ^
@31~{--------------------------------------------------------------------------}^
{Alarm                         -a monitoring command used to provide access to }^
{                               Tenor alarm display.                           }^
{                                                                              }^
{    Syntax: <alarm> null|a|h|c                                                }^
{                         a - active                                           }^
{                           h - history                                        }^
{                             c - clear alarm history in the Tenor systems     }^
{                                                                              }^
--------------------------------------------------------------------------------^
Alarm                          -a command used to provide access to             ^
                                Tenor alarm display.                            ^
                                                                                ^
     Syntax: <alarm> null|a|h|c                                                 ^
                          a - active                                            ^
                            h - history                                         ^
                              c - clear alarm history in the Tenor systems      ^
                                                                                ^
@32~{--------------------------------------------------------------------------}^
{GK                            -                                               }^
{                                                                              }^
--------------------------------------------------------------------------------^
GK                             -                                                ^
                                                                                ^
@33~{--------------------------------------------------------------------------}^
{Calls                         -a monitoring command used to monitor all active}^
{                               calls.                                         }^
{                                                                              }^
--------------------------------------------------------------------------------^
Calls                          -a monitoring command used to monitor all active ^
                                calls.                                          ^
                                                                                ^
     Example two shows how to display all calls.                                ^
             Example 2: monitor-MasterChassis-1# calls                          ^
                                                                                ^
@34~{--------------------------------------------------------------------------}^
{Status                        -a monitor command used to display status of    }^
{                               certain entities.                              }^
{                                                                              }^
--------------------------------------------------------------------------------^
Status                         -a monitor command used to display status of     ^
                                certain entities.                               ^
                                                                                ^
     Example one shows how to display status of MasterChassis 1.                ^
             Example 1: monitor-MasterChassis-1# status                         ^
                                                                                ^
@40~{--------------------------------------------------------------------------}^
{Diagnostics                   -Perform the diagnostics|test operations.       }^
{                                                                              }^
{ping                          -Perform ping test to check network connectivity}^
{                                                                              }^
{as                            -Display autoswitch status or manually toggle   }^
{                               autoswitch.                                    }^
{                                                                              }^
{do                            -do command is for doing some diagnostics on DS1}^
{                               lines.                                         }^
{                                                                              }^
--------------------------------------------------------------------------------^
Diagnostics                    -Perform the diagnostics|test operations.        ^
                                                                                ^
ping                           -Perform ping test to check network connectivity.^
                                                                                ^
     Example one shows how to use ping test to check network connectivity.      ^
             Example 1: diagnostic# ping -l 123.23.42.4                         ^
                                                                                ^
as                             -Display autoswitch status or manually toggle    ^
                                autoswitch.                                     ^
                                                                                ^
     Example one shows how to display autoswitch status.                        ^
             Example 1: diagnostic# as m                                        ^
                                                                                ^
do                             -do command is to run diagnostics on DS1 lines.  ^
                                                                                ^
             Example 1: diagnostic-DigitalInterface-SL2DV1DI1# do help          ^
                                                                                ^
@42~{--------------------------------------------------------------------------}^
{Ping                          Syntax: ping  ipAddress                         }^
{                                                                              }^
--------------------------------------------------------------------------------^
Ping                                                                            ^
     Global command ping is used to send packets to a destination IP address,   ^
     receives the return packets, and measure the packet lost and round trip    ^
     time in milliseconds. This is a tool for checking the network connectivity.^
     Syntax: ping ipAddress                                                     ^
                                                                                ^
                                                                                ^
@50~{--------------------------------------------------------------------------}^
{Global commands:                                                              }^
{------------------------------------------------------------------------------}^
{help or ?                     -Display detailed or terse help                 }^
{help <topic>                  -Display detailed help for <topic>              }^
{exit or exit!                 -Go up a level or go to the top level           }^
{< or >                        -Navigate through configuration level history   }^
{show <param>                  -Optional param is; -a -b -c -d -l -o -p -t -v  }^
{logout                        -End this CLI session                           }^
{document <param>              -Display document information. param is: -r     }^
{date                          -Display current date and time on the Tenor.    }^
{Ctrl-p or Ctrl-n              -Access command history <previous or next>      }^
{                                                                              }^
--------------------------------------------------------------------------------^
Global commands:                                                                ^
--------------------------------------------------------------------------------^
help or ?                      -Display detailed or terse help                  ^
help <topic>                   -Display detailed help for <topic>               ^
exit or exit!                  -Go up a level or to the top level               ^
< or >                         -Navigate through configuration level history    ^
show <param>                   -Display settings where optional <param> is;     ^
      -a                       -Settings contained in the current level         ^
      -b                       -Settings under the current level                ^
      -c                       -Settings immediately under the current level    ^
      -d                       -Debug path                                      ^
      -l                       -All decendent entitities and attributes         ^
      -o <entity>              -Settings of all <entity name>                   ^
      -p                       -Level absolute path                             ^
      -t                       -All entitities in system                        ^
      -v                       -System revision information                     ^
logout                         -End this CLI session                            ^
document <param>               -Display document information. param is: -r      ^
Ctrl-p or Ctrl-n               -Access command history <previous or next>       ^
                                                                                ^
@51~{--------------------------------------------------------------------------}^
{Current level commands:                                                       }^
--------------------------------------------------------------------------------^
Current level commands:                                                         ^
@52~{--------------------------------------------------------------------------}^
{help                          -Display detailed help for the current level    }^
{help <level>                  -Display help on a specific configuration level }^
{help <parameter>              -Display detailed help for <parameter> <in the  }^
{                               context of the current level>                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
help                           -Display detailed help for the current level     ^
help <level>                   -Display help on a specific configuration level  ^
help <parameter>               -Display detailed help for <parameter> <in the   ^
                                context of the current level>                   ^
                                                                                ^
@53~{--------------------------------------------------------------------------}^
{show <parameter>                                                              }^
{   where <parameter is:                                                       }^
{                                                                              }^
{  -a                          -to show the attributes and immediate children  }^
{                               of the current entity                          }^
{  -b                          -to show the family tree under the current      }^
{                               entity                                         }^
{  -c                          -to show the immediate children entity instances}^
{                               under the current entity                       }^
{  -d                          -to show the current entity path with absolute  }^
{                               index                                          }^
{  -l                          -to show all decendent entities and attributes  }^
{                               under the current level                        }^
{  -o <entitytype>             -to list of all instances of the <entitytype>   }^
{  -p                          -to show the path to the current entity instance}^
{  -t                          -to show the total hierarchical entity model and}^
{                               instances                                      }^
{  -v                          -to show all the system hardware, software, and }^
{                               database version                               }^
{                                                                              }^
--------------------------------------------------------------------------------^
show <parameter>                                                                ^
   where <parameter is:                                                         ^
                                                                                ^
   -a                          -to show the attributes and immediate children of^
                                the current entity                              ^
   -b                          -to show the family tree under the current entity^
   -c                          -to show the immediate children entity instances ^
                                under the current entity                        ^
   -d                          -to show the current entity path with absolute   ^
                                index                                           ^
   -l                          -to show all decendent entities and attributes   ^
                                under the current level                         ^
   -o <entitytype>             -to list of all instances of the <entitytype>    ^
   -p                          -to show the path to the current entity instance ^
   -t                          -to show the total hierarchical entity model and ^
                                instances                                       ^
   -v                          -to show all the system hardware, software, and  ^
                                database version                                ^
                                                                                ^
@54~{--------------------------------------------------------------------------}^
{exit                          -Exit back one prompt level.                    }^
{exit!                         -Exit back to the top level.                    }^
{<                             -Navigate commands for level history. Moves to  }^
{                               previous level.                                }^
{>                             -Navigate commands for level history. Moves     }^
{                               forward to next level.                         }^
{                                                                              }^
--------------------------------------------------------------------------------^
exit                           -Exit back one prompt level.                     ^
exit!                          -Exit back to the top level.                     ^
<                              -Navigate commands for level history. Moves to   ^
                                previous level.                                 ^
>                              -Navigate commands for level history. Moves      ^
                                forward to next level.                          ^
                                                                                ^
@55~{--------------------------------------------------------------------------}^
{?                             -Display brief help for the current level       }^
{? <level>                     -Display brief help on a specific configuration }^
{                               level                                          }^
{? <parameter>                 -Display brief help for <parameter> <in the     }^
{                               context of the current level>                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
?                              -Display brief help for the current level        ^
? <level>                      -Display brief help on a specific configuration  ^
                                level                                           ^
                                                                                ^
     Example:config-DigitalInterface-1# ? dev                                   ^
                                                                                ^
? <parameter>                  -Display brief help for <parameter> <in the      ^
                                context of the current level>                   ^
                                                                                ^
     Example:config-DigitalInterface-1# ? set                                   ^
     Example:config-DeVice-1# ? devicetype                                      ^
                                                                                ^
--------------------------------------------------------------------------------^
Setting             :Value              Description                             ^
--------------------------------------------------------------------------------^
DeviceType          0                   System controller                       ^
DeviceType          1                   Line device                             ^
DeviceType          2                   DSP device                              ^
                                                                                ^
--------------------------------------------------------------------------------^
@56~{--------------------------------------------------------------------------}^
{Clear                         -a config command used to clear the entire table}^
{                               of bandwidth management.                       }^
{                                                                              }^
--------------------------------------------------------------------------------^
Clear                          -a config command used to clear the entire table ^
                                of bandwidth management.                        ^
                                                                                ^
@57~{--------------------------------------------------------------------------}^
{Logout                        -a config command used to close the session     }^
{                                                                              }^
--------------------------------------------------------------------------------^
Logout                         -a config command used to close the session      ^
                                                                                ^
                                                                                ^
@58~{--------------------------------------------------------------------------}^
{Document                       -a global command used to display document     }^
{                                information.                                  }^
--------------------------------------------------------------------------------^
Document                        -a global command used to display document      ^
                                 information.                                   ^
                                                                                ^
     Example:config#document -r                                                 ^
                                                                                ^
             <to be filled>                                                     ^
                                                                                ^
                                                                                ^
--------------------------------------------------------------------------------^
Logout                         -a config command used to close the session      ^
                                                                                ^
     Example:config-MasterChassis-1-SLot-1# logout                              ^
                                                                                ^
                                The telnet session will be immediately          ^
                                terminated                                      ^
                                                                                ^
@79~{--------------------------------------------------------------------------}^
{Submit                        -a config command used to submit any changes in }^
{                               configuration.                                 }^
{                                                                              }^
--------------------------------------------------------------------------------^
Submit                         -a config command used to submit any changes in  ^
                                configuration.                                  ^
                                                                                ^
     Example: config* sub                                                       ^
                                                                                ^
@80~{--------------------------------------------------------------------------}^
{Discard                       -a config command used to discard any changes   }^
{                                in configuration.                             }^
{                                                                              }^
--------------------------------------------------------------------------------^
Discard                        -a config command used to discard any changes in ^
                                configuration.                                  ^
                                                                                ^
     Example: config* disca                                                     ^
                                                                                ^
@81~{--------------------------------------------------------------------------}^
{Password                      -a maint command used to change the login user  }^
{                               password.                                      }^
{                                                                              }^
--------------------------------------------------------------------------------^
Password                       -a maint command used to change the login user   ^
                                password.                                       ^
     Example: maintain# password                                                ^
                                                                                ^
@82~{--------------------------------------------------------------------------}^
{Enable                                                                        }^
{                                                                              }^
--------------------------------------------------------------------------------^
Enable                                                                          ^
                                                                                ^
@83~{--------------------------------------------------------------------------}^
{Disable                                                                       }^
{                                                                              }^
--------------------------------------------------------------------------------^
Disable                                                                         ^
@84~{--------------------------------------------------------------------------}^
{Passthru                                                                      }^
{                                                                              }^
--------------------------------------------------------------------------------^
Passthru                                                                        ^
                                                                                ^
@100~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <SIte>.-                                                          }^
{    Physically, a VoIP Network consists of many sites. Each site includes from}^
{    one to several Tenor units <known as chassis'>.                           }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <SIte>.                                                             ^
     Physically, a VoIP Network consists of many sites. Each site includes from ^
     one to several Tenor units.                                                ^
@103~{-------------------------------------------------------------------------}^
{Set site <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                       (:site ID)                                     }^
{Name <name>-                   (:site name)                                   }^
{AdminContact <ac>-             (:administrator name)                          }^
--------------------------------------------------------------------------------^
Set %SIte <parameter><value>                                                    ^
   where <parameter> is:                                                        ^
                                                                                ^
&id-                                                                            ^
              (:site ID)                                                        ^
                                                                                ^
&Name-                                                                          ^
              (:site name)                                                      ^
                                                                                ^
&AdminContact-                                                                  ^
              (:administrator name)                                             ^
                                                                                ^
&EnableDBDailyBackup-                                                           ^
             (0:Diabled;Default)  (1:Enabled)                                   ^
                                                                                ^
&DBDailyBackupHour-                                                             ^
             (:hour)                                                            ^
                                                                                ^
@200~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <mc>.-                                                            }^
{    MasterChassis is a physical Tenor unit under Site.                        }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <MasterChassis>.-                                                   ^
     MasterChassis is a physical Tenor unit under Site.                         ^
@201~{-------------------------------------------------------------------------}^
{new sysls  <id>                  Create new SysLogServer named <id>           }^
{new cdrs <id>                    Create new CdrServer named <id>              }^
{new cg   <id>                    Create new ChannelGroup named <id>           }^
{                                                                              }^
--------------------------------------------------------------------------------^
new SYSLogServer <id>             Create new SysLogServer named <id>            ^
new CallDetailRecordServer <id>   Create new CdrServer named <id>               ^
new ChannelGroup <id>             Create new ChannelGroup named <id>            ^
                                                                                ^
@202~{-------------------------------------------------------------------------}^
{delete sysls <id>                Delete existing SysLogServer named <id>      }^
{delete cdrs <id>                 Delete existing CdrServer named <id>         }^
{delete cg <id>                   Delete existing ChannelGroup named <id>      }^
{                                                                              }^
--------------------------------------------------------------------------------^
delete SYSLogServer <id>          Delete existing SysLogServer named <id>       ^
delete CallDetailRecordServer<id> Delete existing CdrServer named <id>          ^
delete ChannelGroup <id>          Delete existing ChannelGroup named <id>       ^
                                                                                ^
@203~{-------------------------------------------------------------------------}^
{Set mc <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{PrimaryClockSource <pcs>-        (0:Internal)                                 }^
{                                 (1:Line,default)                             }^
{PrimaryClockLineID <pclid>-      (SlxDVyDIz:PrimaryClockLineID)               }^
{SecondaryClockSource <scs>-      (1:Line, 0:Internal,default)                 }^
{SecondaryClockLineID <sclid>-    (:SlxDVyDIz:SecondaryClockLineID)            }^
{SNMPSysLocation <snmpsl>-        (:location info for SNMP).                   }^
{SNMPSysContact <snmpsc>-         (:contact info for SNMP).                    }^
{SNMPSysDescription <snmpsd>-     (:SNMP description).                         }^
{SNMPSysName <snmpsn>-            (:System name for SNMP)                      }^
{SNMPTrapIP1 <snmptip1>-          (:SNMP Trap IP addr 1)                       }^
{SNMPTrapIP2 <snmptip2>-          (:SNMP Trap IP addr 2)                       }^
{SNMPTrapIP3 <snmptip3>-          (:SNMP Trap IP addr 3)                       }^
{SNMPPublicCommunity <snmppc>-    (:id information)                            }^
{SNMPPRivateCommunity <snmpprc>   (:id information)                            }^
{SNMPTrapCommunity <snmptc>-      (:id information)                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %MasterChassis <parameter><value>                                           ^
   where <parameter> is:                                                        ^
                                                                                ^
&PrimaryClockSource-                                                            ^
             (0:Internal)                                                       ^
             (1:Line,default)                                                   ^
                                                                                ^
&PrimaryClockLineID-                                                            ^
             (SLxDVyDIz:PrimaryClockLineID)                                     ^
                                                                                ^
&SecondaryClockSource-                                                          ^
             (0:Internal; default)                                              ^
             (1:Line )                                                          ^
                                                                                ^
&SecondaryClockLineID-                                                          ^
             (SlxDVyDIz:SecondaryClockLineID).                                  ^
                                                                                ^
&SNMPSysLocation-                                                               ^
             (:location info for SNMP).                                         ^
                                                                                ^
&SNMPSysContact-                                                                ^
             (:contact info for SNMP).                                          ^
                                                                                ^
&SNMPSysDescription-                                                            ^
             (:SNMP Description)                                                ^
                                                                                ^
&SNMPSysName-                                                                   ^
             (:System name for SNMP)                                            ^
                                                                                ^
&SNMPTrapIP1-                                                                   ^
             (:SNMP Trap IP addr 1)                                             ^
                                                                                ^
&SNMPTrapIP2-                                                                   ^
             (:SNMP Trap IP addr 2)                                             ^
                                                                                ^
&SNMPTrapIP3-                                                                   ^
             (:SNMP Trap IP addr 3)                                             ^
                                                                                ^
&SNMPPublicCommunity-    (:id information)                                      ^
                                                                                ^
&SNMPPRivateCommunity-   (:id information)					^
										^
&SNMPTrapCommunity-      (:id information)                                      ^										^
										^
@300~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <slot>.                                                           }^
{    A slot is a physical device under Site-MasterChassis <an actual slot is   }^
{    where system cards are housed within the chassis>.                        }^
{                                                                              }^
--------------------------------------------------------------------------------^
Level Name: <Slot>.                                                             ^
     A slot is a physical device under Site-MasterChassis <an actual slot is    ^
     where system cards are housed within the chassis>.                         ^
                                                                                ^
@303~{-------------------------------------------------------------------------}^
{Set slot <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{Type <t>-                      Card Type is a number identifying a card type  }^
{SlotNumber <sn>-               Numeric values ranging from 1 to 14.<Read-Only>}^
{Online <o>-                    (0:Disabled,default)                           }^
{                               (1:Enabled)                                    }^
{PhantomPowerPassthru <ppp>-    (0:Disabled,default)                           }^
{                               (1:Enabled)                                    }^
{PowerOffBypass <pob>-          (0:Disabled)                                   }^
{                               (1:Enabled)                                    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %Slot <parameter><value>                                                    ^
   where <parameter> is:                                                        ^
                                                                                ^
&Type-                                                                          ^
                   (:Read only, Card Type)                                      ^
                                                                                ^
&SlotNumber-                                                                    ^
                   (:Read only, Slot Number)                                    ^
                                                                                ^
&Online-           (0:Disabled,default)                                         ^
                   (1:Enabled)                                                  ^
&PhantomPowerPassthru-                                                          ^
                   (0:Disabled,default)                                         ^
                   (1:Enabled)                                                  ^
&PowerOffBypass- (0:Disabled,default)                                           ^
                 (1:Enabled)                                                    ^
                                                                                ^
@305~{-------------------------------------------------------------------------}^
{Remove                        -a config command, requires admin login and     }^
{                               slot prompt to remove a card configuration     }^
{                               from a slot.                                   }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                         -a config command, requires admin login and      ^
                                slot prompt to remove a card configuration      ^
                                from a slot.                                    ^
     Example one shows how to remove any card database info from a slot say 10  ^
             Example 1: config-MasterChassis-1-SLot-10# remove                  ^
                                                                                ^
@306~{-------------------------------------------------------------------------}^
{Replace                       -a config command, requires admin login, and    }^
{                               slot prompt to replace a card configuration    }^
{                               in a slot with the card in the slot.           }^
{                                                                              }^
--------------------------------------------------------------------------------^
Replace                        -a config command, requires company login, and   ^
                                slot prompt to replace a card configuration in  ^
                                a slot with the card in the slot.               ^
                                                                                ^
@400~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <dev>.                                                            }^
{    A Device is part of a system card inserted into a slot; it consists of an }^
{    Ethernet Interface <for System Controller card> or Digital Interface      }^
{    <for WAN T1 or WAN E1 cards>.                                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <Device>.                                                           ^
     A Device is part of a system card inserted into a slot; it consists of an  ^
     Ethernet Interface <for System Controller card> or Digital Interface       ^
     <for WAN T1 or WAN E1 cards>.                                              ^
                                                                                ^
@403~{-------------------------------------------------------------------------}^
{ Set dev <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{DeviceType                     Device Type                                    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %Device <parameter><value>                                                  ^
   where <parameter> is:                                                        ^
                                                                                ^
&Name-                   Device Name                                            ^
                        (:Read only)                                            ^
&DeviceType-             Device Type <Read Only>                                ^
                        (:Read only)                                            ^
&DeviceNumber-           Device Number <Read Only>                              ^
                        (:Read only)                                            ^
@500~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <ei>.                                                             }^
{    Ethernet is a Local Area Network <LAN> data network design that connects  }^
{    devices like computers, printers and terminals. It transmits data over    }^
{    twisted pair or coaxial cable at speeds of 10 or 100 Mbps. Standard RJ-45 }^
{    connection for a 10/100 base-T Ethernet connection to a switch or hub.    }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <EthernetInterface>.                                                ^
     Ethernet is a Local Area Network <LAN> data network design that connects   ^
     devices like computers, printers and terminals. It transmits data over     ^
     twisted pair or coaxial cable at speeds of 10 or 100 Mbps. Standard RJ-45  ^
     connection for a 10/100 base-T Ethernet connection to a switch or hub.     ^
                                                                                ^
@503~{-------------------------------------------------------------------------}^
{Set ei <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{name <name>-                   (:name)                                        }^
{PortNumber <pn>-               (:Read Only, Physical port number)             }^
{ManagementAccess <ma>-         (0:No access), (1:access).                     }^
{Duplex <duplex>-               (0:auto), (1:full), (2:half).                  }^
{Speed <speed>-                 (0:auto 10/100 mbps)(10:10 mbps),(100:100 mbps)}^
{IPAddress <ipa>-               (:IP address,default 0.0.0.0)                  }^
{WebServerPort <wsp>-           (:fixed port)                                  }^
{SubnetMask <sm>-               (:Subnet Mask)                                 }^
{ExternalNATIPAddr <enatipa>-   (:Tenor NAT address)                           }^
{DHCPEnabled <dhcpe>-           (0:Disabled)                                   }^
{                               (1:Enabled,default)                            }^
{PPPoEEnabled <pppee>-          (0:Disabled, default)                          }^
{                               (1:Keep Alive)                                 }^
{                               (2:On Demand)                                  }^
{PPPOERedialInterval <pppoeri>- (0:default)                                    }^
{                               (:seconds)                                     }^
{PPPOEUserName <pppoeun>-       (:user defined)                                }^
{PPPOEPassword <pppoep>-        (:user defined)                                }^
{InternalNATIPDirAttached <inatipda>-   (:directory of all IPs behind NAT)     }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %EthernetInterface <parameter><value>                                       ^
   where <parameter> is:                                                        ^
                                                                                ^
&Name-                  (:name)                                                 ^
&PortNumber-            (:Read Only, Physical port number)                      ^
                                                                                ^
&ManagementAccess-                                                              ^
             (0:Access Disabled)                                                ^
             (1:Access Enabled; Default)                                        ^
                                                                                ^
&Duplex-                                                                        ^
             (0:Auto)                                                           ^
             (1:Full)                                                           ^
             (2:Half)                                                           ^
                                                                                ^
&Speed-                                                                         ^
             (0:Auto 10/100 mbps; Default),                                     ^
             (10:10 mbps)                                                       ^
             (100:100 mbps)                                                     ^
                                                                                ^
&IPAddress-                                                                     ^
             (:IP Address,default 0.0.0.0)                                      ^
                                                                                ^
&WebServerPort-                                                                 ^
             (:Port Number)                                                     ^
                                                                                ^
&SubnetMask-                                                                    ^
             (:Subnet Mask)                                                     ^
                                                                                ^
&ExternalNATIPAddr-                                                             ^
             (:Tenor NAT address)                                               ^
                                                                                ^
&DHCPEnabled-                                                                   ^
             (0:Disabled)                                                       ^
             (1:Enabled,default)                                                ^
                                                                                ^
&PPPOEEnabled-                                                                  ^
             (0:Disabled, default)                                              ^
             (1:Keep live)                                                      ^
             (2:On Demand)                                                      ^
                                                                                ^
&PPPOERedialInterval-                                                           ^
             (0:default) (:seconds)                                             ^
                                                                                ^
&PPPOEUserName-                                                                 ^
             (:user defined)                                                    ^
                                                                                ^
&PPPOEPassword-                                                                 ^
             (:user defined)                                                    ^
                                                                                ^
&InternalNATIPDirAttached-                                                      ^
             (:NAT IP directory)                                                ^
                                                                                ^
&FilterIPDirAttached-                                                           ^
             (:Filter IP Dir)                                                   ^
                                                                                ^
&DefaultGateway-                                                                ^
             (:Default Gateway)                                                 ^
                                                                                ^
@600~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <dom>.                                                            }^
{    Domains provide a way to maintain a single directory of users in a large  }^
{    distributed-network environment. A domain is an administrative entity that}^
{    encompasses a collection of Tenor units; the units may be physically close}^
{    to each other, or separated by some distance.                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <Domain>.                                                           ^
     Domains provide a way to maintain a single directory of users in a large   ^
     distributed-network environment. A domain is an administrative entity that ^
     encompasses a collection of Tenor units; the units may be physically close ^
     to each other, or separated by some distance.                              ^
                                                                                ^
@601~{-------------------------------------------------------------------------}^
{new user                        Create new User named <id>                    }^
{                                                                              }^
--------------------------------------------------------------------------------^
new User                        Create new User named <id>                      ^
                                                                                ^
@602~{-------------------------------------------------------------------------}^
{delete usr                     Delete existing User named <id>                }^
{                                                                              }^
--------------------------------------------------------------------------------^
delete User                     Delete existing User named <id>                 ^
                                                                               }^
@603~{-------------------------------------------------------------------------}^
{Set dm <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id<id>-                        (:domain id)                                   }^
{                                                                              }^
{Name <name>-                   Used to enter a name (:name)                   }^
{AdminContact <ac>-             Used to enter contact info for administer      }^
{Company <company>-             Used to enter (:company)                       }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %Domain <parameter><value>                                                  ^
   where <parameter> is:                                                        ^
                                                                                ^
&id-               (:domain id)                                                 ^
&Name-             (:name)                                                      ^
&AdminContact-                                                                  ^
     Used to enter (:contact information).                                      ^
                                                                                ^
&Company-                                                                       ^
     Used to enter (:company name)                                              ^
                                                                                ^
@700~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <be>.                                                             }^
{    The Border Element <BE> provides access into or out of an administrative  }^
{    domain.                                                                   }^
--------------------------------------------------------------------------------^
Level Name: <BorderElement>.                                                    ^
     The Border Element provides access into or out of an administrative domain.^
                                                                                ^
@703~{-------------------------------------------------------------------------}^
{Set be <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{ServiceAddressIPAddr <beip>-     (:Border Element IP address)                 }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %BorderElement <parameter><value>                                           ^
   where <parameter> is:                                                        ^
                                                                                ^
&ServiceAddressPort-                                                            ^
          (:Service Address Port)                                               ^
                                                                                ^
&ServiceAddressIPAddr-                                                          ^
          (:default Border Element<BE> IP Addr); This Tenor in not a BE)        ^
                                                                                ^
@800~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <zone>.                                                           }^
{    A zone is defined as any number of gateways controlled by a single        }^
{    Gatekeeper.                                                               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <Zone>.                                                             ^
     Each domain consists of one or more zones.  Each zone consists of one or   ^
     more network elements. An element can be a Border Element, Gatekeeper,     ^
     Gateway, Application Server, or SIP Server, etc.                           ^
                                                                                ^
@803~{-------------------------------------------------------------------------}^
{Set zone <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                      (:read only)                                    }^
{name <name>-                  (:name)                                         }^
{AdminContact <ac>-            (:contact info for administer)                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %Zone <parameter><value>                                                    ^
   where <parameter> is:                                                        ^
                                                                                ^
&id-               (:read only)                                                 ^
&name-             (:name of zone)                                              ^
&AdminContact-                                                                  ^
                   (:contact info for administer.)                              ^
                                                                                ^
@900~{Current Level                                                            }^
{------------------------------------------------------------------------------}^
{Level Name: <gw>.                                                             }^
{    H.323 Gateway used to configure a multi-cast IP address for Gatekeeper    }^
{    discovery, or for manually assigning a Gatekeeper.                        }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <Gateway>.                                                          ^
     H.323 Gateway used to configure a multi-cast IP address for Gatekeeper     ^
     discovery, or for manually assigning a Gatekeeper.                         ^
     configuration.                                                             ^
                                                                                ^
@901~{-------------------------------------------------------------------------}^
{new cassg                      Create new CasSignalingGroup named <id>        }^
{new isdnsg                     Create new ISDNSignalingGroup named <id>       }^
{new trunkrg                    Create new TrunkCircuitRG named <id>           }^
{new lcrg                       Create new LineCircuitRG named <id>            }^
{new tp                         Create new ToneProfile   named <id>            }^
{                                                                              }^
--------------------------------------------------------------------------------^
new CASSignalingGroup           Create new CasSignalingGroup named <id>         ^
new ISDNSignalingGroup          Create new ISDNSignalingGroup named <id>        ^
new TrunkCircuitRoutingGroup    Create new TrunkCircuitRG named <id>            ^
new LineCircuitRoutingGroup     Create new LineCircuitRG named <id>             ^
new ToneProfile                 Create new ToneProfile   named <id>             ^
                                                                                ^
@902~{-------------------------------------------------------------------------}^
{delete cassg                   Delete existing CasSignalingGroup named <id>   }^
{delete isdnsg                  Delete existing ISDNSignalingGroup named <id>  }^
{delete trunkrg                 Delete existing TrunkCircuitRG named <id>      }^
{delete lcrg                    Delete existing LineCircuitRG named <id>       }^
{delete tp                      Delete existing ToneProfile named <id>         }^
--------------------------------------------------------------------------------^
delete CASSignalingGroup        Delete existing CasSignalingGroup named <id>    ^
delete ISDNSignalingGroup       Delete existing ISDNSignalingGroup named <id>   ^
delete TrunkCircuitRoutingGroup Delete existing TrunkCircuitRG named <id>       ^
delete LineCircuitRoutingGroup  Delete existing LineCircuitRG named <id>        ^
delete ToneProfile              Delete existing ToneProfile named <id>          ^
                                                                                ^
@903~{-------------------------------------------------------------------------}^
{Set gw <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Description<d>-                     (:product name, max 31 char)              }^
{OutgoingIPRouting <oipr>-           (0:H323 only)                             }^
{                                    (1:SIP only)                              }^
{ModemBypassRetentionHours <mbrh>-   (:time,default 168)                       }^
{RemoteNAT <rnat>-                   (0:disabled,default)                      }^
{                                    (1:enabled)                               }^
{RTPSourceValidation <rtpsv>-        (0:disabled,default)                      }^
{                                    (1:SSRC)                                  }^
{                                    (2:IP Address/Port #)                     }^
{ResourceThresholdHi <rth>-          (0:disable)                               }^
{                                    (1-99:max calls)                          }^
{ResourceThresholdLow <rtl>-          (0:disable)                              }^
{                                    (1-99:minimum calls)                      }^
--------------------------------------------------------------------------------^
Set %gateway <parameter><value>                                                 ^
   where <parameter> is:                                                        ^
                                                                                ^
&Description-                                                                   ^
     (:product name, max 31 char)                                               ^
&OutgoingIPRouting-                                                             ^
     (0:H323 only)                                                              ^
     (1:SIP only)                                                               ^
                                                                                ^
&ModemBypassRetentionHours-                                                     ^
     (:time,default 168)                                                        ^
                                                                                ^
&RemoteNAT-                          (0:disabled,default)                       ^
                                     (1:enabled)                                ^
&RTPSourceValidation-                (0:disabled,default)                       ^
                                     (1:SSRC)                                   ^
                                     (2:IP Address/Port #)                      ^
&ResourceThresholdHigh-          (0:disable)                                    ^
                                 (1-99:max calls)                               ^
&ResourceThresholdLow-           (0:disable)                                    ^
                                 (1-99:minimum calls)                           ^
@1000~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <nd>.                                                             }^
{    Number Directories has various telephone numbers directories. In here     }^
{    there are directories for Hopoff numbers, Hunt directory numbers, bypass  }^
{    telephone numbers and autoswitch numbers.                                 }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <NumberDirectories>.                                                ^
     Number Directories has various telephone numbers directories. In here      ^
     there are directories for Hopoff numbers, Hunt directory numbers, bypass   ^
     telephone numbers and autoswitch numbers.                                  ^
                                                                                ^
@1100~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <bnd>.                                                            }^
{    A bypass directory number is a telephone number that is automatically sent}^
{    to the trunk-side <i.e., PSTN>; it will not be routed via VoIP. Some      }^
{    examples of bypass numbers include local calls, emergency calls <911>, or }^
{    high security calls.                                                      }^
{    A bypass number should be specified in the format dialed from the line-   }^
{    side <i.e., PBX>. It is permissible to use a "*" as a wildcard digit      }^
{    <i.e., 1800*>                                                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <BypassNumberDirectory>.                                            ^
     A bypass directory number is a telephone number that is automatically sent ^
     to the trunk-side; it will not be routed via VoIP. Some examples of bypass ^
     numbers include local calls, emergency calls <911>, or high security calls.^
     A bypass number should be specified in the format dialed from the line-side^
     <i.e.,PBX>. It is permissible to use a "*" as a wildcard digit <i.e.,1800*>^
                                                                                ^
           ByPassNumber Table                                                   ^
                                                                                ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     5552222                                                        ^
                                                                                ^
     The Bypass Number that the Tenor will route automatically to the           ^
     trunk-side. This number should be specified in the format dialed from the  ^
     line-side.                                                                 ^
                                                                                ^
@1101~{------------------------------------------------------------------------}^
{new bnd                        Create new BypassNumberDirctory named <id>     }^
{                                                                              }^
--------------------------------------------------------------------------------^
new BypassNumberDirectory       Create new BypassNumberDirectory named <id>     ^
                                                                                ^
@1102~{------------------------------------------------------------------------}^
{delete bnd                     Delete existing Bypassnumber named <id>        }^
{                                                                              }^
--------------------------------------------------------------------------------^
delete BypassNumberDirectory    Delete existing Bypassnumber named <id>         ^
                                                                                ^
@1104~{------------------------------------------------------------------------}^
{Change                         -a config command used to change DN in         }^
{                                BypassNumber table                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                          -a config command used to change DN in          ^
                                 BypassNumber Table.                            ^
                                                                                ^
     Example one shows how to change DN in BypassNumber table.                  ^
             Example 1: config-BypassNumberDirectory-3# change 1 dn 2223333     ^
                                                                                ^
           BypassNumber Table                                                   ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     2223333                                                        ^
           2     2225555                                                        ^
                                                                                ^
@1105~{------------------------------------------------------------------------}^
{Add                            -a config command used to add a DN number to   }^
{                                BypassNumber Table.                           }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                             -a config command used to add a DN number to    ^
                                 BypassNumber Table                             ^
                                                                                ^
     Example one shows how to add DN to BypassNumber Table                      ^
             Example 1: config-BypassNumberDirectory-1# add 3337777             ^
                                                                                ^
           BypassNumber Table                                                   ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     2223333                                                        ^
           2     2225555                                                        ^
           3     3337777                                                        ^
                                                                                ^
@1106~{------------------------------------------------------------------------}^
{rem                            -a config command used to remove a DN number   }^
{                                from BypassNumber Table                       }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                          -a config command used to remove a DN number    ^
                                 from BypassNumber Table                        ^
                                                                                ^
     Example one shows how to remove 3rd DN from BypassNumber Table             ^
             Example 1: config-BypassNumberDirectory-1# rem 3                   ^
                                                                                ^
           BypassNumber Table                                                   ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     2223333                                                        ^
           2     2225555                                                        ^
                                                                                ^
@1200~                                                                          ^
{------------------------------------------------------------------------------}^
{Level Name: <bn>.                                                             }^
{    The Bypass Number that the Tenor unit will route automatically to the     }^
{    trunk-side. This number should be specified in the format dialed from the }^
{    line-side.                                                                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Level Name: <BypassNumber>.                                                     ^
     The Bypass Number that the Tenor unit will route automatically to the      ^
     trunk-side. This number should be specified in the format dialed from the  ^
     line-side.                                                                 ^
                                                                                ^
@1203~{------------------------------------------------------------------------}^
{Set bn <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{DN <dn> -                      (:bypass number to route to PSTN). The number  }^
{                               should be in the international number format.  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %ByPassNumber <parameter><value>                                            ^
   where <parameter> is:                                                        ^
                                                                                ^
&Dn -                                                                           ^
         (:bypass DN route to PSTN)                                             ^
                                                                                ^
@1300~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <hldnd pub>.                                                      }^
{    A Hunt Local Directory Number Public is used to configure Local Directory }^
{    numbers, or Station Ranges, of calls that will route to the line-side     }^
{    <i.e., PBX> for a public dial plan.                                       }^
{                                                                              }^
{Level Name <hldnd priv>                                                       }^
{    A Hunt Local Directory Number Private is used to configure Local Directory}^
{    numbers, or Station Ranges, of calls that will route to the line-side     }^
{    <i.e., PBX> for a private dial plan.                                      }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <HuntLDNDirectory>.                                                 ^
     A Hunt Local Directory Number Public is used to configure Local Directory  ^
     numbers, or Station Ranges, of calls that will route to the line-side      ^
     <i.e., PBX> for a public dial plan.                                        ^
     A Hunt Local Directory Number should be specified in the local format and  ^
     not the full international format even though these calls are matched      ^
     based on the international format.                                         ^
     The Tenor will build the number<s> to the international format based on the^
     country code and area code you configured earlier. You do not need to      ^
     specify an index number; the next available index number will be           ^
     automatically assigned when you add the directory number.                  ^
                                                                                ^
     HuntLDN                                                                    ^
     -------------                                                              ^
     5552222                                                                    ^
                                                                                ^
     HuntLDN - The number that will be assigned to HuntLdnDir.                  ^
                                                                                ^
     A Hunt Local Directory Number Private is used to configure Local Directory ^
     numbers, or Station Ranges, of calls that will route to the line-side      ^
     <i.e., PBX> for a private dial plan.                                       ^
     A Hunt Local Directory Number should be specified in the local format and  ^
     not the full international format even though these calls are matched      ^
     based on the international format.                                         ^
     The Tenor will build the number<s> to the international format based on the^
     country code and area code you configured earlier. You do not need to      ^
     specify an index number; the next available index number will be           ^
     automatically assigned when you add the directory number.                  ^
                                                                                ^
     HuntLDN                                                                    ^
     -------------                                                              ^
     5552222                                                                    ^
                                                                                ^
     HuntLDN - The number that will be assigned to HuntLdnDir.                  ^
                                                                                ^
@1301~{------------------------------------------------------------------------}^
{new hldnd <id>                 Create new HuntLDNDirectory named <id>         }^
{                                                                              }^
--------------------------------------------------------------------------------^
new HuntLDNDirectory <id>       Create new HuntLDNDirectory named <id>          ^
                                                                                ^
     Example one shows how to create new HuntLDNDirectory with unique id.       ^
             Example 1: config-NumberDirectories-1# new hldnd pub2              ^
                                                                                ^
@1302~{------------------------------------------------------------------------}^
{Delete hldnd <id>              Delete existing HuntLDNDirectory named <id>    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Delete HuntLDN                  Delete existing HuntLDNDirectory  named <id>    ^
                                                                                ^
@1303~{------------------------------------------------------------------------}^
{Set hldnd <parameter><value>                                                  }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id> -                      (:read only)                                   }^
{name <name> -                  (:name)                                        }^
{LDNType <ldnt> -               (0:Public), (1:Private)                        }^
{RegisterDN <rdn>-              (0:no register)                                }^
{                               (1:register)                                   }^
{PrefixCCAC <pccac>-            (0:do not prefix)                              }^
{                               (1:prefix CC,AC)                               }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %HuntLDNDirectory <parameter><value>                                        ^
   where <parameter> is:                                                        ^
                                                                                ^
&id-         (:read only)                                                       ^
&name-       (:name)                                                            ^
&LDNType-                                                                       ^
             (0:public)                                                         ^
             (1:private)                                                        ^
&RegisterDN- (0:no register)                                                    ^
             (1:register)                                                       ^
&PrefixCCAC-                                                                    ^
             (0:do not prefix)                                                  ^
             (1:prefix CC,AC)                                                   ^
                                                                                ^
@1304~{------------------------------------------------------------------------}^
{Change                         -a config command used to change a DN in the   }^
{                                HuntLDN Table.                                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                          -a config command used to change a DN in the    ^
                                 HuntLDN Table.                                 ^
                                                                                ^
     Example one shows how to change DN in HuntLDN Table                        ^
             Example 1: config-HuntLDNDirectory-pub1# change 1 dn 4441111       ^
                                                                                ^
           HuntLDN Table                                                        ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     4441111                                                        ^
           2     2223333                                                        ^
                                                                                ^
@1305~{------------------------------------------------------------------------}^
{Add                            -a config command used to add a DN to HuntLDN  }^
{                                Table                                         }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                             -a config command used to add a DN to HuntLDN   ^
                                 Table                                          ^
                                                                                ^
     Example one shows how to add DN to HuntLDN Table                           ^
             Example 1: config-HuntLDNDirectory-pub1# add 3337777               ^
                                                                                ^
           HuntLDN Table                                                        ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     4441111                                                        ^
           2     2223333                                                        ^
           3     3337777                                                        ^
                                                                                ^
@1306~{------------------------------------------------------------------------}^
{rem                            -a config command used to remove a DN from     }^
{                                HuntLDN Table.                                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                          -a config command used to remove a DN from      ^
                                 HuntLDN Table.                                 ^
                                                                                ^
     Example one shows how to remove a DN from HuntLDN Table via index number.  ^
             Example 1: config-HuntLDNDirectory-pub1# rem 1                     ^
                                                                                ^
           HuntLDN Table                                                        ^
           Index DN                                                             ^
           ----- ----------------                                               ^
           1     2223333                                                        ^
           2     3337777                                                        ^
                                                                                ^
@1400~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <hldn>.                                                           }^
{     Hunt Local Directory Number is used to configure Local Directory numbers,}^
{     or Station Ranges, of calls that will route to the line-side <i.e., PBX> }^
{     for a public dial plan.                                                  }^
{                            .                                                 }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <HuntLDN>.                                                          ^
      Hunt Local Directory Number is used to configure Local Directory numbers, ^
      or Station Ranges, of calls that will route to the line-side <i.e., PBX>  ^
      for a public dial plan.                                                   ^
                                                                                ^
@1403~{------------------------------------------------------------------------}^
{Set hldn <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{DN <dn>-                       (:Hunt local directory number)                 }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %HuntLDN <parameter><value>                                                 ^
   where <parameter> is:                                                        ^
                                                                                ^
&Dn-                                                                            ^
         (:Hunt local DN)                                                       ^
                                                                                ^
@1500~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <hnd>.                                                            }^
{    A Hop Off  PBX call travels over IP, and then "hops" off into the public  }^
{    network on the distant side to reduce or eliminate public toll charges    }^
{    <also referred to as Leaky Area Mapping>. You may have multiple           }^
{    HopoffNumber Directories. To create a new Directory Group, type: "new hnd }^
{    <#>" , where <#> equals the number of the new group.                      }^
{    Ex: new hnd 3- to create the 3rd group.                                   }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <HopoffNumberDirectory>.                                            ^
     A Hop Off  PBX call travels over IP, and then "hops" off into the public   ^
     network on the distant side to reduce or eliminate public toll charges     ^
     <also referred to as Leaky Area Mapping>. You may have multiple            ^
     HopoffNumber Directories. To create a new Directory Group, type: "new hnd  ^
     <#>" , where <#> equals the number of the new group.                       ^
     Ex: new hnd 3- to create the 3rd group.                                    ^
                                                                                ^
@1501~{------------------------------------------------------------------------}^
{New hnd <id>                   Create new HopoffNumberDirectory named <id>    }^
{                                                                              }^
--------------------------------------------------------------------------------^
New HopoffNumberDirectory <id>  Create new HopoffNumber named <id>              ^
                                                                                ^
     Example:config-NumberDirectory-1# new hnd 2                                ^
                                                                                ^
@1502~{------------------------------------------------------------------------}^
{Delete hnd <id>                   Delete existing HopoffNumberDirectory named }^
{                                  <id>                                        }^
{                                                                              }^
--------------------------------------------------------------------------------^
Delete HopoffNumberDirectory <id>  Delete existing HopoffNumberDirectory named  ^
                                   <id>                                         ^
                                                                                ^
@1503~{------------------------------------------------------------------------}^
{Set hnd <parameter><value>                                                    }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{HopoffRoutingPriority <hrp>-   This is an integer value.                      }^
{                               This is for providing priority for certain     }^
{                               phone numbers over IP calls for Ckt switching  }^
{Pattern <p>-                   (:calling pattern for country and area code).  }^
{                               <e.g. 1212, which indicates 1 <country code>   }^
{                               and 212 <area code>>, used for calls that hop  }^
{                               through the public network to reach the        }^
{                               destination Tenor.                             }^
{Replacement <r>-               (:numbers to replace  in the Pattern field),   }^
{                               if other dial  elements <such as 10 or 011> are}^
{                               required for the call to reach the destination }^
{                               Tenor.                                         }^
{NumType <nt>-                  (0:Public; default), (1:Private).              }^
{TON <ton>-                     (0:Unknown,default)                            }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (4:Local)                                      }^
{NPI <npi>-                     (0:Unknown,default)                            }^
{                               (1:ISDN)                                       }^
{                               (9:Private)                                    }^
{Name <n>-                      (:name)                                        }^
{RegisterDN <rdn>-              (0:does not register DNs)                      }^
{                               (1:registers DNs)                              }^
--------------------------------------------------------------------------------^
Set %HopoffNumberDirectory <parameter><value>                                   ^
   where <parameter> is:                                                        ^
                                                                                ^
&HopoffRoutingPriority-                                                         ^
             (0:IP preferred over hopoff)                                       ^
             (:priority).                                                       ^
                                                                                ^
&Pattern-                                                                       ^
     (:calling pattern for country and area code)                               ^
                                                                                ^
&Replacement-                                                                   ^
     (:numbers to replace in the Pattern field)                                 ^
                                                                                ^
&NumType-                                                                       ^
             (0:public; default),                                               ^
             (1:private).                                                       ^
                                                                                ^
&TON-                                                                           ^
             (0:Unknown,default)                                                ^
             (1:International)                                                  ^
             (2:National)                                                       ^
             (4:Local)                                                          ^
                                                                                ^
&NPI-                                                                           ^
             (0:Unknown,default)                                                ^
             (1:ISDN)                                                           ^
             (9:Private)                                                        ^
&Name-       (:name)                                                            ^
&RegisterDN-  (0:does not register DNs)                                         ^
              (1:registers DNs)                                                 ^
                                                                                ^
@1504~{------------------------------------------------------------------------}^
{Change                        -a config command used to change table values by}^
{                               the index                                      }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change table values by ^
                                the index                                       ^
                                                                                ^
     Example one shows how to change pattern number in a HopoffNumber table:    ^
             Example 1: config-HopoffNumberDirectory-1# change 1 p 44           ^
                                                                                ^
                 HopoffNumber Table                                             ^
                 Index Pattern          Replacement      NumType TON  NPI       ^
                 ----- ---------------- ---------------- ------- ---- ----      ^
                 1     44               124              0       0    0         ^
                                                                                ^
     Example two shows how to change replacement number in a HopoffNumber table:^
             Example 2: config-HopoffNumberDirectory-1* change 1 r 00144        ^
                                                                                ^
                 HopoffNumber Table                                             ^
                 Index Pattern          Replacement      NumType TON  NPI       ^
                 ----- ---------------- ---------------- ------- ---- ----      ^
                 1     44               00144            0       0    0         ^
                                                                                ^
@1505~{------------------------------------------------------------------------}^
{Add                           -a config command used to add a new pattern     }^
{                               number to HopoffNumber Table                   }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                            -a config command used to add a new pattern      ^
                                number to HopoffNumber Table                    ^
                                                                                ^
     Example one shows how to add new pattern number to a HopoffNumber table:   ^
             Example 1: config-HopoffNumberDirectory-1# add 22                  ^
                                                                                ^
              HopoffNumber Table                                                ^
              Index Pattern          Replacement      NumType TON  NPI          ^
              ----- ---------------- ---------------- ------- ---- ----         ^
              1     44               00144            0       1    1            ^
              2     22                                0       0    0            ^
                                                                                ^
@1506~{------------------------------------------------------------------------}^
{rem                           -a config command used to remove pattern number }^
{                               from HopoffNumber Table                        }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                         -a config command used to remove pattern number  ^
                                from HopoffNumber Table                         ^
                                                                                ^
     Example one shows how to remove 2nd indexed entry from a HopoffNumber table^
     table:                                                                     ^
             Example 1:config-HopoffNumberDirectory-1* rem 2                    ^
                                                                                ^
              HopoffNumber Table                                                ^
              Index Pattern          Replacement      NumType TON  NPI          ^
              ----- ---------------- ---------------- ------- ---- ----         ^
              1     44               00144            0       1    1            ^
                                                                                ^
@1600~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <hn>.                                                             }^
{    The telephone number used as the Hop-off line-side number. Valid entry up }^
{    to 31 digits. This number should be in international format.              }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <HopoffNumber>.                                                     ^
     The telephone number used as the Hop-off line-side number. Valid entry up  ^
     to 31 digits. This number should be in international format.               ^
                                                                                ^
@1603~{------------------------------------------------------------------------}^
{Set hn <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Pattern <p>-                   (:calling pattern for country and area code)   }^
{                               <e.g. 1212, which indicates 1 <country code>   }^
{                               and 212 <area code>>, used for calls that hop  }^
{                               through the public network to reach the        }^
{                               destination Tenor.                             }^
{Replacement <r>-               (:numbers to replace  in the Pattern field)    }^
{                               if other dial  elements <such as 10 or 011> are}^
{                               required for the call to reach the destination }^
{                               Tenor.                                         }^
{NumType <nt>-                  The type of telephone number.                  }^
{                               (0:public; default)                            }^
{                               (1:private).                                   }^
{TON <ton>-                     (0:Unknown,default)                            }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (4:Local)                                      }^
{NPI <npi>-                     (0:Unknown,default)                            }^
{                               (1:ISDN)                                       }^
{                               (9:Private)                                    }^
--------------------------------------------------------------------------------^
Set %HopoffNumber <parameter><value>                                            ^
   where <parameter> is:                                                        ^
                                                                                ^
&HopoffNumber-                                                                  ^
     The telephone number used as the Hop-off line-side number. Valid entry up  ^
     to 31 digits. This number should be in international format.               ^
                                                                                ^
&Pattern-                                                                       ^
     (:calling pattern for country and area code)                               ^
                                                                                ^
&Replacement-                                                                   ^
     (:numbers to replace  in the Pattern field)                                ^
                                                                                ^
&NumType-                                                                       ^
             (0:public; default),                                               ^
             (1:private).                                                       ^
                                                                                ^
&TON-                                                                           ^
             (0:Unknown,default)                                                ^
             (1:International)                                                  ^
             (2:National)                                                       ^
             (4:Local)                                                          ^
                                                                                ^
&NPI-                                                                           ^
             (0:Unknown,default)                                                ^
             (1:ISDN)                                                           ^
             (9:Private)                                                        ^
                                                                                ^
@1700~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <asnd>.                                                           }^
{    Number Directory that contains numbers that will be dialed by other Tenors}^
{    or gateways to initiate an Auto- Switch to this Tenor.  These numbers     }^
{    can be created under NumberDirectory using new and add commands.          }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <AutoSwitchNumberDirectory>.                                        ^
     Number Directory that contain numbers which will be dialed by other Tenors ^
     or gateways to initiate an Auto-Switch to this Tenor.                      ^
                                                                                ^
@1703~{------------------------------------------------------------------------}^
{Set asnd <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Type <t>-                      Auto-Switch type.                              }^
{                               (0:No DID is received),                        }^
{                               (1:DID is received).                           }^
{Number <n>-                    (:Number to initiate auto-switch).             }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %AutoSwitchNumberDirectory <parameter><value>                               ^
   where <parameter> is:                                                        ^
                                                                                ^
&AutoSwitchNumber-                                                              ^
             (:Phone number that are used to initiate an Auto-Switch.)          ^
                                                                                ^
&Type-                                                                          ^
             (0:No DID is received),                                            ^
             (1:DID is received).                                               ^
                                                                                ^
&Number-                                                                        ^
             (:Number to initiate auto-switch).                                 ^
                                                                                ^
@1704~{------------------------------------------------------------------------}^
{add <asn>                      Add new AutoSwitchNumber in international      }^
{                                   format named <id>                          }^
{                                                                              }^
--------------------------------------------------------------------------------^
add AutoSwitchNumber            Add new AutoSwitchNumber named <id>             ^
                                                                                ^
     Example one shows how to add a DID asn number to AutoSwitchNumber Table    ^
             If the type field is set to 0 <default if not specified in the add ^
             command> the asn will be a Non-DID number.                         ^
             The number added should be in international format.                ^
             Example 1: config-AutoSwitchNumbeDirectory-1# add 2225555 t 1      ^
                                                                                ^
             AutoSwitchNumber Table                                             ^
             Index    Number              Type                                  ^
             -----    ----------------    ----                                  ^
             1        2225555             1<DID>                                ^
                                                                                ^
@1705~{------------------------------------------------------------------------}^
{remove <id>                    Remove existing AutoSwitchNumber named <id>    }^
{                                                                              }^
--------------------------------------------------------------------------------^
remove AutoSwitchNumber         Remove existing AutoSwitchNumber named <id>     ^
                                                                                ^
@1706~{------------------------------------------------------------------------}^
{Change                        -a config command used to change table values by}^
{                               the index.                                     }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change table values by ^
                                the index.                                      ^
                                                                                ^
     This xample shows to change AutoSwitchNumber for index 3:                  ^
        Example 3:config-AutoSwitchNumberDirectory-1# change 3 n 2225555        ^
                                                                                ^
           AutoSwitchNumber Table                                               ^
           Index Number           Type                                          ^
           ----- ---------------- ----                                          ^
           1     2223333          1<DID>                                        ^
           2     3337777          1<DID>                                        ^
           3     2225555          0<Non-DID>                                    ^
                                                                                ^
@1707~{------------------------------------------------------------------------}^
{Add                           -a config command used to add a DN number to    }^
{                               AutoSwitchNumber Table                         }^
{                                                                              }^
 -------------------------------------------------------------------------------^
Add     -a config command used to add a DN number to AutoSwitchNumber Table     ^
                                                                                ^
     Example one shows how to add a new DN to AutoSwitchNumber table            ^
        Example 1: config-AutoSwitchNumberDirectory-1# add 5552222              ^
                                                                                ^
           AutoSwitchNumber Table                                               ^
           Index Number           Type                                          ^
           ----- ---------------- ----                                          ^
           1     2223333          0                                             ^
           2     3337777          0                                             ^
           3     2225555          0                                             ^
           4     5552222          0                                             ^
                                                                                ^
@1708~{------------------------------------------------------------------------}^
{rem                           -a config command used to remove a DN number    }^
{                               from AutoSwitchNumber Table                    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove  -a config command used to remove a DN number from AutoSwitchNumber Table^
                                                                                ^
     Example one shows how to remove 2nd DN from AutoSwitchNumber table via the ^
     assign index number.                                                       ^
        Example 1: config-AutoSwitchNumberDirectory-1# rem 2                    ^
                                                                                ^
           AutoSwitchNumber Table                                               ^
           index Number           Type                                          ^
           ----- ---------------- ----                                          ^
           1     2223333          0                                             ^
           2     2225555          0                                             ^
           3     5552222          0                                             ^
                                                                                ^
                                                                                ^
@1720~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <asn>.                                                            }^
{    Numbers that will be dialed by other Tenors or gateways to initiate an    }^
{    Auto-Switch to this Tenor.  These numbers can be created under            }^
{    NumberDirectory using new and add commands.                               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <AutoSwitchNumber>.                                                 ^
     Numbers that will be dialed by other Tenors or gateway to initiate an      ^
     Auto-Switch to this Tenor. These numbers can be created under              ^
     NumberDirectory using new and add commands.                                ^
                                                                                ^
@1721~{------------------------------------------------------------------------}^
{Set asn <parameter><value>                                                    }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Type <t>-                      Auto-Switch type.                              }^
{                               (0:No DID is received),                        }^
{                               (1:DID is received).                           }^
{Number <n>-                    (:Number to initiate auto-switch).             }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %AutoSwitchNumber <parameter><value>                                        ^
   where <parameter> is:                                                        ^
                                                                                ^
&Type-                                                                          ^
             (0:No DID is received)                                             ^
             (1:DID is received).                                               ^
                                                                                ^
&Number-                                                                        ^
             (:Number to initiate auto-switch).                                 ^
                                                                                ^
@1800~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <cp>.                                                             }^
{    Voice Codec Profile.  Used to hold up to 8 different voice codecs.        }^
{                     .                                                        }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <CodecProfile>.                                                     ^
     Voice Codec Profile.  Used to hold up to 8 differenct voice codecs.        ^
     Each voice codec defined a voice compression algorithm and its payload     ^
     size.            .                                                         ^
                                                                                ^
@1803~{------------------------------------------------------------------------}^
{Set cp <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{name <name>-           (:name)                                                }^
{VoiceCodecIndex <vci>-  used to assigned a specified Voice Codec              }^
{                        instance,vc-<id>. Default is assigned to vc-1.        }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %CodecProfile <parameter><value>                                            ^
   where <parameter> is:                                                        ^
                                                                                ^
&name-  (:name)                                                                 ^
&VoiceCodecIndex-                                                               ^
     Used to assigned a specified Voice Codec instance,VoiceCodec-<id>.         ^
             Default entry: VoiceCode-1.                                        ^
                                                                                ^
        (:assigned Voice Codec),                                                ^
        (VoiceCodec-1: default)                                                 ^
                                                                                ^
     Example show how to set VoiceCodecIndex[2] to VoiceCodec-3                 ^
                                                                                ^
     Example 1. config-CodecProfile-1# set vci[2] vc-3                          ^
                                                                                ^
@1810~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <vc>.                                                             }^
{    Voice Codec.  Used to set the compression algorithm that will be used by  }^
{                  voice encoding and decoding.       .                        }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <VoiceCodec>.                                                       ^
     Voice Codec.  Used to set the compression algorithm that will be used by   ^
     voice encoding and decoding.                                               ^
                                                                                ^
@1813~{------------------------------------------------------------------------}^
{Set vc <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{name <name>-                   (:name)                                        }^
{CodecVoiceCoding <cvc>-        Voice Coding Compression Algorithm.            }^
{                                                                              }^
{        (8:G.711 A-Law),             (9:G.711 Mu-Law),                        }^
{        (68:G.729AB at 8kbps),       (80:G7.723.1 at 5.3kbps)                 }^
{        (81:G.723.1 at 6.3kbps)                                               }^
{        (10:G.726 at 16kbps)                                                  }^
{        (11:G.726 at 24kbps)                                                  }^
{        (12:G.726 at 32kbps)                                                  }^
{        (13:G.726 at 40kbps)                                                  }^
{CodecPayloadSize <cps>-        Voice Information Field Size.                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %VoiceCodec <parameter><value>                                              ^
   where <parameter> is:                                                        ^
                                                                                ^
&name-       (:name)                                                            ^
&CodecVoiceCoding-                                                              ^
        (8:G.711 A-Law),                                                        ^
        (9:G.711 Mu-Law),                                                       ^
        (68:G.729AB at 8kbps),       (80:G.723.1 at 5.3kbps)                    ^
        (81:G.723.1 at 6.3kbps)                                                 ^
        (10:G.726 at 16kbps)                                                    ^
        (11:G.726 at 24kbps)                                                    ^
        (12:G.726 at 32kbps)                                                    ^
        (13:G.726 at 40kbps)                                                    ^
&CodecPayloadSize-                                                              ^
        (10:ms), (20:ms),                                                       ^
        (30:ms), (40:ms),                                                       ^
        (50:ms), (60:ms),                                                       ^
        (90:ms), (120:ms),                                                      ^
                                                                                ^
@1900~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <cg>.                                                             }^
{    A ChannelGroup consists of one or more channels from a line device.  Each }^
{    channel is associated with a particular Signaling Group for setting up a  }^
{    call or a service.                                                        }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <ChannelGroup>.                                                     ^
     A ChannelGroup consists of one or more channels from a line device.  Each  ^
     channel is associated with a particular Signaling Group for setting up a   ^
     call or a service.                                                         ^
                                                                                ^
@1903~{------------------------------------------------------------------------}^
{Set cg <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{SignalingGroupAttached <sg>-   (:Signaling group ID)                          }^
{RoutingGroupAttached <rg>-     (:Routing group ID)                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %ChannelGroup <parameter><value>                                            ^
   where <parameter> is:                                                        ^
                                                                                ^
&SignalingGroupAttached-                                                        ^
     (:Signaling group ID)                                                      ^
                                                                                ^
&RoutingGroupAttached-                                                          ^
     (:Routing group ID)                                                        ^
                                                                                ^
@2000~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <cassg>.                                                          }^
{    CAS Signaling Group Signaling is a type of signaling that enables T1 or E1}^
{    interfaces to share the same D channel.                                   }^
{    CASSignalingGroup enables you to configure signaling type, E and M        }^
{    Incoming protocol, outgoing protocol, orientation, dial tone detect, dial }^
{    delay etc.                                                                }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <CASSignalingGroup>.                                                ^
     CAS Signaling Group Signaling is a type of signaling that enables T1 or E1 ^
     interfaces to share the same D channel.                                    ^
     CASSignalingGroup enables you to configure signaling type, E and M Incoming^
     protocol, outgoing protocol, orientation, dial tone detect, dial delay etc.^
                                                                                ^
@2003~{------------------------------------------------------------------------}^
{Set cassg <parameter><value>                                                  }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                       (:read only)                                   }^
{name <name>-                   (:name)                                        }^
{Orientation <or>-              (0:Slave, User)(1:Master, Network)             }^
{                                                                              }^
{Disconnect Supervision <as>-   (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{                                                                              }^
{RingFrequency <rf>-            (+15 - +40:Hz)                                 }^
{                                                                              }^
{DTMFONTone <dtmfon>-           (:50-1000ms,def 100)                           }^
{                                                                              }^
{DTMFOFFTone <dtmfoff>-         (:50-1000ms,def 100)                           }^
{                                                                              }^
{LineTemplate<lt>-                                                             }^
{             (0:See CLI guide)                                                }^
{             (1:See CLI guide)                                                }^
{             (2:See CLI guide)                                                }^
{             (3:See CLI guide)                                                }^
{             (4:See CLI guide)                                                }^
{             (5:See CLI guide)                                                }^
{             (6:See CLI guide)                                                }^
{             (7:See CLI guide)                                                }^
{             (8:See CLI guide)                                                }^
{             (9:See CLI guide)                                                }^
{             (10:See CLI guide)                                               }^
{             (11:See CLI guide)                                               }^
{             (12:See CLI guide)                                               }^
{                                                                              }^
{RxGain <rg>-                                                                  }^
{             (-14 - +14:db)                                                   }^
{                                                                              }^
{TxGain <tg>-                                                                  }^
{             (-14 - +14:db)                                                   }^
{                                                                              }^
{Impedance <i>-                                                                }^
{             (0:600 ohms,default)                                             }^
{             (1 - 7:phone side,see CLI guide)                                 }^
{             (1 - 15:line side,see CLI guide)                                 }^
{									       }^
{LocalLoopType <llt>-                                       		       }^
{             (0:EIA Type 0, default)                                          }^
{             (1:EIA Type 1)						       }^
{             (2:EIA Type 2)						       }^
{             (3:EIA Type 3)						       }^
{             (4:EIA Type 4)						       }^
{             (5:EIA Type 5)						       }^
{             (6:EIA Type 6)						       }^
{             (7:EIA Type 7)						       }^
{									       }^
{CadenceONTime <cont>-                                                         }^
{             (:numeric,ms)                                                    }^
{                                                                              }^
{CadenceOFFTime <cofft>-                                                       }^
{             (:numeric,ms)                                                    }^
{                                                                              }^
{CadenceOFFTime2                                                               }^
{             (:numeric,ms)                                                    }^
{                                                                              }^
{GuardTime <gt>-                                                               }^
{             (numeric,ms)                                                     }^
{                                                                              }^
{Ring12Delay <rd>-                                                             }^
{              (:numeric,seconds)                                              }^
{                                                                              }^
{MINRingFrequency <minrf>-                                                     }^
{               (:numeric,default 15Hz)                                        }^
{                                                                              }^
{MAXRingFrequency <maxrf>-                                                     }^
{               (:numeric,default 50Hz)                                        }^
{                                                                              }^
{DisconnectSupervisionOptions <dso>-                                           }^
{               (2:on,off interval,default)                                    }^
{               (3:on,off interval)                                            }^
{               (4:on,off interval)                                            }^
{               (5:on,off interval)                                            }^
{               (6:on,off interval)                                            }^
{               (7:on,off interval)                                            }^
{               (8:on,off interval)                                            }^
{SilenceBasedDisconnect <sbd>-                                                 }^
{               (:seconds)                                                     }^
{ToneBasedSupervision <tbs>-                                                   }^
{               (0:None, default)                                              }^
{               (1:Disconnect)                                                 }^
{               (2:Answer)                                                     }^
{               (3:Answer and Disconnect)                                      }^
{                                                                              }^
{SignalingType <st>-            (0:E and M signaling)                          }^
{                               (1:Loop Start)                                 }^
{                               (2:LoopSt Rev Battery)                         }^
{                               (3:LoopSt Forward Disc)                        }^
{                               (5:Feature Group D)                            }^
{                               (6:MFC R2)                                     }^
{                               (7:MFC R1)                                     }^
{                                                                              }^
{RElayANI <reani>-              (0:No Relay ANI)                               }^
{                               (1:Relay ANI)                                  }^
{                               (99:Get ANI from file)                         }^
{                                                                              }^
{IncomingStartDial <insd>-      (0:Wink Start)                                 }^
{                               (1:Automatic dialing)                          }^
{                               (2:Immediate dialing)                          }^
{                               (3:Delay dialing)                              }^
{                                                                              }^
{OutgoingStartDial <outsd>-     (0:Wink Start)                                 }^
{                               (1:Automatic dialing)                          }^
{                               (2:Immediate dialing)                          }^
{                               (3:Delay dialing)                              }^
{DisconnectToneProfileAttached <dtpa>-                                         }^
{                               (:associated tp Id)                            }^
{                                                                              }^
{CallerIDDetection <cidd>-                                                     }^
{                               (0:Disabled,default)                           }^
{                               (1:FSK or DTMF)                                }^
{                               (2:PassThrough)                                }^
{                               (3:DTMF,ETSI,Rev Battery)                      }^
{                               (4:NTT,Japan CID)                              }^
{                               (5:ETSI)                                       }^
{                               (6:FSK,Rev Battery)                            }^
{                               (7:DTMF,No Ring)                               }^
{                                                                              }^
{DialToneDetect <dtd>-          (0:No), (1:Yes)                                }^
{DialDelay <dd>-                (:dial delay in ms)                            }^
{AnswerDelay <ad>-              (0-360:seconds)                                }^
{FlashhookSignal <fs>-          (0:No), (1:Yes)                                }^
{FlashhookDuration <fd>-        (:Flash hook duration in ms)                   }^
{MAXFlashhook <maxf>-           (:maximum flash hook in ms)                    }^
{MINFlashhook <minf>-           (:minimum flash hook in ms)                    }^
{                                                                              }^
{CallerIDGeneration <cidg>-     (0:disabled)                                   }^
{                               (1:FSK)                                        }^
{                               (2:DTMF)                                       }^
{                               (3:DTMF,Rev Battery)                           }^
{                               (4:ETSI,Rev Battery)                           }^
{                               (5:NTT,Japan CID)                              }^
{                               (6:ETSI)                                       }^
{                               (7:DTMF,No Ring)                               }^
{                                                                              }^
{AnswerSupervisionMoreSensitive <asms>-                                        }^
{                               (0:Disabled)                                   }^
{                               (1:Enabled)                                    }^
{                                                                              }^
{AnswerSupervisionDelayAnswer <asda>-                                          }^
{                               (0:Disabled)                                   }^
{                               (1:Enabled)                                    }^
{                                                                              }^
{AnswerSupervisionLessFilter <aslf>-                                           }^
{                               (0:Disabled)                                   }^
{                               (1:Enabled)                                    }^
{                                                                              }^
{CdBits <cb>-                   (0: 0000), (1:0001), (2:0010), (3:0011)        }^
{InvertABCD <iabcd>-            (:Invert ABCD)                                 }^
{ReqCatDigit <rcd>-             (6:China, Malaysia, and Singapore), (5:Other)  }^
{ReqANIDigit <ranid>-           (6:China, Malaysia, and Singapore), (5:Other)  }^
{Send1stDigit <sd>-             (9:Korea), (0:Other)                           }^
{GbIdleSent <gis>-              (1:China, Malaysia, and Singapore), (6:Other)  }^
{GbBusySent <gbs>-              (3:Gb Busy sent)                               }^
{A6Cat <a6c>-                   (:A6 cat)                                      }^
{A6Cat <a3c>-                   (:A3 cat)                                      }^
{DNISLen <dnisl>-               (:DNIS Length)                                 }^
{ReqANI <rani>-                 (:Request ANI)                                 }^
{ANILen <anil>-                 (:ANI Length)                                  }^
{                                                                              }^
{GbIdleRcvdBits <girb>-         (0x21:China, B1 and B6),                       }^
{                               (0x61:Other, B1, B6 *B7)                       }^
{                                                                              }^
{GbBusyRcvdBits <gbrb>-         (0x0e:China, B2, B3, B4)                       }^
{                               (0x04:Other, B3)                               }^
{                                                                              }^
{FwdToneONtime <fton>-          (:Forward tone On time)                        }^
{FwdToneOFFtime <ftoff>-        (:Forward tone Off time)                       }^
{ConsFwdToneTime <cftt>-        (:Cons forward tone time)                      }^
{RelGuardTime <rgt>-            (:rel Guard time, in ms)                       }^
{SeizureAckTime <sat>-          (:Seizure acknowledge time in ms)              }^
{UCFrequency <ucf>-             (0:DTMF)(1:MF)                                 }^
{UCAddressAck <ucaa>-           (0:No)(1:Yes)                                  }^
{DefaultANI <dani>-             (:Feature Group D default ANI)                 }^
{PulseONTime <pont>-            (:0-255ms,default 60)                          }^
{PulseOFFTime <pofft>-          (:0-255ms,default 40)                          }^
{PulseInterDigitPause <pidp>-   (:0-3000ms,default 700)                        }^
{DialMode <dm>-                 (0:DTMF Tone Dial)                             }^
{                               (1:Pulse Dial)                                 }^
{AnswerSupervisionHoldoff <asho>- (:seconds,0-60)                              }^
{IncomingTone <it>-             (0:MF)                                         }^
{                               (1:DTMF)                                       }^
{OutgoingTone <ot>-             (0:MF)                                         }^
{                               (1:DTMF)                                       }^
{MEterCode <mec>-               (0:no meter)                                   }^
{                               (1:Pulsed Clear Back)                          }^
{                               (2:Pulsed Answer)                              }^
{RingValidation <rv>-           (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{RelayCallingNAMe <rcnam>-      (0:do not relay)                               }^
{                               (1:relay in ISDN,H.323 or SIP)                 }^
{                               (3:relay DefaultCallingNAMe)                   }^
{MWIType <mwit>-                (0:Stutter only)                               }^
{                               (1:SMDF FSK,Stutter)                           }^
{                               (2:MMDF FSK,Stutter)                           }^
{                               (3:Euro FSK,Stutter)                           }^
{                               (4:Neon only)                                  }^
{                               (5:LED only)                                   }^
{DefaultCallingNAMe <dcnam>-    (:calling name,15 alphanum)                    }^
{ForwardDisconnectDelay <fdd>-  (0-32767:ms delay)                             }^
{                               (500:delay,user)                               }^
{                               (800:delay,network)                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %CASSignalingGroup <parameter><value>                                       ^
   where <parameter> is:                                                        ^
                                                                                ^
&id-       (:read only)                                                         ^
&name-     (:name)                                                              ^
&ORientation-                                                                   ^
             (0:Slave, User; default)                                           ^
             (1:Master, Network)                                                ^
                                                                                ^
&DisconnectSupervision-                                                         ^
             (0:disabled)                                                       ^
             (1:enabled)                                                        ^
                                                                                ^
&RingFrequency-                                                                 ^
              (+15 - +40:Hz)                                                    ^
                                                                                ^
&DTMFONTime-                                                                    ^
              (:50-1000ms,def 100)                                              ^
                                                                                ^
&DTMFOFFTime-                                                                   ^
              (:50-1000ms,def 100)                                              ^
                                                                                ^
&LineTemplate-                                                                  ^
              (0:See CLI guide)                                                 ^
              (1:See CLI guide)                                                 ^
              (2:See CLI guide)                                                 ^
              (3:See CLI guide)                                                 ^
              (4:See CLI guide)                                                 ^
              (5:See CLI guide)                                                 ^
              (6:See CLI guide)                                                 ^
              (7:See CLI guide)                                                 ^
              (8:See CLI guide)                                                 ^
              (9:See CLI guide)                                                 ^
              (10:See CLI guide)                                                ^
              (11:See CLI guide)                                                ^
              (12:See CLI guide)                                                ^
                                                                                ^
&RxGain-                                                                        ^
              (-14 - +14:db)                                                    ^
&TxGain-                                                                        ^
              (-14 - +14:db)                                                    ^
                                                                                ^
&Impedance-                                                                     ^
                                                                                ^
              (0:600 ohms,default)                                              ^
              (1 - 7:phone side,see CLI guide)                                  ^
              (1 - 15:line side,see CLI guide)                                  ^
                                                                                ^
&LocalLoopType-									^
              (0:EIA Type 0, default)							^			
              (1:EIA Type 1)							^			
              (2:EIA Type 2)							^			
              (3:EIA Type 3)							^			
              (4:EIA Type 4)							^			
              (5:EIA Type 5)							^			
              (6:EIA Type 6)							^			
              (7:EIA Type 7)							^			
										^
&CadenceONTime-                                                                 ^
              (:numeric,ms)                                                     ^
                                                                                ^
&CadenceOFFTime-                                                                ^
              (:numeric,ms)                                                     ^
                                                                                ^
&CadenceOFFTime2-                                                               ^
              (:numeric,ms)                                                     ^
                                                                                ^
&GuardTime-                                                                     ^
              (:numeric,default 10 ms)                                          ^
                                                                                ^
&Ring12Delay-                                                                   ^
              (:numeric;seconds)                                                ^
                                                                                ^
&MINRingFrequency-                                                              ^
              (:numeric,default 15Hz)                                           ^
                                                                                ^
&MAXRingFrequency-                                                              ^
              (:numeric,default 50Hz)                                           ^
                                                                                ^
&DisconnectSupervisionOptions-                                                  ^
                (2:on,off interval, default)                                    ^
                (3:on,off interval)                                             ^
                (4:on,off interval)                                             ^
                (5:on,off interval)                                             ^
                (6:on,off interval)                                             ^
                (7:on,off interval)                                             ^
                (8:on,off interval)                                             ^
&SilenceBasedDisconnect-                                                        ^
              (:seconds)                                                        ^
                                                                                ^
&ToneBasedSupervision-                                                          ^
               (0:None, default)                                                ^
               (1:Disconnect)                                                   ^
               (2:Answer)                                                       ^
               (3:Answer and Disconnect)                                        ^
                                                                                ^
&SignalingType-                                                                 ^
             (0:E and M signaling),                                             ^
             (1:Loop Start)                                                     ^
             (2:LoopSt Reverse Battery)                                         ^
             (3:LoopSt Forward Disc)                                            ^
             (5:Feature Group D)                                                ^
             (6:MFC R2)                                                         ^
             (7:MFC R1)                                                         ^
                                                                                ^
                                                                                ^
&RElayANI-                                                                      ^
             (0:No Relay ANI)                                                   ^
             (1:Relay ANI)                                                      ^
             (99:Get ANI from file)                                             ^
                                                                                ^
&DialToneDetect-                                                                ^
            (0:No, no dial tone detect before dialing out)                      ^
            (1:Yes, dial tone detect before dialing out)                        ^
                                                                                ^
&DiscSupervision-                                                               ^
            (0:Off) (1:On)                                                      ^
                                                                                ^
&INcomingStartDial-                                                             ^
             (0:Wink Start)                                                     ^
             (1:Automatic dialing)                                              ^
             (2:Immediate dialing)                                              ^
             (3:Delay dialing)                                                  ^
                                                                                ^
&OUTgoingStartDial-                                                             ^
             (0:Wink Start)                                                     ^
             (1:Automatic dialing)                                              ^
             (2:Immediate dialing)                                              ^
             (3:Delay dialing)                                                  ^
                                                                                ^
&DisconnectToneProfileAttached-                                                 ^
             (:Associated Tone Profile Id)                                      ^
                                                                                ^
&DialDelay-                                                                     ^
             (0:ms delay; 0-default)                                            ^
                                                                                ^
&AnswerDelay-                                                                   ^
             (0-360:seconds)                                                    ^
                                                                                ^
&FlashhookSignal-                                                               ^
             (0:No)                                                             ^
             (1:Yes)                                                            ^
                                                                                ^
&FlashhookDuration-                                                             ^
             (:Flash hook duration in ms)                                       ^
             (500:500 ms)                                                       ^
                                                                                ^
&MAXFlashhook-                                                                  ^
             (:maximum flash hook in ms)                                        ^
             (700:700 ms)                                                       ^
                                                                                ^
&MINFlashhook-                                                                  ^
             (:minimum flash hook in ms)                                        ^
             (200:200 ms)                                                       ^
                                                                                ^
&CallerIDGeneration-                                                            ^
             (0:disabled)                                                       ^
             (1:FSK)                                                            ^
             (2:DTMF)                                                           ^
             (3:DTMF,Rev Battery)                                               ^
             (4:ETSI,Rev Battery)                                               ^
             (5:NTT,Japan CID)                                                  ^
             (6:ETSI)                                                           ^
             (7:DTMF,No Ring)                                                   ^
                                                                                ^
&AnswerSupervisionMoreSensitive-                                                ^
             (0:Disabled)                                                       ^
             (1:Enabled)                                                        ^
                                                                                ^
&AnswerSupervisionDelayAnswer-                                                  ^
             (0:Disabled)                                                       ^
             (1:Enabled)                                                        ^
                                                                                ^
&AnswerSupervisionLessFilter-                                                   ^
             (0:Disabled)                                                       ^
             (1:Enabled)                                                        ^
                                                                                ^
&CallerIDDetection-                                                             ^
             (0:Disabled,default)                                               ^
             (1:FSK or DTMF)                                                    ^
             (2:PassThrough)                                                    ^
             (3:DTMF,ETSI,Rev Battery)                                          ^
             (4:NTT,Japan CID)                                                  ^
             (5:ETSI)                                                           ^
             (6:FSK,Rev Battery)                                                ^
             (7:DTMF,No Ring)                                                   ^
                                                                                ^
&DefaultANI-                                                                    ^
             (:Calling party number for out bound calls)                        ^
                                                                                ^
&CdBits-                                                                        ^
             (0:0000)                                                           ^
             (1:0001)                                                           ^
             (2:0010)                                                           ^
             (3:0011)                                                           ^
                                                                                ^
&InvertABCD-                                                                    ^
             (0:0000)               (1:0001)                                    ^
             (2:0010)               (3:0011)                                    ^
             (4:0100)               (5:0101)                                    ^
             (6:0110)               (7:0111)                                    ^
             (8:1000)               (9:1001)                                    ^
             (10:1010)              (11:1011)                                   ^
             (12:1100)              (13:1101)                                   ^
             (14:1110)              (15:1111)                                   ^
                                                                                ^
&ReqCatDigit-                                                                   ^
             (6:China, Malaysia, and Singapore)                                 ^
             (5:Other)                                                          ^
                                                                                ^
&ReqANIDigit-                                                                   ^
             (6:China, Malaysia, and Singapore)                                 ^
             (5:Other)                                                          ^
                                                                                ^
&AnsDigit-                                                                      ^
             (:Answer digit)                                                    ^
                                                                                ^
&Send1stDigit-                                                                  ^
             (9:Korea)                                                          ^
             (0:Other)                                                          ^
                                                                                ^
&GbIdleSent-                                                                    ^
             (1:China, Malaysia, and Singapore)                                 ^
             (6:Other)                                                          ^
                                                                                ^
&GbBusySent-                                                                    ^
             (:Gb Busy sent)                                                    ^
             (3:most countries)                                                 ^
                                                                                ^
&A6Cat-                                                                         ^
             (:A6 cat)                                                          ^
                                                                                ^
&A3Cat-                                                                         ^
             (:A3 cat)                                                          ^
                                                                                ^
&DNISLen-                                                                       ^
             (0:Variable DNIS Length)                                           ^
             (:Specified DNIS Length)                                           ^
                                                                                ^
&ReqANI-                                                                        ^
             (0:Do not request ANI)                                             ^
             (:Request ANI after the specified DNIS digit)                      ^
             (-1:Request ANI after complete DNIS receipt)                       ^
                                                                                ^
&CatANI-                                                                        ^
             (:Specified tone to request ANI Category)                          ^
                                                                                ^
&ANILen-                                                                        ^
             (0:Variable length ANI)                                            ^
             (:Specified ANI Length)                                            ^
                                                                                ^
&GbIdleRcvdBits-                                                                ^
             (33:100001 China, B1 and B6)                                       ^
             (97:1100001 Other, B1, B6 *B7)                                     ^
                                                                                ^
&GbBusyRcvdBits-                                                                ^
             (14:1110 China, B2, B3, B4)                                        ^
             (4:100 Other, B3)                                                  ^
                                                                                ^
&FwdToneONtime-                                                                 ^
             (0:0 ms)                                                           ^
             (:Forward tone On time in ms)                                      ^
                                                                                ^
&FwdToneOFFtime-                                                                ^
     Forward tone Off time                                                      ^
             (0:0 ms)                                                           ^
             (:Forward tone Off time in ms)                                     ^
                                                                                ^
&ConsFwdToneTime-                                                               ^
             (0:0 ms)                                                           ^
             (:Cons forward tone time in ms)                                    ^
                                                                                ^
&RelGuardTime-                                                                  ^
             (0:0 ms)                                                           ^
             (:rel Guard time in ms)                                            ^
                                                                                ^
&SeizureAckTime-                                                                ^
             (0:0 ms)                                                           ^
             (:Seizure acknowledge time in ms)                                  ^
                                                                                ^
&UCFrequency-                                                                   ^
             (0:DTMF)(1:MF)                                                     ^
                                                                                ^
&UCAddressAck-                                                                  ^
             (0:No)(1:Yes)                                                      ^
                                                                                ^
&DefaultANI-                                                                    ^
             (:default ANI)                                                     ^
&PulseONTime-  (:0-255ms,default 60)                                            ^
&PulseOFFTime- (:0-255ms,default 40)                                            ^
&PulseInterDigitPause-   (:0-3000ms,default 700)                                ^
&DialMode- (0:DTMF Tone Dial)                                                   ^
           (1:Pulse Dial)                                                       ^
&AnswerSupervisionHoldoff- (:seconds,0-60)                                      ^
                                                                                ^
&IncomingTone-      (0:MF)                                                      ^
                    (1:DTMF)                                                    ^
&OutgoingTone-      (0:MF)                                                      ^
                    (1:DTMF)                                                    ^
&MEterCode-         (0:no meter)                                                ^
                    (1:Pulsed Clear Back)                                       ^
                    (2:Pulsed Answer)                                           ^
&RingValidation-    (0:disabled)                                                ^
                    (1:enabled)                                                 ^
&RelayCallingNAMe-              (0:do not relay)                                ^
                                (1:relay in ISDN,H.323 or SIP)                  ^
                                (3:relay DefaultCallingNAMe)                    ^
&MWIType-                       (0:Stutter only)                                ^
                                (1:SMDF FSK,Stutter)                            ^
                                (2:MMDF FSK,Stutter)                            ^
                                (3:Euro FSK,Stutter)                            ^
                                (4:Neon only)                                   ^
                                (5:LED only)                                    ^
&DefaultCallingNAMe-            (:calling name,15 alphanum)                     ^
&ForwardDisconnectDelay-        (0-32767:ms delay)                              ^
                                (500:delay,user)                                ^
                                (800:delay,network)                             ^
                                                                                ^
@2100~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <isdnsg>.                                                         }^
{    ISDN Signaling Group or Common Channel Signaling <CCS> is a type of       }^
{    signaling that enables T1 or E1 interfaces to share the same D channel.   }^
{    ISDNSignalingGroup enables you to configure ISDN data; you are able to    }^
{    choose the ISDN protocol type, such as 4ESS, 5ESS, DMS, NI2, etc.         }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <ISDNSigalingGroup>.                                                ^
     ISDN Signaling Group or Common Channel Signaling <CCS> is a type of        ^
     signaling that enables T1 or E1 interfaces to share the same D channel.    ^
     ISDNSignalingGroup enables you to configure ISDN data; you are able to     ^
     choose the ISDN protocol type, such as 4ESS, 5ESS, DMS, NI2, etc.          ^
                                                                                ^
@2103~{------------------------------------------------------------------------}^
{Set isdnsg <parameter><value>                                                 }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Orientation <or>-              (0:User; default), (1:Network).                }^
{                                                                              }^
{Protocol <prot>-               (0:PRI_5ESS; default), (1:PRI_4ESS),           }^
{                               (2:PRI_DMS),        (3:PRI_NI2),               }^
{                               (4:PRI_INSNET1500), (5:PRI_ETSI),              }^
{                               (6:PRI_QSIG),       (7:PRI_DASS2).             }^
{                               (17:BRI_ETSI),      (18:BRI_CCITT QSIG),       }^
{                               (19:BRI_TSO13),     (20:BRI_1TR6),             }^
{                               (21:BRI_NTT),       (22:BRI_VNX)               }^
{DCH <dc>-                      (0:default)                                    }^
{L2Estab <l2e>-                 (1:Always; default), (0:On Demand).            }^
{IgnoreTonNPI <itnpi>-          (0:Observe TON and NPI)                        }^
{                               (128:Ignore TON and NPI)                       }^
{                               (145:Treated as TON of International, NPI of   }^
{                               ISDN)                                          }^
{RelayProgress <rp>-            (0:No) (1:Yes,default)                         }^
{DefaultANI <dani>-             (:Calling Party Number)                        }^
{T308 <t308>-                   (:timeout in secs)                             }^
{RejCallNoANI <rcnani>-         (0:Accept all calls)                           }^
{                               (1:Reject no/short ANI calls)                  }^
{ 				(2:Route no/short ANI calls to IVR             }^
{CauseRejNoANI <crnani>-        (:cause value when rejecting no ANI calls)     }^
{MinimumANILength <manil>-      (:minimum acceptable value of ANI)             }^
{OutBndBearerCap <obbc>-        (0:3.1KHz) (1:speech; default)                 }^
{RElayANI <reani>-              (0:No Relay ANI)                               }^
{                               (1:Relay ANI)                                  }^
{                               (2:Relay ANI with TON,NPI)                     }^
{                               (99:Get ANI from file)                         }^
{EtsiDiscNoInBand <ednib>-      (1:default, Prog Msg) (0:In one message)       }^
{NSFFacilityCodeValue <nsffcv>- (0:disabled,default)                           }^
{                               (1:SDN)                                        }^
{                               (2:Megacom 800)                                }^
{                               (3:Megacom)                                    }^
{                               (6:Accunet)                                    }^
{                               (7:Long Distance)                              }^
{                               (8:International 800)                          }^
{                               (16:AT&T Multiquest)                           }^
{DisconnectOnSuspend <dos>-     (0:suspend disconnect)                         }^
{                               (1:call disc upon on-hook)                     }^
{UseChannelExtensionBit <uceb>- (0:no chan ext bit)                            }^
{                               (1:use chan ext bit)                           }^
{DefaultANITON <daniton>-       (0:unknown,default)                            }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (3:Network Specific)                           }^
{                               (4:Subscriber)                                 }^
{                               (6:Abbreviated)                                }^
{DefaultANINPI <daninpi>-       (0:unknown,default)                            }^
{                               (1:ISDN,Telephony)                             }^
{                               (3:Data Numbering)                             }^
{                               (4:Telex Numbering)                            }^
{                               (8:National Standard Numbering)                }^
{                               (9:Private)                                    }^
{TEI <tei>-                     (:endpoint id)                                 }^
{                               (64:automatic)                                 }^
{DefaultANIScreenInd <danisi>-  (0:passthrough received)                       }^
{                               (1:user-provided)                              }^
{                               (2:user-provided,passed)                       }^
{                               (3:user-provided,failed)                       }^
{                               (4:network provided)                           }^
{RelayCallingNAMe <rcnam>-      (0:do not relay)                               }^
{                               (1:relay in ISDN or H.323)                     }^
{                               (2:relay in ISDN)                              }^
{                               (3:relay in DefaultCallingNAMe)                }^
{DefaultCallingNAMe <dcnam>-    (:calling name,15 alphanum)                    }^
{DefaultANIPresentationInd <danipi>-   (0:relay ANI)                           }^
{                                      (1:No ANI,set CLIR)                     }^
{                                      (2:Always set CLIR and Relay ANI)       }^
{T310 <t310>-                          (:numeric,default 30)                   }^
--------------------------------------------------------------------------------^
Set %ISDNSignalingGroup <parameter><value>                                      ^
   where <parameter> is:                                                        ^
                                                                                ^
&ORientation-                                                                   ^
             (0:User; default),                                                 ^
             (1:Network).                                                       ^
                                                                                ^
&PROTocol-                                                                      ^
             (0:PRI_5ESS; default), (1:PRI_4ESS),                               ^
             (2:PRI_DMS),           (3:PRI_NI2),                                ^
             (4:PRI_INSNET1500),    (5:PRI_ETSI),                               ^
             (6:PRI_QSIG),          (7:PRI_DASS2),                              ^
             (17:BRI_ETSI),         (18:BRI_CCITT QSIG),                        ^
             (19:BRI_TSO13),        (20:BRI_1TR6),                              ^
             (21:BRI_NTT),          (22:BRI_VNX)                                ^
&DCH-                                                                           ^
             (0:default)                                                        ^
             (16:D-Channels for E1)                                             ^
             (24:D-Channels for T1)                                             ^
                                                                                ^
&L2Estab-                                                                       ^
             (1:Always;default),                                                ^
             (0:On Demand).                                                     ^
                                                                                ^
&IgnoreTonNPI-                                                                  ^
             (0:Observe TON and NPI)                                            ^
             (128:Ignore TON and NPI)                                           ^
             (145:Treated as TON of International, NPI of ISDN)                 ^
                                                                                ^
&RelayProgress-                                                                 ^
             (0:No)                                                             ^
             (1:Yes;default)                                                    ^
                                                                                ^
&DefaultANI-                                                                    ^
             (:Calling party number for out bound calls)                        ^
                                                                                ^
&T308-                                                                          ^
             (4:4 Secs, default)                                                ^
             (:Secs)                                                            ^
                                                                                ^
&RejCallNoANI-                                                                  ^
             (1:Yes) (0:No)                                                     ^
                                                                                ^
&CauseRejNoANI-                                                                 ^
             (:cause code value)                                                ^
                                                                                ^
&MinimumANILength-								^
             (:minimum acceptable value of ANI)	        	      		^						
										^
&OutBndBearerCap-                                                               ^
             (0:3.1KHz)                                                         ^
             (1:Speech; default)                                                ^
                                                                                ^
&RElayANI-                                                                      ^
             (0:No Relay ANI)                                                   ^
             (1:Relay ANI)                                                      ^
             (2:Relay ANI with TON,NPI)                                         ^
             (99:Get ANI from file)                                             ^
&EtsiDiscNoInBand-                                                              ^
            (1:Prog Msg separate from Disc),                                    ^
            (0:All in one message)                                              ^
                                                                                ^
&NSFFacilityCodeValue-          (0:disabled,default)                            ^
                                (1:SDN)                                         ^
                                (2:Megacom 800)                                 ^
                                (3:Megacom)                                     ^
                                (6:Accunet)                                     ^
                                (7:Long Distance)                               ^
                                (8:International 800)                           ^
                                (16:AT&T Multiquest)                            ^
&DisconnectOnSuspend-           (0:suspend disconnect)                          ^
                                (1:call disc upon on-hook)                      ^
&UseChannelExtensionBit-        (0:no chan ext bit)                             ^
                                (1:use chan ext bit)                            ^
&DefaultANITON-                 (0:unknown,default)                             ^
                                (1:International)                               ^
                                (2:National)                                    ^
                                (3:Network Specific)                            ^
                                (4:Subscriber)                                  ^
                                (6:Abbreviated)                                 ^
&DefaultANINPI-                 (0:unknown,default)                             ^
                                (1:ISDN,Telephony)                              ^
                                (3:Data Numbering)                              ^
                                (4:Telex Numbering)                             ^
                                (8:National Standard Numbering)                 ^
                                (9:Private)                                     ^
&TEI-                           (0-63:endpoint id)                              ^
                                (64:automatic)                                  ^
&DefaultANIScreenInd-           (0:passthrough received)                        ^
                                (1:user-provided)                               ^
                                (2:user-provided,passed)                        ^
                                (3:user-provided,failed)                        ^
                                (4:network provided)                            ^
&RelayCallingNAMe-              (0:do not relay)                                ^
                                (1:relay in ISDN or H.323)                      ^
                                (2:relay in ISDN)                               ^
                                (3:relay in DefaultCallingNAMe)                 ^
&DefaultCallingNAMe-            (:calling name,15 alphanum)                     ^
&DefaultANIPresentationInd-            (0:relay ANI)                            ^
                                       (1:No ANI,set CLIR)                      ^
                                       (2:Always set CLIR and Relay ANI)        ^
&T310-                                 (:numeric,default 30)                    ^
@2200~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <h323sg>.                                                         }^
{    H.323 Signaling Group is used to configure a multi-cast IP address for    }^
{    Gatekeeper discovery or for manually assigning a Gatekeeper.              }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <H323SignalingGroup>.                                               ^
     H.323 Signaling Group is used to configure a multi-cast IP address for     ^
     Gatekeeper discovery or for manually assigning a Gatekeeper.               ^
                                                                                ^
@2203~{------------------------------------------------------------------------}^
{Set H323sg <parameter><value>                                                 }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{PrimaryGateKeeperIPAddr <pgkipa>-   (:0.0.0.0-255.255.255.255)                }^
{                                                                              }^
{SecondaryGateKeeperIPAddr <sgkipa>- (:0.0.0.0-255.255.255.255)                }^
{                                                                              }^
{GRQPrimaryGK <grqpgk>-                                                        }^
{     (0:No, not allow)              (1:Yes, allow)                            }^
{                                                                              }^
{GRQSecondaryGK <grqsgk>-                                                      }^
{     (0:No, not allow)              (1:Yes, allow)                            }^
{                                                                              }^
{RelayProgress <rp>-                                                           }^
{     (1:Yes;default)                (0:No)                                    }^
{RegisterDN-                                                                   }^
{     (0:No register)                                                          }^
{     (1:GW prefixes)                                                          }^
{     (1:E.164 IDs)                                                            }^
{                                                                              }^
{IgnoreGrantedBandwidth <igb>-                                                 }^
{     (0:No, no ignore)              (1:Yes, ignore)                           }^
{                                                                              }^
{DefaultH245Tunneling <dht>-                                                   }^
{     (0:No, disables;default)       (1:Yes)                                   }^
{UsePartyNumber <upn>-                                                         }^
{     (0:Off)                                                                  }^
{     (1:Used in Setup only)                                                   }^
{     (2:Used in ARQ only)                                                     }^
{     (3:Used in both ARQ and Setup)                                           }^
{EarlyH245 <eh>-                                                               }^
{     (0:sent after connect)                                                   }^
{     (1:sent after alert)                                                     }^
{StartH245Collision <shc>-                                                     }^
{     (0:H245 not by spec)                                                     }^
{     (1:H245 by spec)                                                         }^
{AllowFSonly <afso>                                                            }^
{     (0:disconnect without H245)                                              }^
{     (1:no disconnect without H245)                                           }^
{IgnoreFSifH245Addr-                                                           }^
{     (0:default;does Faststart)                                               }^
{     (1:no Faststart)                                                         }^
{MediaAfterConnect-                                                            }^
{        (0:default;opens H245 immediately)                                    }^
{        (1:opens H245 after Q.931)                                            }^
{CRDoInboundARQ-                                                               }^
{        (0:default;disables inbound ARQ)                                      }^
{        (1:enables inbound ARQ)                                               }^
{AutoExtIP <aeip>-                                                             }^
{        (0:disable)                                                           }^
{        (1:enable)                                                            }^
{RRQV3Plus <rrqv3p>-                                                           }^
{     (0:Don't use V3 plus)                                                    }^
{     (1:Use V3 plus)                                                          }^
{MuxServerPort                                                                 }^
{     (:port number)                                                           }^
{MuxCAPability <mcap>-                                                         }^
{     (0:Disabled)                                                             }^
{     (1:Multiplex Client)                                                     }^
{     (2:Server)                                                               }^
{     (3:Multiplex Client & Server)                                            }^
{MuxEndpoint1Port <me1p>-                                                      }^
{     (:port number)                                                           }^
{MuxEndpoint1IPAddr <me1ipa>-                                                  }^
{     (:no IP address)                                                         }^
{MuxEndpoint2Port <me2p>-                                                      }^
{     (:port number)                                                           }^
{MuxEndpoint2IPAddr <me2ipa>-                                                  }^
{     (:IP address)                                                            }^
{MuxEndpoint3Port <me3p>-                                                      }^
{     (:port number)                                                           }^
{MuxEndpoint3IPAddr <me3ipa>-                                                  }^
{     (:IP address)                                                            }^
{MuxEndpoint4Port <me4p>-                                                      }^
{     (:port number)                                                           }^
{MuxEndpoint4IPAddr <me4ipa>-                                                  }^
{     (:IP address)                                                            }^
{H323ID <h323id>-                                                              }^
{     (:Alphnum string,1-31                                                    }^
{                                                                              }^
{TimeOutRIP <torip>-                                                           }^
{     (:timeout setting in secs)                                               }^
{                                                                              }^
{LightWeightRRQ <lwrrq>-                                                       }^
{     (0:No;default)    (1:Yes)                                                }^
{                                                                              }^
{GateWayType <gwt>-                                                            }^
{     (0:h323gw;default)   (1:VoIP GW)                                         }^
{                                                                              }^
{H245TimerVal <h245tv>-                                                        }^
{     (:Seconds)                                                               }^
{DirectGWRouting <dgwr>-                                                       }^
{     (0:disabled)                                                             }^
{     (1:LRQ,then GK)                                                          }^
{     (2:GK,then local)                                                        }^
{     (3:LRQ,GK on timeout)                                                    }^
{REServed <res>-                                                               }^
{     (:user specific)                                                         }^
{RRQInterval  <rrqi>-                                                          }^
{     (:0-65535,0 default)                                                     }^
{AllowURQ <aurq>-                                                              }^
{     (0:disabled)                                                             }^
{     (1:enabled)                                                              }^
{H323GWPrefix <h323gwp>-                                                       }^
{     (:Alphnumeric string)                                                    }^
{                                                                              }^
{RTPVerify <rtpv>-                                                             }^
{     (0:disabled)                                                             }^
{     (1:enabled)                                                              }^
{GKBusyOut <gkbo>-   (:0-10,retry num)                                         }^
--------------------------------------------------------------------------------^
Set %H323SignalingGroup <parameter><value>                                      ^
   where <parameter> is:                                                        ^
                                                                                ^
&PrimaryGateKeeperIPAddr-                                                       ^
     (0.0.0.0: Default)                                                         ^
     (:0.0.0.0-255.255.255.255)                                                 ^
                                                                                ^
&SecondaryGateKeeperIPAddr-                                                     ^
     (0.0.0.0:default)                                                          ^
     (:0.0.0.0-255.255.255.255)                                                 ^
                                                                                ^
&GRQPrimaryGK-                                                                  ^
     (0:No, do not allow)     (1:Yes, allow)                                    ^
                                                                                ^
&GRQSecondaryGK-                                                                ^
     (0:No, do not allow)          (1:Yes, allow)                               ^
                                                                                ^
&RegisterDN-                                                                    ^
     (0:No register)                                                            ^
     (1:GW Prefixes)                                                            ^
     (2:E.164 IDs)                                                              ^
                                                                                ^
&RelayProgress-                                                                 ^
     (0:No)                   (1:Yes,default)                                   ^
&IgnoreGrantedBandwidth-                                                        ^
     (0:No, not ignore)       (1:Yes, ignore)                                   ^
                                                                                ^
&DefaultH245Tunneling-                                                          ^
     (0:No,disabled;default) (1:enabled)                                        ^
                                                                                ^
&H323ID-                                                                        ^
     (:Alphnum string,1-31)                                                     ^
                                                                                ^
&TimeOutRIP-                                                                    ^
     (:seconds)                                                                 ^
                                                                                ^
&LightWeightRRQ-                                                                ^
    (0:Disable LwRRQ; default),                                                 ^
    (1:Enable LwRRQ)                                                            ^
                                                                                ^
&GateWayType-                                                                   ^
     (0:H323 GW; default),                                                      ^
     (1:VoIP GW)                                                                ^
                                                                                ^
&UsePartyNumber-                                                                ^
          (0:Off)                                                               ^
          (1:Used in Setup only)                                                ^
          (2:Used in ARQ only)                                                  ^
          (3:Used in both ARQ and Setup)                                        ^
                                                                                ^
                                                                                ^
&EarlyH245-                                                                     ^
          (0:sent after connect)                                                ^
          (1:sent after alert)                                                  ^
                                                                                ^
&StartH245Collision-                                                            ^
         (0:H245 not by spec)                                                   ^
         (1:H245 by spec)                                                       ^
                                                                                ^
&AllowFSOnly-                                                                   ^
          (0:disconnect without H245)                                           ^
          (1:no disconnect without H245)                                        ^
                                                                                ^
&IgnoreFSifH245Addr-                                                            ^
         (0:default;does Faststart)                                             ^
         (1:no Faststart)                                                       ^
                                                                                ^
&MediaAfterConnect-                                                             ^
         (0:default; opens H245 immediately)                                    ^
         (1:opens H245 after Q.931)                                             ^
                                                                                ^
&CRDoInboundARQ-                                                                ^
         (0:default;disables inbound ARQ)                                       ^
         (1:enables inbound ARQ)                                                ^
                                                                                ^
&AutoExtIP-                                                                     ^
         (0:disable)                                                            ^
         (1:enable)                                                             ^
                                                                                ^
&H245TimerVal-                                                                  ^
         (:Seconds)                                                             ^
                                                                                ^
&RRQV3Plus-                                                                     ^
     Sets whether or not to use V3 plus for RRQ packets.                        ^
         (0:Don't use V3 plus)                                                  ^
         (1:Use V3 plus)                                                        ^
                                                                                ^
&MuxServerPort-                                                                 ^
         (:port number )                                                        ^
                                                                                ^
&MuxCAPability-                                                                 ^
         (0:Disabled)                                                           ^
         (1:Multiplex Client)                                                   ^
         (2:Server)                                                             ^
         (3:Multiplex Client & Server)                                          ^
                                                                                ^
&MuxEndpoint1Port-                                                              ^
         (:port number)                                                         ^
                                                                                ^
&MuxEndpoint1IPAddr-                                                            ^
         (:IP address)                                                          ^
                                                                                ^
&MuxEndpoint2Port-                                                              ^
         (:port number)                                                         ^
                                                                                ^
&MuxEndpoint2IPAddr-                                                            ^
         (:IP address)                                                          ^
                                                                                ^
&MuxEndpoint3Port-                                                              ^
         (:port number)                                                         ^
                                                                                ^
&MuxEndpoint3IPAddr-                                                            ^
         (:IP address)                                                          ^
                                                                                ^
&MuxEndpoint4Port-                                                              ^
         (:port number)                                                         ^
                                                                                ^
&MuxEndpoint4IPAddr-                                                            ^
         (:IP address)                                                          ^
&DirectGWRouting-                                                               ^
         (0:disabled)                                                           ^
         (1:LRQ,then GK)                                                        ^
         (2:GK,then local)                                                      ^
         (3:LRQ,GK on timeout)                                                  ^
&REServed-                                                                      ^
         (:user specific)                                                       ^
&RRQInterval-                                                                   ^
         (:0-65535,0 default)                                                   ^
&AllowURQ-                                                                      ^
         (0:disabled)                                                           ^
         (1:enabled)                                                            ^
&H323GWPrefix-                                                                  ^
        (:Alphnumeric string)                                                   ^
&RTPVerify-                                                                     ^
      (0:disabled)                                                              ^
      (1:enabled)                                                               ^
                                                                                ^
&GKBusyOut-   (:0-10,retry num)                                                 ^
@2300~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <tcrg>.                                                           }^
{    A Trunk Circuit Routing Group is a collection  of T1 or E1 channels used  }^
{    to connect the Tenor to a public switched telephone network <trunk        }^
{    circuit>.                                                                 }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <TrunkCircuitRoutingGroup>.                                         ^
     A Trunk Circuit Routing Group is a collection  of T1 or E1 channels used   ^
     to connect the Tenor to a public switched telephone network <trunk         ^
     circuit>.                                                                  ^
                                                                                ^
@2303~{------------------------------------------------------------------------}^
{Set tcrg <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                       (:read only)                                   }^
{name <name>-                   (:name)                                        }^
{OverlapDial <od>-              (0:No, default), (1:Yes)                       }^
{DIRection <dir>-               (0:Incoming), (1:Outgoing), (2:Bi-dir; default)}^
{ProgressTone <pt>-             (0:Off; default), (1:On).                      }^
{PubOrPrivNumPlan <popnp>-      (0:Public; default), (1:Private)               }^
{EndOfDial <eod>-               (0:Disable default), (1:Enable)                }^
{EndOfDialDigit <eodd>-         (#:Default: Ending Digit) (:0-9,#,*)           }^
{AddEndOfDialDigit <aeodd>-     (0:No; default), (1:Yes)                       }^
{ForcedRoutingNum <frn>-        (:A Dialed Number)                             }^
{ForcedRoutingNumType <frnt>-   (0:Public), (1:Private)                        }^
{TrunkID <tid>-                 (:Numeric string)                              }^
{                               (:#,*)                                         }^
{TrunkIDDelivery <tidd>-        (0:No Delivery; default)                       }^
{                               (1:Calling Party Number)                       }^
{                               (2:Called Party Number)                        }^
{                                                                              }^
{TrunkIDDeliveryFormat <tiddf>- (d:Destination Number; default)                }^
{                               (c:Trunk ID)                                   }^
{                               (o:Origination DN)                             }^
{                               (:0-9,*,#,literal character)                   }^
{                                                                              }^
{HUNTAlgorithm <hunta>-         (0:Ascending)                                  }^
{                               (1:Descending; default)                        }^
{                               (2:Acending-Round-Robin)                       }^
{                               (3:Decendng-Round-Robin)                       }^
{                                                                              }^
{ModemBypass <mb>-              (0:Disable)                                    }^
{                               (1:Enable, default)                            }^
{                               (2:MoIP)                                       }^
{PassThroughEnable <pte>-       (0:No; default)                                }^
{                               (1:Yes)                                        }^
{                               (2:low priority passthru)                      }^
{                               (3:channelized passthru)                       }^
{PassThroughID <ptid>-          (0:Idx of LCRG to passthru RG)                 }^
{MaxHopoffCallsAllowed <mhca>-  (24:default) (:1-32767;24 default)             }^
{BusyOut <bo>-                  (0:Ring Back)                                  }^
{                               (1:Ring back,then Off Hook)                    }^
{                               (2:Immediately Off Hook)                       }^
{                                                                              }^
{IVRType <ivrt>-                (0:No IVR; default)                            }^
{                               (1:Second Dial Tone)                           }^
{                               (2:Prepaid Calling Card)                       }^
{                               (3:Postpaid Account)                           }^
{                               (4:ANI Auth.Type 1)                            }^
{                               (5:ANI Auth.Type 2)                            }^
{                               (6:Postpaid Acc.Type 2)                        }^
{                               (7:Hear full msg before 2ND DT)                }^
{                               (8:Message before 2nd dial tone)               }^
{                               (9:Single stage pass through authentication)   }^
{                               (11:Prepaid or Postpaid)                       }^
{PIN <pin>-                     (:0-9 or x)                                    }^
{IVRAccessNumber <ivran>-       (:up to 13 digit string)                       }^
{IVRAnswerDelay <ivrad>-        (0:msec, default)                              }^
{IVRAccountNumLength <ivranl>-  (255:variable)                                 }^
{                               (1-20:accnt length)                            }^
{IVRPinNumLength <ivrpnl>-      (0-14:pin)                                     }^
{                               (255:variable)                                 }^
{IVRCardNumLength <ivrcnl>-     (1-20:card length)                             }^
{                               (255:variable)                                 }^
{IVRLanguage <ivrl>-            (0:English)                                    }^
{                               (1:Farsi)                                      }^
{                               (2:Mandarin Chinese)                           }^
{                               (3:French)                                     }^
{                               (4:Spanish)                                    }^
{                               (5:German)                                     }^
{                               (6:Arabic)                                     }^
{                               (7:Russian)                                    }^
{                               (8:Cantonese Chinese)                          }^
{                               (9:Turkish)                                    }^
{                               (:language)                                    }^
{IVRMultiSession <ivrms>-       (:##|**multisession on)                        }^
{IVRRetries <ivrr>-             (+1 - +10:retry,default 1)                     }^
{IVRDisablePrompt <ivrdp>-      (0:enable amt,time)                            }^
{                               (1:disable credit amt)                         }^
{                               (2:disable credit time)                        }^
{                               (3:disable amt,time)                           }^
{IPExtension <ipe>-             (0:No default), (1:Yes)                        }^
{TwoStageDialing <tsd>-         (0:No)(1:Yes)                                  }^
{AccessNumber <an>-             (:0-9*# up to 20 digits)                       }^
{AccessFormat <af>-             (d:Original DNIS)                              }^
{                               (c:Trunk ID)                                   }^
{                               (o:Calling Party Number)                       }^
{                               (,:comma adds 1 sec delay)                     }^
{                               (:0-9,*,# literal character)                   }^
{ProvideAutoSwitchProgressTone <paspt>-                                        }^
{                               (0:No;default)                                 }^
{                               (1:Yes)                                        }^
{Hairpinning <h>-                                                              }^
{                               (0:No;default)                                 }^
{                               (1:Yes)                                        }^
{IVRPreAuthentication <ivrpa>-                                                 }^
{                               (0:Disabled                                    }^
{                               (1:ANI)                                        }^
{                               (2:DNIS)                                       }^
{EnableExternalRouting <eer>-                                                  }^
{                               (0:No; Default)                                }^
{                               (1:Yes; ri-routingserver)                      }^
{MaxTalkTime <mtt>-                                                            }^
{                               (:Mins,default 0)                              }^
{AutoSwitchNumberAttached <asna>-                                              }^
{                               (:A full E.164 number)                         }^
{HopoffNumberDirAttached <hnda> -                                              }^
{                               (:idx of hopoff ND)                            }^
{InBoundAccessLevel <ibal>-                                                    }^
{                               (:Access level between 0 and 127)              }^
{                                                                              }^
{OutBoundAccessLevel <obal>-                                                   }^
{                               (:Access level between 0 and 127)              }^
{StopAcctID <said> -                                                           }^
{                               (0:IP Addr,default)                            }^
{                               (1:TrunkID of IC RG)                           }^
{                               (2:DNIS)                                       }^
{                               (3:Remote Signaling IP)                        }^
{                               (4:Term Signaling IP)                          }^
{                               (5:ANI)                                        }^
{                                                                              }^
{CallerIDType <cidt> -                                                         }^
{                               (0:Caller ID)                                  }^
{                               (1:TrunkID)                                    }^
{                               (2:Trunk ID + CallerID)                        }^
{                               (5:Prefix + CallerID)                          }^
{                                                                              }^
{IVRAllowDID <ivradid> -                                                       }^
{                               (0:No;Default)                                 }^
{                               (1:Yes)                                        }^
{Play1700Prompt <p1700p> -                                                     }^
{                               (0:No;Default)                                 }^
{                               (1:Yes)                                        }^
{PrefiXTrunkID <pxtid> -                                                       }^
{                               (0:No;Default)                                 }^
{                               (1:Yes)                                        }^
{AnswerDisconnectTone <adt>-    (0:disabled,default)                           }^
{                               (1:answer only)                                }^
{                               (2:disconnect only)                            }^
{                               (3:answer and disconnect)                      }^
{AnswerToneDuration <atd>-      (:ms,200 default)                              }^
{TranslateInboundANI <tiani>-   (0:no translation,default)                     }^
{                               (1:translation done)                           }^
{OutboundANINumDigits <oanind>- (0:caller id sent out)                         }^
{                               (:numeric,caller id sent)                      }^
{OutboundCallDetectionEnable <ocde>-   (0:disable,default)                     }^
{                                      (1:enable)                              }^
{AutoSwitchNumber <asn>-                                                       }^
{                               (:DN)                                          }^
{                                                                              }^
{AutoSwitchNumberType <asnt>-                                                  }^
{                               (0:DID received)                               }^
{                               (1:No DID received)                            }^
{HolD <hd>-                     (0:disable)                                    }^
{                               (1:enable)                                     }^
{HoldKeystroke <hk>-            (:alphanumeric,def 46)                         }^
{UnattendedTRansfer <utr>-      (0:disable)                                    }^
{                               (1:enable)                                     }^
{UnattendedTransferKeystroke <utk>-   (:alphanumeric,def 90)                   }^
{AttendedTRansfer <atr>-        (0:disable)                                    }^
{                               (1:enable)                                     }^
{AttendedTransferKeystroke <atk>-    (:alphanumeric,def HU)                    }^
{CallHangupKeystroke <chk>-      (:alphanumeric,def 48)                        }^
{CallWaiting <cw>-               (0:disable)                                   }^
{                                (1:enable)                                    }^
{AttendedXfrDiscExpiryTimer <axdet>-    (:seconds,def 5)                       }^
{CallWaitToConfKeystroke <cwtcf>-       (:keystroke,def 22)                    }^
{IVRAuthType <ivrat>-                   (0:ANI)                                }^
{                                       (6:DNIS Based)                         }^
{                                       (7:Normalized DNIS)                    }^
{CallTerminationINDication <ctind>-     (0:disable)                            }^
{                                       (1:enable)                             }^
--------------------------------------------------------------------------------^
Set %TrunkCircuitRoutingGroup <parameter><value>                                ^
   where <parameter> is:                                                        ^
                                                                                ^
&id <id>-                                                                       ^
             (:read only)                                                       ^
                                                                                ^
&name <name>-                                                                   ^
             (:name)                                                            ^
&OverlapDial -                                                                  ^
             (0:No, default),                                                   ^
             (1:Yes)                                                            ^
                                                                                ^
&DIRection -                                                                    ^
             (0:Incoming),                                                      ^
             (1:Outgoing),                                                      ^
             (2:Bi-direction;default)                                           ^
                                                                                ^
&ProgressTone-                                                                  ^
             (0:Off;default),                                                   ^
             (1:On).                                                            ^
                                                                                ^
&PubOrPrivNumPlan-                                                              ^
             (0:Public;default),                                                ^
             (1:Private)                                                        ^
                                                                                ^
&EndOfDial-                                                                     ^
             (0:Disable;default),                                               ^
             (1:Enable).                                                        ^
                                                                                ^
&EndOfDialDigit-                                                                ^
             (:#,*,0-9)                                                         ^
             (#:default;#,*,0-9)                                                ^
                                                                                ^
&AddEndOfDialDigit-                                                             ^
             (0:No;default)                                                     ^
             (1:Yes)                                                            ^
                                                                                ^
&ForcedRoutingNum-                                                              ^
             (:A Dialed Number)                                                 ^
                                                                                ^
&ForcedRoutingNumType-                                                          ^
             (0:Public; default)                                                ^
             (1:Private)                                                        ^
                                                                                ^
&TrunkID-                                                                       ^
             (:Numeric string)                                                  ^
             (:#,*)                                                             ^
                                                                                ^
&TrunkIDDelivery-                                                               ^
             (0:No Delivery)                                                    ^
             (1:Calling Party Number)                                           ^
             (2:Called Party Number)                                            ^
                                                                                ^
&TrunkIDDeliveryFormat-                                                         ^
             (d:Destination Number)                                             ^
             (c:Trunk ID)                                                       ^
             (o:Origination DN)                                                 ^
             (:0-9,*,#,literal character)                                       ^
                                                                                ^
&HUNTAlgorithm-                                                                 ^
             (0:Ascending)                                                      ^
             (1:Descending; default)                                            ^
             (2:Ascending-Round-Robin)                                          ^
             (3:Descending-Round-Robin)                                         ^
                                                                                ^
&ModemBypass-                                                                   ^
             (0:Disabled)                                                       ^
             (1:Enabled)                                                        ^
             (2:MoIP)                                                           ^
                                                                                ^
&PassThroughEnable-                                                             ^
             (0:No; default),                                                   ^
             (1:Yes).                                                           ^
             (2:Yes,try IP first)                                               ^
             (3:Yes,block of channels)                                          ^
&PassThroughID-                                                                 ^
             (0:Idx of a LCRG;default)                                          ^
             (:Idx of a LCRG)                                                   ^
                                                                                ^
&MaxHopoffCallsAllowed-                                                         ^
             (:1-32767; 24 default)                                             ^
             (24:default)                                                       ^
                                                                                ^
&BusyOut-                                                                       ^
             (0:Ring Back)                                                      ^
             (1:Ring back,then Off Hook)                                        ^
             (2:Immediately Off Hook)                                           ^
                                                                                ^
&IVRType-                                                                       ^
                                (0:No IVR; default)                             ^
                                (1:Second Dial Tone)                            ^
                                (2:Prepaid Calling Card)                        ^
                                (3:Postpaid Acc.Type 1)                         ^
                                (4:ANI Auth.Type 1)                             ^
                                (5:ANI Auth.Type 2)                             ^
                                (6:Postpaid Acc.Type 2)                         ^
                                (7:Hear full msg before 2ND DT)                 ^
                                (8:Message before 2nd dial tone)                ^
                                (9:Single stage pass through authentication)    ^
                                (11:Prepaid or Postpaid)                        ^
&PIN-                                                                           ^
                                (:0-9 or x).                                    ^
                                                                                ^
&IVRAccessNumber-                                                               ^
                                (:Up to 13 digit string)                        ^
                                                                                ^
&IVRAnswerDelay-                                                                ^
                                (0:msec;default)                                ^
                                                                                ^
&IVRAccountNumLength-                                                           ^
                                (255:variable)                                  ^
                                (1-20:account length)                           ^
&IVRPinNumLength-                                                               ^
                                (0-14:pin)                                      ^
                                (255:variable)                                  ^
&IVRCardNumLength-              (1-20:card length)                              ^
                                (255:variable)                                  ^
                                                                                ^
&IVRLanguage-                                                                   ^
                                 (0:English)                                    ^
                                 (1:Farsi)                                      ^
                                 (2:Mandarin Chinese)                           ^
                                 (3:French)                                     ^
                                 (4:Spanish)                                    ^
                                 (5:German)                                     ^
                                 (6:Arabic)                                     ^
                                 (7:Russian)                                    ^
                                 (8:Cantonese Chinese)                          ^
                                 (9:Turkish)                                    ^
                                 (:language)                                    ^
&IVRMultiSession-                                                               ^
                                 (:##|**multisession on)                        ^
                                                                                ^
&IVRRetries-                     (+1 - +10:retry,default 1)                     ^
&IVRDisablePrompt -             (0:enable amt,time)                             ^
                                (1:disable credit amt)                          ^
                                (2:disable credit time)                         ^
                                (3:disable amt,time)                            ^
&IPExtension-                                                                   ^
             (0:No)                                                             ^
             (1:Yes)                                                            ^
                                                                                ^
&TwoStageDialing-                                                               ^
          (0:No)                                                                ^
          (1:Yes)                                                               ^
                                                                                ^
&AccessNumber-                                                                  ^
          (:0-9*# up to 20 digits)                                              ^
                                                                                ^
&AccessFormat-                                                                  ^
         (d:Original DNIS)                                                      ^
         (c:Trunk ID)                                                           ^
         (o:Calling Party Number)                                               ^
         (,:comma adds 1 sec delay)                                             ^
         (:0-9,*,# literal character)                                           ^
                                                                                ^
&ProvideAutoSwitchProgressTone-                                                 ^
     (0:No,Default)                                                             ^
     (1:Yes)                                                                    ^
                                                                                ^
&Hairpinning-                                                                   ^
     (0:No,Default)                                                             ^
     (1:Yes)                                                                    ^
                                                                                ^
&IVRPreAuthentication-                                                          ^
     (0:Disabled)                                                               ^
     (1:ANI)                                                                    ^
     (2:DNIS)                                                                   ^
                                                                                ^
&EnableExternalRouting-                                                         ^
     (0:No; Default)                                                            ^
     (1:Yes; ri-routingserver)                                                  ^
                                                                                ^
&MaxTalkTime-                                                                   ^
     (:Mins,default 0)                                                          ^
                                                                                ^
&AutoSwitchNumberAttached-                                                      ^
     (:A full E.164 number)                                                     ^
                                                                                ^
&HopoffNumberDirAttached-                                                       ^
     (:Index of Hop-Off Directory)                                              ^
&InBoundAccessLevel-                                                            ^
     (:0 to 127)                                                                ^
                                                                                ^
&OutBoundAccessLevel-                                                           ^
     (:0 to 127)                                                                ^
                                                                                ^
&StopAcctID-                                                                    ^
           (0:IP Addr,default)                                                  ^
           (1:TrunkID of IC RG)                                                 ^
           (2:DNIS)                                                             ^
           (3:Remote Signaling IP)                                              ^
           (4:Term Signaling IP)                                                ^
           (5:ANI)                                                              ^
&CallerIDType-                                                                  ^
            (0:Caller ID)                                                       ^
            (1:TrunkID)                                                         ^
            (2:Trunk ID + CallerID)                                             ^
            (5:Prefix + CallerID)                                               ^
                                                                                ^
&IVRAllowDID-                                                                   ^
            (0:No;Default)                                                      ^
            (1:Yes)                                                             ^
                                                                                ^
&Play1700Prompt-                                                                ^
                                (0:No;Default)                                  ^
                                (1:Yes)                                         ^
                                                                                ^
&PrefiXTrunkID-                                                                 ^
                                (0:No;Default)                                  ^
                                (1:Yes)                                         ^
                                                                                ^
&AnswerDisconnectTone-          (0:disabled,default)                            ^
                                (1:answer only)                                 ^
                                (2:disconnect only)                             ^
                                (3:answer and disconnect)                       ^
&AnswerToneDuration-            (:ms,200 default)                               ^
&TranslateInboundANI-           (0:no translation,default)                      ^
                                (1:translation done)                            ^
&OutboundANINumDigits-          (0:caller id sent out)                          ^
                                (:numeric,caller id sent)                       ^
&OutboundCallDetectionEnable-   (0:disable,default)                             ^
                                (1:enable)                                      ^
&AutoSwitchNumber-                                                              ^
                                (:DN)                                           ^
                                                                                ^
&AutoSwitchNumberType-                                                          ^
                                (0:DID received)                                ^
                                (1:No DID received)                             ^
&HolD-                          (0:disable)                                     ^
                                (1:enable Hold)                                 ^
&HoldKeystroke-                 (:alphanumeric,def 46)                          ^
&UnattendedTRansfer-            (0:disable)                                     ^
                                (1:enable)                                      ^
&UnattendedTransferKeystroke-   (:alphanumeric,def 90)                          ^
&AttendedTRansfer-              (0:disable)                                     ^
                                (1:enable)                                      ^
&AttendedTransferKeystroke-     (:alphanumeric,def HU)                          ^
&CallHangupKeystroke-           (:alphanumeric,def 48)                          ^
&CallWaiting-                    (0:disable)                                    ^
                                 (1:enable)                                     ^
&AttendedXfrDiscExpiryTimer-    (:seconds,def 5)                                ^
&CallWaitToConfKeystroke-       (:keystroke,def 22)                             ^
&IVRAuthType-                   (0:ANI)                                         ^
                                (6:DNIS Based)                                  ^
                                (7:Normalized DNIS)                             ^
&CallTerminationINDication-     (0:disable)                                     ^
                                (1:enable)                                      ^
@2400~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <lcrg>.                                                           }^
{    The Line Circuit Routing Group is a collection of T1 or E1 channels used  }^
{    to connect the Tenor unit to line-side. Also LineCircuitRoutingGroup has  }^
{    features that are unique to it and only available when configured here.   }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <LineCircuitRoutingGroup>.                                          ^
     The Line Circuit Routing Group is a collection of T1 or E1 channels used to^
     connect the Tenor unit to line-side. Also LineCircuitRoutingGroup has      ^
     features that are unique to it and only available when configured here.    ^
                                                                                ^
@2403~{------------------------------------------------------------------------}^
{Set lcrg <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                       (:read only)                                   }^
{name <name>-                   (:name)                                        }^
{OverlapDial <od>-              (0:No), (1:Yes, default)                       }^
{DIRection <dir>-               (0:Incoming), (1:Outgoing), (2:Bi-dir; default)}^
{ProgressTone <pt>-             (0:Off), (1:On;default).                       }^
{PubOrPrivNumPlan <popnp>-      (0:Public; default), (1:Private).              }^
{EndOfDial <eod>-               (0:Disable; default), (1:Enable).              }^
{                                                                              }^
{EndOfDialDigit <eodd>-         Available only when EndOfDial is enabled.      }^
{                               (:#,*,0-9)  (#:default)                        }^
{                                                                              }^
{AddEndOfDialDigit <aeodd>-     Available only when EndOfDial is Enabled.      }^
{                               (0:No; default)                                }^
{                               (1:Yes)                                        }^
{                                                                              }^
{ForcedRoutingNum <frn>-        (:A Dailed Number)                             }^
{ForcedRoutingNumType <frnt>-   (0:Public; default), (1:Private).              }^
{TrunkID <tid>-                 (:Numeric String)                              }^
{                               (:#,*)                                         }^
{TrunkIDDelivery <tidd>-        (0:No Delivery; default)                       }^
{                               (1:Calling Party Number)                       }^
{                               (2:Called Party Number).                       }^
{                                                                              }^
{TrunkIDDeliveryFormat <tiddf>- (0:Destination Number)                         }^
{                               (1:Trunk ID)                                   }^
{                               (2:Original Destination Num)                   }^
{                                                                              }^
{HUNTAlgorithm <hunta>-         (0:Ascending; default)                         }^
{                               (1:Descending)                                 }^
{                               (2:Ascending-RR)                               }^
{                               (3:Descending-RR).                             }^
{                                                                              }^
{ModemBypass <mb>-              (0:Disable)                                    }^
{                               (1:Enable; default)                            }^
{                               (2:MoIP)                                       }^
{                                                                              }^
{PassThroughEnable <pte>-       (0:No)                                         }^
{                               (1:Yes; default)                               }^
{                               (3:channelized passthru)                       }^
{                                                                              }^
{PassThroughID <ptid>-          (:Index of a LCRG)                             }^
{                                                                              }^
{PUBlicTON <pubton>-            (0:Unknown; default)                           }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (3:Local).                                     }^
{                                                                              }^
{PUBlicNPI <pubnpi>-            (0:Unknown; default)                           }^
{                               (1:ISDN)                                       }^
{                               (9:Private).                                   }^
{                                                                              }^
{PRIVateTON <privton>-          (0:Unknown; default)                           }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (3:Local).                                     }^
{                                                                              }^
{PRIVateNPI <privnpi>-          (0:Unknown; default)                           }^
{                               (1:ISDN)                                       }^
{                               (9:Private).                                   }^
{                                                                              }^
{PUBlicNumDigits <pubnd>-       (:Digits length of Pub DN)                     }^
{PRIVateNumDigits <privnd>-     (:Digits length of Priv DN)                    }^
{                                                                              }^
{EnableMultiPath <emp>-         (0:No, disable multi path)                     }^
{                               (1:Yes, default, enable multi path)            }^
{IVRType <ivrt>-                (0:No IVR; default)                            }^
{                               (1:Provide Second Dial Tone)                   }^
{                               (2:Prepaid Calling Card)                       }^
{                               (3:Postpaid Acc.Type 1)                        }^
{                               (4:ANI Auth.Type 1)                            }^
{                               (5:ANI Auth.Type 2)                            }^
{                               (6:Postpaid Acc.Type 2)                        }^
{                               (7:Hear full msg before 2ND DT)                }^
{                               (8:Message before 2nd dial tone)               }^
{                               (9:Single stage pass through authentication)   }^
{                               (11:Prepaid or Postpaid)                       }^
{PIN <pin>-                     (:String of 0-9 or x)                          }^
{IVRAccessNumber <ivran>-        (:Up to 13 digit string)                      }^
{IVRAnswerDelay <ivrad>-         (:msec;0,default)                             }^
{IVRAccountNumLength <ivranl>-   (1-20:acct length)                            }^
{                                (255:variable)                                }^
{IVRPinNumLength <ivrpnl>-       (0-14:pin length)                             }^
{                                (255:variable)                                }^
{IVRCardNumLength <ivrcnl>-      (1-20:card length)                            }^
{                                (255:variable)                                }^
{IVRLanguage <ivrl>-            (0:English)                                    }^
{                               (1:Farsi)                                      }^
{                               (2:Mandarin Chinese)                           }^
{                               (3:French)                                     }^
{                               (4:Spanish)                                    }^
{                               (5:German)                                     }^
{                               (6:Arabic)                                     }^
{                               (7:Russian)                                    }^
{                               (8:Cantonese Chinese)                          }^
{                               (9:Turkish)                                    }^
{                               (:language)                                    }^
{IVRRetries <ivrr>-             (+1 - +10:retry,default 1)                     }^
{IVRDisablePrompt <ivrdp>-      (0:enable amt,time)                            }^
{                               (1:disable credit amt)                         }^
{                               (2:disable credit time)                        }^
{                               (3:disable amt,time)                           }^
{IVRMultiSession <ivrms>-        ("":Disable )                                 }^
{                                (##:Enable)                                   }^
{                                (**:Enable)                                   }^
{                                                                              }^
{TwoStageDialing <tsd>-         (0:No, default)                                }^
{                               (1:Yes)                                        }^
{AccessNumber <an>-             (:0-9*# up to 20 digits)                       }^
{AccessFormat <af>-             (:0-9*# up to 40 digits)                       }^
{                                                                              }^
{IVRPreAuthentication <ivrpa>-                                                 }^
{                               (0:Disabled)                                   }^
{                               (1:ANI)                                        }^
{                               (2:DNIS)                                       }^
{EnableExternalRouting <eer>-                                                  }^
{                               (0:No; Default)                                }^
{                               (1:Yes; ri-routingserver)                      }^
{AutoSwitchNumberAttached <asna>-                                              }^
{                               (:A full E.164 number)                         }^
{                                                                              }^
{BypassNumberDirAttached <bnda> -(:Index of Bypass ND)                         }^
{                                                                              }^
{PUBhuntLdnDirAttached <publda> -                                              }^
{                               (:Index of Pub Hunt ND)                        }^
{                                                                              }^
{PRIVhuntLdnDirAttached <privlda>-                                             }^
{                               (:Index of Priv Hunt ND)                       }^
{                                                                              }^
{InBoundAccessLevel <ibal> -                                                   }^
{                               (:Access level between 0 and 127)              }^
{OutBoundAccessLevel <obal> -                                                  }^
{                               (:Access level between 0 and 127)              }^
{StopAcctID <said> -                                                           }^
{                               (0:IP Addr,default)                            }^
{                               (1:TrunkID of IC RG)                           }^
{                               (2:DNIS)                                       }^
{                               (3:Remote Signaling IP)                        }^
{                               (4:Term Signaling IP)                          }^
{                               (5:ANI)                                        }^
{CallerIDType <cidt> -                                                         }^
{                               (0:CallID or area + HLDN)                      }^
{                               (1:TrunkID)                                    }^
{                               (2:Trunk ID+CallerID)                          }^
{                               (3:CallID or area+LDN)                         }^
{                               (4:CallID or CC+area+LDN)                      }^
{IVRAllowDID <ivradid> -                                                       }^
{                               (0:No;Default)                                 }^
{                               (1:Yes)                                        }^
{Play1700Prompt <p1700p> -                                                     }^
{                               (0:No;Default)                                 }^
{                               (1:Yes)                                        }^
{PrefiXTrunkID <pxtid> -                                                       }^
{                               (0:No;Default)                                 }^
{                               (1:Yes)                                        }^
{PartialTG <ptg>-               (0:disabled,default)                           }^
{                               (1:enabled)                                    }^
{AnswerDisconnectTone <adt>-    (0:disabled,default)                           }^
{                               (1:answer only)                                }^
{                               (2:disconnect only)                            }^
{                               (3:answer and disconnect)                      }^
{AnswerToneDuration <atd>-      (:ms,200 default)                              }^
{TranslateInboundANI <tiani>-   (0:no translation,default)                     }^
{                               (1:translation done)                           }^
{OutboundANINumDigits <oanind>- (0:caller id sent out)                         }^
{                               (:numeric,caller id sent)                      }^
{OutboundCallDetectionEnable <ocde>-   (0:disable,default)                     }^
{                                      (1:enable)                              }^
{AutoSwitchNumber <asn>-                                                       }^
{                               (:DN)                                          }^
{                                                                              }^
{AutoSwitchNumberType <asnt>-                                                  }^
{                               (0:DID received)                               }^
{                               (1:No DID received)                            }^
{HolD <hd>-                     (0:disable)                                    }^
{                               (1:enable)                                     }^
{HoldKeystroke <hk>-            (:alphanumeric,def 46)                         }^
{UnattendedTRansfer <utr>-      (0:disable)                                    }^
{                               (1:enable)                                     }^
{UnattendedTransferKeystroke <utk>-   (:alphanumeric,def 90)                   }^
{AttendedTRansfer <atr>-        (0:disable)                                    }^
{                               (1:enable)                                     }^
{AttendedTransferKeystroke <atk>-    (:alphanumeric,def HU)                    }^
{CallHangupKeystroke <chk>-      (:alphanumeric,def 48)                        }^
{CallWaiting <cw>-               (0:disable)                                   }^
{                                (1:enable)                                    }^
{AttendedXfrDiscExpiryTimer <axdet>-    (:seconds,def 5)                       }^
{CallWaitToConfKeystroke <cwtcf>-       (:keystroke,def 22)                    }^
{IVRAuthType <ivrat>-                   (0:ANI)                                }^
{                                       (6:DNIS Based)                         }^
{                                       (7:Normalized DNIS)                    }^
{CallTerminationINDication <ctind>-     (0:disable)                            }^
{                                       (1:enable)                             }^
--------------------------------------------------------------------------------^
Set %LineCircuitRoutingGroup <parameter><value>                                 ^
   where <parameter> is:                                                        ^
                                                                                ^
&id <id>-                       (:read only)                                    ^
&name <name>-                   (:name)                                         ^
&OverlapDial -                                                                  ^
             (0:No),                                                            ^
             (1:Yes, default)                                                   ^
                                                                                ^
&DIRection-                                                                     ^
             (0:Incoming)                                                       ^
             (1:Outgoing)                                                       ^
             (2:Bi-dir; default)                                                ^
                                                                                ^
&ProgressTone-                                                                  ^
             (0:Off)                                                            ^
             (1:On;default).                                                    ^
                                                                                ^
&PubOrPrivNumPlan-                                                              ^
             (0:Public; default)                                                ^
             (1:Private).                                                       ^
                                                                                ^
&EndOfDial-                                                                     ^
             (0:Disable; default)                                               ^
             (1:Enable).                                                        ^
                                                                                ^
&EndOfDialDigit-                                                                ^
             (:#,*,0-9)                                                         ^
             (#:default;#,*,0-9)                                                ^
                                                                                ^
&AddEndOfDialDigit-                                                             ^
             (0:No; default)                                                    ^
             (1:Yes)                                                            ^
                                                                                ^
&ForcedRoutingNum-                                                              ^
             (:A Dialed Number)                                                 ^
                                                                                ^
&ForcedRoutingNumType-                                                          ^
             (0:Public; default)                                                ^
             (1:Private).                                                       ^
                                                                                ^
&TrunkID-                                                                       ^
             (:Numeric String)                                                  ^
             (:#,*)                                                             ^
                                                                                ^
&TrunkIDDelivery-                                                               ^
             (0:No Delivery; default)                                           ^
             (1:Calling Party Number)                                           ^
             (2:Called Party Number).                                           ^
                                                                                ^
&TrunkIDDeliveryFormat-                                                         ^
             (0:Destination Number)                                             ^
             (1:Trunk ID)                                                       ^
             (2:Original Destination Num).                                      ^
                                                                                ^
&HUNTAlgorithm-                                                                 ^
             (0:Ascending; default)                                             ^
             (1:Descending)                                                     ^
             (2:Ascending-Round-Robin)                                          ^
             (3:Descending-Round-Robin).                                        ^
                                                                                ^
&ModemBypass-                                                                   ^
             (0:Disabled)                                                       ^
             (1:Enabled, default)                                               ^
             (2:MoIP)                                                           ^
                                                                                ^
&PassThroughEnable-                                                             ^
             (0:No; default)                                                    ^
             (1:Yes)                                                            ^
             (3:Yes,block of channels)                                          ^
&PassThroughID-                                                                 ^
             (:Index of a LCRG)                                                 ^
             (0:Index of a LCRG; default)                                       ^
                                                                                ^
&PUBlicTON-                                                                     ^
             (0:Unknown; default)                                               ^
             (1:International)                                                  ^
             (2:National)                                                       ^
             (3:Local)                                                          ^
                                                                                ^
&PUBlicNPI-                                                                     ^
             (0:Unknown; default)                                               ^
             (1:ISDN)                                                           ^
             (9:Private)                                                        ^
                                                                                ^
&PRIVateTON-                                                                    ^
             (0:Unknown; default)                                               ^
             (1:International)                                                  ^
             (2:National)                                                       ^
             (3:Local)                                                          ^
                                                                                ^
&PRIVateNPI-                                                                    ^
             (0:Unknown; default)                                               ^
             (1:ISDN)                                                           ^
             (9:Private)                                                        ^
                                                                                ^
&PUBlicNumDigits-                                                               ^
         (7:default)                                                            ^
                                                                                ^
&PRIVateNumDigits-                                                              ^
        (4:default)                                                             ^
                                                                                ^
&EnableMultiPath-                                                               ^
        (0:No, disable multi path)                                              ^
        (1:Yes, default, enable multi path)                                     ^
                                                                                ^
&IVRType-                                                                       ^
                                (0:No IVR; default)                             ^
                                (1:Second Dial Tone)                            ^
                                (2:Prepaid Calling Card)                        ^
                                (3:Postpaid Acc.Type 1)                         ^
                                (4:ANI Auth.Type 1)                             ^
                                (5:ANI Auth.Type 2)                             ^
                                (6:Postpaid Acc.Type 2)                         ^
                                (7:Hear full msg before 2ND DT)                 ^
                                (8:Message before 2nd dial tone)                ^
                                (9:Single stage pass through authentication)    ^
                                (11:Prepaid or Postpaid)                        ^
&PIN-                                                                           ^
                  (:Pin code to verify 0-9 or x).                               ^
                                                                                ^
&IVRAccessNumber-                                                               ^
                  (:Up to 13 digit string)                                      ^
                                                                                ^
&IVRAnswerDelay-                                                                ^
                                (0:msec;default)                                ^
                                (:msec)                                         ^
                                                                                ^
&IVRAccountNumLength-            (1-20:acct length)                             ^
                                 (255:variable)                                 ^
                                                                                ^
&IVRPinNumLength-                                                               ^
                                 (0-14:pin length)                              ^
                                 (255:variable)                                 ^
                                                                                ^
&IVRCardNumLength-               (1-20:card length)                             ^
                                 (255:variable)                                 ^
                                                                                ^
&IVRLanguage-                                                                   ^
                                (0:English)                                     ^
                                (1:Farsi)                                       ^
                                (2:Mandarin Chinese)                            ^
                                (3:French)                                      ^
                                (4:Spanish)                                     ^
                                (5:German)                                      ^
                                (6:Arabic)                                      ^
                                (7:Russian)                                     ^
                                (8:Cantonese Chinese)                           ^
                                (9:Turkish)                                     ^
                                (:language)                                     ^
&IVRRetries-                    (+1 - +10:retry,default 1)                      ^
&IVRDisablePrompt-              (0:enable amt,time)                             ^
                                (1:disable credit amt)                          ^
                                (2:disable credit time)                         ^
                                (3:disable amt,time)                            ^
&IVRMultiSession-                                                               ^
                            ("":Disable;default)                                ^
                            (##:Enable )                                        ^
                            (**:Enable)                                         ^
&TwoStageDialing-                                                               ^
          (0:No, default)                                                       ^
          (1:Yes)                                                               ^
                                                                                ^
&AccessNumber-                                                                  ^
          (:0-9*# up to 20 digits)                                              ^
                                                                                ^
&AccessFormat-                                                                  ^
          (:0-9*# up to 40 digits)                                              ^
                                                                                ^
&IVRPreAuthentication-                                                          ^
             (0:Disabled)                                                       ^
             (1:ANI)                                                            ^
             (2:DNIS)                                                           ^
                                                                                ^
&EnableExternalRouting-                                                         ^
     (0:No; Default)                                                            ^
     (1:Yes; ri-routingserver)                                                  ^
                                                                                ^
&AutoSwitchNumberAttached-                                                      ^
     (:A full E.164 number)                                                     ^
                                                                                ^
&BypassNumberDirAttached-                                                       ^
     (:0-9,*;* for any index)                                                   ^
&PUBhuntLdnDirAttached-                                                         ^
     (:0-9,*;* for any index)                                                   ^
                                                                                ^
&PRIVhuntLdnDirAttached-                                                        ^
     (:0-9,*;* for any index)                                                   ^
                                                                                ^
&InBoundAccessLevel-                                                            ^
     (:Access level, 0 to 127)                                                  ^
                                                                                ^
&OutBoundAccessLevel-                                                           ^
     (:Access level, 0 to 127)                                                  ^
                                                                                ^
&StopAcctID-                                                                    ^
                                (0:IP Addr, default)                            ^
                                (1:TrunkID of IC RG)                            ^
                                (2:DNIS)                                        ^
                                (3:Remote Signaling IP)                         ^
                                (4:Term Signaling IP)                           ^
                                (5:ANI)                                         ^
                                                                                ^
&CallerIDType-                                                                  ^
                                (0:CallID or area + HLDN)                       ^
                                (1:TrunkID)                                     ^
                                (2:Trunk ID+CallerID)                           ^
                                (3:CallID or area+LDN)                          ^
                                (4:CallID or CC+area+LDN)                       ^
&IVRAllowDID-                                                                   ^
                                (0:No;Default)                                  ^
                                (1:Yes)                                         ^
                                                                                ^
&Play1700Prompt-                                                                ^
                                (0:No;Default)                                  ^
                                (1:Yes)                                         ^
                                                                                ^
&PrefiXTrunkID-                                                                 ^
                                (0:No;Default)                                  ^
                                (1:Yes)                                         ^
                                                                                ^
&PartialTG-                     (0:disabled,default)                            ^
                                (1:enabled)                                     ^
&AnswerDisconnectTone-          (0:disabled,default)                            ^
                                (1:answer only)                                 ^
                                (2:disconnect only)                             ^
                                (3:answer and disconnect)                       ^
&AnswerToneDuration-            (:ms,200 default)                               ^
&TranslateInboundANI-           (0:no translation,default)                      ^
                                (1:translation done)                            ^
&OutboundANINumDigits-          (0:caller id sent out)                          ^
                                (:numeric,caller id sent)                       ^
&OutboundCallDetectionEnable-   (0:disable,default)                             ^
                                (1:enable)                                      ^
&AutoSwitchNumber-                                                              ^
                                (:DN)                                           ^
                                                                                ^
&AutoSwitchNumberType-                                                          ^
                                (0:DID received)                                ^
                                (1:No DID received)                             ^
&HolD-                          (0:disable)                                     ^
                                (1:enable)                                      ^
&HoldKeystroke-                 (:alphanumeric,def 46)                          ^
&UnattendedTRansfer-            (0:disable)                                     ^
                                (1:enable)                                      ^
&UnattendedTransferKeystroke-   (:alphanumeric,def 90)                          ^
&AttendedTRansfer-              (0:disable)                                     ^
                                (1:enable)                                      ^
&AttendedTransferKeystroke-     (:alphanumeric,def HU)                          ^
&CallHangupKeystroke-            (:alphanumeric,def 48)                         ^
                                                                                ^
&CallWaiting-                    (0:disable)                                    ^
                                 (1:enable)                                     ^
&AttendedXfrDiscExpiryTimer-    (:seconds,def 5)                                ^
&CallWaitToConfKeystroke-       (:keystroke,def 22)                             ^
&IVRAuthType-                          (0:ANI)                                  ^
                                       (6:DNIS Based)                           ^
                                       (7:Normalized DNIS)                      ^
&CallTerminationINDication-             (0:disable)                             ^
                                        (1:enable)                              ^
@2500~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <tp>.                                                             }^
{    The ToneProfile is a profile used to configure various tone behaviors     }^
{    such as first tone frequency, second tone frequency, apply tone interval, }^
{    and no tone interval.                                                     }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <ToneProfile>                                                       ^
    The ToneProfile is a profile used to configure various tone behaviors such  ^
    as first tone frequency, second tone frequency, apply tone interval, and no ^
    tone interval.                                                              ^
                                                                                ^
@2501~{------------------------------------------------------------------------}^
{New tp <id>                   Create new ToneProfile named <id>               }^
{                                                                              }^
--------------------------------------------------------------------------------^
New ToneProfile <id>           Create new ToneProfile named <id>                ^
                                                                                ^
     Example:config-GateWay-1# new tp 2                                         ^
                                                                                ^
@2502~{------------------------------------------------------------------------}^
{Delete tp <id>                Delete existing ToneProfile named <id>          }^
{                                                                              }^
--------------------------------------------------------------------------------^
Delete ToneProfile <id>        Delete existing ToneProfile  named  <id>         ^
                                                                                ^
@2503~{------------------------------------------------------------------------}^
{Set tp <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{  id <id>-                           (:read only)                             }^
{                                                                              }^
{  name <name>-                       (:name)                                  }^
{  DiscToneFreq1    <dtf1>-           (:100-2000 Hz)                           }^
{    First tone frequency                                                      }^
{  DiscToneFreq2    <dtf2>-           (:100-2000 Hz)                           }^
{    Second tone frequency                                                     }^
{  DiscToneONTime   <dtont>-          (:0-2000 ms, default 0 ms)               }^
{    Apply tone interval                                                       }^
{  DiscToneOFFTime  <dtofft>-         (:0-2000 ms, default 0 ms)               }^
{    No tone interval                                                          }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %ToneProfile <parameter><value>                                             ^
   where <parameter> is:                                                        ^
                                                                                ^
&id <id>-                           (:read only)                                ^
                                                                                ^
&name <name>-                       (:name)                                     ^
&DiscToneFreq1-                                                                 ^
     First tone frequency   (:100-2000 Hz,default 480 Hz)                       ^
&DiscToneFreq2-                                                                 ^
     Second tone frequency  (:100-2000 Hz,default 600 Hz)                       ^
&DiscToneONTime-                                                                ^
     Apply tone interval    (0:0-2000 ms, default 0 ms)                         ^
&DiscToneOFFTime-                                                               ^
     No tone interval       (0:0-2000 ms, default 0 ms)                         ^
                                                                                ^
@2600~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <gkp>.                                                            }^
{    The Gatekeeper collects, manages, and distributes call routing information}^
{    in its zone. A Gatekeeper may have to communicate with the Border Element }^
{    to pass on all the routes its is handling.The Gatekeeper gets back all the}^
{    routes the Border Element passes on to it from other Gatekeepers. This way}^
{    our gatekeeper knows all the routes in a network. So in this prompt level }^
{    all the parameters for the Gatekeeper need to know are set.               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <GateKeeperParam>.                                                  ^
     The Gatekeeper collects, manages, and distributes call routing information ^
     in its zone. A Gatekeeper may have to communicate with the Border Element  ^
     to pass on all the routes its is handling. The Gatekeeper gets back all the^
     routes the Border Element passes on to it from other Gatekeepers. This way ^
     our gatekeeper knows all the routes in a network. So in this prompt level  ^
     all the parameters for the Gatekeeper need to know are set.                ^
                                                                                ^
@2603~{------------------------------------------------------------------------}^
{Set gkp <parameter><value>                                                    }^
{   where <parameter> is:                                                      }^
{RegistrationPort <rp>-         (:RAS Port)                                    }^
{GKListeningPort <gklp>-        (:GK Discovery Port)                           }^
{PrimaryBEIPAddr <pbeipa>-      (:IP Address)                                  }^
{SecondaryBEIPAddr <sbeipa>-    (:IP Address)                                  }^
{ZoneName <zn>-                 (:Up to 31 chars).                             }^
{PassWord <pw>-                 (:Alphanumeric string)                         }^
{EPRadiusAuthorization <EPRA>-  (0:No;default)                                 }^
{                               (1:Yes; Use RI-EndpointServer)                 }^
{MaxLRQHops <mlrqh>-            (:between 1 and 8)                             }^
{LRQLdnOnly <lrqlo>-            (0:No;default)                                 }^
{                               (1:Yes; Only LDNs)                             }^
{EnableExtRouting <eer>-        (0:No;default)                                 }^
{                               (1:Yes; See RI-RoutingServer)                  }^
{GateKeeperID <gkid>-           (:An integer)                                  }^
{                                                                              }^
{LCFLRJV3Plus <lcflrjv3p>-      (:)                                            }^
{                                                                              }^
{EnableBEExtRegistrations <ebeer>-  (0:default, BE off)                        }^
{                                   (1:BE on)                                  }^
{UseIPHeader <uiph>-                (0:Disabled)                               }^
{                                   (1:Enabled)                                }^
{UseSecondaryBE <usbe>-             (0:Disabled)                               }^
{                                   (1:Enabled)                                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %GateKeeperParam <parameter><value>                                         ^
   where <parameter> is:                                                        ^
                                                                                ^
&RegistrationPort-                                                              ^
             (:RAS Port)                                                        ^
                                                                                ^
&GKListeningPort-                                                               ^
             (:GK Discovery Port)                                               ^
                                                                                ^
&PrimaryBEIPAddr-                                                               ^
             (:IP address)                                                      ^
                                                                                ^
&SecondaryBEIPAddr-                                                             ^
             (:IP address)                                                      ^
                                                                                ^
&ZoneName-                                                                      ^
             (:Up to 31 Chars)                                                  ^
                                                                                ^
&Password-                                                                      ^
             (:Alphanumeric string)                                             ^
                                                                                ^
&EPRadiusAuthorization-                                                         ^
             (0:No;default)                                                     ^
             (1:Yes)                                                            ^
                                                                                ^
&MaxLRQHops-                                                                    ^
             (:Hops)                                                            ^
                                                                                ^
&LRQLdnOnly-                                                                    ^
             (0:All routes; default)                                            ^
             (1:Yes; Only LDNs)                                                 ^
                                                                                ^
&EnableExtRouting-                                                              ^
             (0:No;default),                                                    ^
             (1:Yes)                                                            ^
                                                                                ^
&GateKeeperID-                                                                  ^
            (:Integer ID)                                                       ^
                                                                                ^
&LCFLRJV3Plus-                                                                  ^
             (1:default; Yes)                                                   ^
             (0:No)                                                             ^
                                                                                ^
&EnableBEExtRegistrations-                                                      ^
             (0:default; BE Off)                                                ^
             (1:BE On)                                                          ^
&UseIPHeader-                                                                   ^
             (0:Disabled)                                                       ^
             (1:Enabled)                                                        ^
&UseSecondaryBE-                                                                ^
             (0:Disabled)                                                       ^
             (1:Enabled)                                                        ^
                                                                                ^
@2700~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <epad>.                                                           }^
{    End point address directory incorporates two tables:                      }^
{    Allowed Endpoints - where you can set up specific IP and/or subnet masks  }^
{                        that are only allowed to make calls to this Tenor     }^
{    Barred Endpoints -  where you can set up specific IP and/or subnet masks  }^
{                        that are not allowed to make calls to Tenor.          }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <EndPointAddressDirectory>.                                         ^
     End point address directory incorporates two tables:                       ^
     Allowed Endpoints - where you can set up specific IP and/or subnet masks   ^
                         that are only allowed to make calls to this Tenor.     ^
     Barred Endpoints - where you can set up specific IP and/or subnet masks    ^
                        that are not allowed to make calls to Tenor.            ^
     If no IP/Mask addresses are set in both tables, then all IP addresses are  ^
     allowed to send VoIP calls to this unit.                                   ^
                                                                                ^
@2703~{------------------------------------------------------------------------}^
{Add, Change and Remove command can be used with both EndPoint tables, also the}^
{following commands are used to                                                }^
{set EndPointAddressDirectory.                                                 }^
{                                                                              }^
{AdmitType <at>-                (0:Barred), (1:Allowed).                       }^
{IPAddress <ipa>-               (:0.0.0.0-255.255.255.255)                     }^
{Mask <m>-                      (:255.255.255.xxx:xxx,0-255)                   }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add, Change and Remove command can be used with both EndPoint tables, also the  ^
following commands are used to:                                                 ^
                                                                                ^
Set %EndPointAddressDirectory <param> <value>:                                  ^
                                                                                ^
&AdmitType-                                                                     ^
             (0:Barred)                                                         ^
             (1:Allowed).                                                       ^
                                                                                ^
&IPAddress-                                                                     ^
             (:0.0.0.0-255.255.255.255)                                         ^
                                                                                ^
&Mask-                                                                          ^
             (:255.255.255.xxx;xxx,0-255)                                       ^
                                                                                ^
@2704~{------------------------------------------------------------------------}^
{Change               - a config command used to change table values by the    }^
{                       index                                                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                -a config command used to change table values by the      ^
                       index                                                    ^
                                                                                ^
     Example one shows how to change AdmitType in EndpointAddressDirectory 1.   ^
             Example 1: config-EndpointAddressDirectory-1# change 3 at 1        ^
                                                                                ^
           Allowed Endpoints                                                    ^
           Index IPAddress        Mask             AdmitType                    ^
           ----- ---------------- ---------------- ---------                    ^
           1     192.168.30.2     255.255.255.0    1<Allowed>                   ^
           2     192.168.30.3     255.255.255.0    1<Allowed>                   ^
                                                                                ^
           Barred Endpoints                                                     ^
           Index IPAddress        Mask             AdmitType                    ^
           ----- ---------------- ---------------- ---------                    ^
           3     192.168.30.210   255.255.255.0    0<Barred>                    ^
                                                                                ^
@2705~{------------------------------------------------------------------------}^
{Add                   -a config command used to add new IP/Mask               }^
{                       to Allowed/Barred Endpoints table                      }^
{                                                                              }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                    -a config command used to add new IP/Mask                ^
                        to Allowed/Barred Endpoints table                       ^
                                                                                ^
     Example one shows how to add a new IP address to a Barred Endpoints table. ^
             Example 1: config-EndpointAddressDirectory-1# add 192.168.30.10    ^
     Example two shows how to add a new IP address to Allowed Endpoints table.  ^
             Example 2: config-EndpointAddressDirectory-1# add 192.168.30.7 at 1^
                                                                                ^
           Allowed Endpoints                                                    ^
           Index IPAddress        Mask             AdmitType                    ^
           ----- ---------------- ---------------- ---------                    ^
           1     192.168.30.2     255.255.255.0    1<Allowed>                   ^
           2     192.168.30.3     255.255.255.0    1<Allowed>                   ^
           3     192.168.30.7     255.255.255.0    1<Allowed>                   ^
                                                                                ^
           Barred Endpoints                                                     ^
           Index IPAddress        Mask             AdmitType                    ^
           ----- ---------------- ---------------- ---------                    ^
           4     192.168.30.210   255.255.255.0    0<Barred>                    ^
           5     192.168.30.10    255.255.255.0    0<Barred>                    ^
                                                                                ^
@2706~{------------------------------------------------------------------------}^
{rem                   -a config command used to remove entry from the tables. }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                  -a config command used to remove entry from the tables. ^
                                                                                ^
     Example one shows how to remove IP/Mask from Allowed Endpoints table.      ^
             Example 1: config-EndpointAddressDirectory-1# rem 2                ^
                                                                                ^
           Allowed Endpoints                                                    ^
           Index IPAddress        Mask             AdmitType                    ^
           ----- ---------------- ---------------- ---------                    ^
           1     192.168.30.2     255.255.255.0    1                            ^
           2     192.168.30.7     255.255.255.0    1                            ^
                                                                                ^
           Barred Endpoints                                                     ^
           Index IPAddress        Mask             AdmitType                    ^
           ----- ---------------- ---------------- ---------                    ^
           3     192.168.30.210   255.255.255.0    0                            ^
           4     192.168.30.10    255.255.255.0    0                            ^
                                                                                ^
@2720~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <epa>.                                                            }^
{    End point addresses consists of two admit types:          :               }^
{    Allowed Endpoints - where you can set up specific IP and/or subnet masks  }^
{                        that are only allowed to make calls to this Tenor.    }^
{    Barred Endpoints -  where you can set up specific IP and/or subnet masks  }^
{                        that are not allowed to make calls to Tenor.          }^
{                                                                              }^
Current Level                                                                  }^
--------------------------------------------------------------------------------^
Level Name: <EndPointAddress>.                                                  ^
     End point addresses consist of two admit types:     :                      ^
     Allowed Endpoints - where you can set up specific IP and/or subnet masks   ^
                         that are only allowed to make calls to this Tenor.     ^
     Barred Endpoints - where you can set up specific IP and/or subnet masks    ^
                        that are not allowed to make calls to a Tenor.          ^
     If no IP/Mask addresses are set in both tables, then all IP addresses are  ^
     allowed to send VoIP calls to this unit.                                   ^
                                                                                ^
@2721~{------------------------------------------------------------------------}^
{Add, Change and Remove command can be used with both EndPoint tables, also the}^
{following commands are used to                                                }^
{set EndPointAddress         .                                                 }^
{                                                                              }^
{AdmitType <at>-                (0:Barred), (1:Allowed).                       }^
{IPAddress <ipa>-               (:0.0.0.0-255.255.255.255)                     }^
{Mask <m>-                      (:255.255.255.xxx;xxx,0-255)                   }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add, Change and Remove command can be used with both EndPoint tables, also the  ^
following commands are used to:                                                 ^
                                                                                ^
Set %EndPointAddress <param> <value>:                                           ^
                                                                                ^
&AdmitType-                                                                     ^
             (0:Barred)                                                         ^
             (1:Allowed).                                                       ^
                                                                                ^
&IPAddress-                                                                     ^
             (:0.0.0.0-255.255.255.255)                                         ^
                                                                                ^
&Mask-                                                                          ^
             (:255.255.255.xxx;xxx,0-255)                                       ^
                                                                                ^
                                                                                ^
@2800~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <ts>.                                                             }^
{    The TimeServerInfo is a PC that acquire the Universal Time from e.g., USNO}^
{    <US Navy Official Observatory> Master Clock and VoIP network and Tenor    }^
{    interface with the TimeServer by SNTP to sync the time between the UTC    }^
{    time <not GMT> with Tenor's internal clock.                               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <TimeServer>.                                                       ^
    The TimeServerInfo is a PC that acquire the Universal Time from e.g., USNO  ^
    <US Navy Official Observatory> Master Clock and our VoIP network and Tenor  ^
    interface with the TimeServer by SNTP to sync the time between the UTC time ^
    <not GMT> with a Tenor's internal clock.                                    ^
                                                                                ^
@2803~{------------------------------------------------------------------------}^
{Set ts <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{utco-     (-24\:00 to 24\:00:in +/-hrs from UTC time, default 0)              }^
{                                                                              }^
{psipa-    (:0.0.0.0-255.255.255.255)                                          }^
{                                                                              }^
{ssipa-    (:0.0.0.0-255.255.255.255)                                          }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %TimeServer <parameter><value>                                              ^
   where <parameter> is:                                                        ^
                                                                                ^
&UTCOffset-                                                                     ^
   (-24\:00 to 24\:00:in +/-hrs from UTC time,default 0)                        ^
                                                                                ^
&PrimaryServerIPAddr-                                                           ^
   (:0.0.0.0-255.255.255.255)                                                   ^
   (0.0.0.0:default)                                                            ^
                                                                                ^
&SecondaryServerIPAddr-                                                         ^
   (:0.0.0.0-255.255.255.255)                                                   ^
   (0.0.0.0:default)                                                            ^
                                                                                ^
@3000~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <qosp>.                                                           }^
{    A QOS Policy is associated with a Zone for the QOS parameters and service }^
{    level specification between end points. A QOS policy consists of an       }^
{    AutoSwitch profile that defines the thresholds for transparent autoswitch }^
{    quality services.                                                         }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <QOSPolicy>.                                                        ^
     A QOS Policy is associated with a Zone for the QOS parameters and service  ^
     level specification between end points. A QOS policy consists of an        ^
     AutoSwitch profile that defines the thresholds for transparent autoswitch  ^
     quality services.                                                          ^
                                                                                ^
@3003~{------------------------------------------------------------------------}^
{Set qosp <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{AutoSwitchThreshold <ast>-     (1-1000:Tenths % packet loss).                 }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %QOSPolicy <parameter><value>                                               ^
   where <parameter> is:                                                        ^
                                                                                ^
&AutoSwitchThreshold-                                                           ^
              (1-1000:Tenths % packet loss)                                     ^
                                                                                ^
@3100~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <rd>.                                                             }^
{    Route Directory is located under Domain. A route directory consists of a  }^
{    number of static routes.                                                  }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <RouteDirectory>.                                                   ^
     Route Directory is located under Domain. A route directory consists of a   ^
     number of static routes.                                                   ^
                                                                                ^
@3101~{------------------------------------------------------------------------}^
{new sr                         Create new Static Route named <id>             }^
{                                                                              }^
--------------------------------------------------------------------------------^
new StaticRoute                 Create new Static Route named <id>              ^
                                                                                ^
@3102~{------------------------------------------------------------------------}^
{delete sr                      Delete existing Static Route named <id>        }^
{                                                                              }^
--------------------------------------------------------------------------------^
delete StaticRoute              Delete existing Static Route named <id>         ^
                                                                                ^
@3200~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <sr>.                                                             }^
{    Static route is located under Route Directory. Used to build static       }^
{    routing tables between networks and other H.323 devices that are          }^
{    registered to this network through the Border Element such as Net Meeting }^
{    or Cisco Gateways.  Use Add, Change and Remove commands to configure the  }^
{    Alias Address.                                                            }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <StaticRoute>.                                                      ^
     Static route is located under Route Directory. Used to build static        ^
     routing tables between networks and other H.323 devices that are           ^
     registered to this network through the Border Element such as Net Meeting  ^
     or Cisco Gateways.  Use Add, Change and Remove commands to configure the   ^
     Alias Address.                                                             ^
                                                                                ^
@3203~{------------------------------------------------------------------------}^
{Set sr <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                      (:read only)                                    }^
{name <name>-                  (:name)                                         }^
{CallSignalIP <csip>-          (:IP of the destination static route unit)      }^
{                                                                              }^
{          AliasAddress Table                                                  }^
{          Index DN               Type    Priority                             }^
{          ----- ---------------- ----   -----------                           }^
{          1     73298*****       0<PUB>  0<Lowest>                            }^
{          2     847*******       1<PRIV> 3                                    }^
{          3     312768****       1<PRIV> 16                                   }^
{          4     708989****       0<PUB>  255<Highest>                         }^
{                                                                              }^
{Registered <r>-                (0:default for BE) (1: registered to GK)       }^
{GKMode <gkm>-                  (0:Gateway) (1:Gatekeeper)                     }^
{IPRoutingGroupAttached <iprga>- (:attached IPRG)                              }^
--------------------------------------------------------------------------------^
Set %StaticRoute <parameter><value>                                             ^
   where <parameter> is:                                                        ^
                                                                                ^
id <id>-                                                                        ^
               (:read only)                                                     ^
name <name>-                                                                    ^
               (:name)                                                          ^
&CallSignalIP-                                                                  ^
               (:IP of the destination static route unit)                       ^
                                                                                ^
&Registered-                                                                    ^
              (0:default for BE) (1: registered to GK)                          ^
                                                                                ^
&GKMode-                                                                        ^
              (0:Gateway) (1:Gatekeeper)                                        ^
                                                                                ^
&IPRoutingGroupAttached-                                                        ^
              (0:def; Regular SR) (1: proxy route)                              ^
                                                                                ^
@3204~{------------------------------------------------------------------------}^
{Change                        -a config command used to change settings in    }^
{                               AliasAddressTable table.                       }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change settings in     ^
                                AliasAddress Table .                            ^
                                                                                ^
     Example one shows how to change DN in a AliasAddress Table                 ^
             Example 1: config-StaticRoute-1# change 1 DN 312355                ^
     Example two shows how to change type of number in AliasAddress Table       ^
             Example 2: config-StaticRoute-1# change 1 t 1                      ^
                                                                                ^
           AliasAddress Table                                                   ^
           Index DN               Type   Priority                               ^
           ----- ---------------- ----   --------                               ^
           1     312355****       1<PRIV> 0<Lowest>                             ^
           2     847*******       1<PRIV> 3                                     ^
           3     312768****       1<PRIV> 16                                    ^
           4     708989****       0<PUB>  255<Highest>                          ^
                                                                                ^
@3205~{------------------------------------------------------------------------}^
{Add                           -a config command used to add a DN to           }^
{                               AliasAddress Table.                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                            -a config command used to add a DN to            ^
                                AliasAddress Table.                             ^
                                                                                ^
     Example one shows how to add DN in a AliasAddress Table                    ^
             Example 1: config-StaticRoute-1# add 847298* p 2                   ^
                                                                                ^
           AliasAddress Table                                                   ^
           Index DN               Type   Priority                               ^
           ----- ---------------- ----   -----------                            ^
           1     312355****       1<PRIV> 0<Lowest>                             ^
           2     847*******       1<PRIV> 3                                     ^
           3     312768****       1<PRIV> 16                                    ^
           4     708989****       0<PUB>  255<Highest>                          ^
           5     847298****       0<PUB>  2                                     ^
                                                                                ^
@3206~{------------------------------------------------------------------------}^
{rem                           -a config command used to remove a DN from      }^
{                                 AliasAddress Table                           }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                         -a config command used to remove a DN from       ^
                                the AliasAddress Table.                         ^
                                                                                ^
     Example 1 shows how to remove DN from the AliasAddress Table. Specify the  ^
             index of the entry to be removed.                                  ^
             Example 1: config-StaticRoute-1# remove 5                          ^
                                                                                ^
           AliasAddress Table                                                   ^
           Index DN               Type   Priority                               ^
           ----- ---------------- ----   --------                               ^
           1     312355****       1<PRIV> 0<Lowest>                             ^
           2     847*******       1<PRIV> 3                                     ^
           3     312768****       1<PRIV> 16                                    ^
           4     708989****       0<PUB>  255<Highest>                          ^
                                                                                ^
@3300~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{AliasAddress Table.                                                           }^
{    Alias Address Table is located under Static Route. Used to configure the  }^
{    address for static routing group table between network and other H.323    }^
{    devices that are registered to this network through the Border Element,   }^
{    such as NetMeeting or Cisco Gateways.                                     }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
AliasAddress Table:                                                             ^
     Alias Address Table is located under Static Route. Used to configure the   ^
     address for static routing group table between network and other H.323     ^
     devices that are registered to this network through the Border Element,    ^
     such as Net Meeting or Cisco Gateways.                                     ^
                                                                                ^
@3303~{------------------------------------------------------------------------}^
{Set AliasAddress                                                              }^
{Use Add, Change and Remove to modify the address values.                      }^
{                                                                              }^
{Index <Read Only>-             (:Index for AliasAddress).                     }^
{DN <dn>-                       (:Directory number)                            }^
{Type <t>-                                                                     }^
{Priority <p>-                  (:<0-255>. Higher number, higher priority.)    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %AliasAddress  <parameter><value>                                           ^
Use Add, Change and Remove to modify the table values.                          ^
   where <parameter> is:                                                        ^
                                                                                ^
&Index-                                                                         ^
             (:entity Id for AliasAddress) read only                            ^
                                                                                ^
&DN-                                                                            ^
             (:Directory number)                                                ^
&Type-                                                                          ^
             (0:PUB)                                                            ^
             (1:PRIV)                                                           ^
                                                                                ^
&Priority-                                                                      ^
             (:0-255,Higher number, higher priority)                            ^
                                                                                ^
@3400~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <usr>.                                                            }^
{    Users are classified into two groups:                                     }^
{    Administrators <admin> -                                                  }^
{                     who can use CLI to most of the system management         }^
{                     functionality except OEM only system parameters and      }^
{                     diagnostics functions.                                   }^
{                                                                              }^
{    User <usr> -     who can read the system parameters and diagnostics       }^
{                     functions.                                               }^
                                                                                ^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <User>.                                                             ^
     Users are classified into two groups:                                      ^
                                                                                ^
     Administrators - who can use CLI to most of the system management          ^
                      functionality except OEM only system parameters and       ^
                      diagnostics functions.                                    ^
                                                                                ^
     User -           who can read the system parameters and diagnostics        ^
                      functions.                                                ^
                                                                                ^
@3403~{------------------------------------------------------------------------}^
{Set usr <parameter><value>                                                    }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id-                                                                           }^
{            (:read only)                                                      }^
{name-                                                                         }^
{            (:name)                                                           }^
{ContactInfo <ci>-              (:contact information)                         }^
{Login <Read Only>-             (0:Admin), (1:User)                            }^
{LastLogin <Read Only>-         (:last user login time)                        }^
--------------------------------------------------------------------------------^
Set %User <parameter><value>                                                    ^
   where <parameter> is:                                                        ^
                                                                                ^
&id-                                                                            ^
             (:read only)                                                       ^
&name-                                                                          ^
             (:name)                                                            ^
                                                                                ^
&ContactInfo-                                                                   ^
             (:contact information)                                             ^
                                                                                ^
&Login-                                                                         ^
             (0:admin)                                                          ^
             (1:user)                                                           ^
                                                                                ^
&LastLogin-                                                                     ^
             (:last user login time)                                            ^
                                                                                ^
@3500~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <voipn>.                                                          }^
{    An enterprise VOIP network consists of an intranet that can expand over   }^
{    several sites and each site can have one PBX with a Gateway connected     }^
{    between the PBX and the Public Switched Telephone Network via a T1/E1 line}^
{    to a Central Office.                                                      }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <VOIPNetwork>.                                                      ^
     An enterprise VOIP network consists of an intranet that can expand over    ^
     several sites and each site can have one PBX with a Gateway connected      ^
     between the PBX and the Public Switched Telephone Network via a T1/E1 line ^
     to a Central Office.                                                       ^
@3503~{------------------------------------------------------------------------}^
{Set voipn <parameter>   <value>                                               }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                      (:read only)                                    }^
{name <name>-                  (:name)                                         }^
{AdminContact <ac>-            (:contact information)                          }^
--------------------------------------------------------------------------------^
Set %VOIPNetwork <parameter><value>                                             ^
   where <parameter> is:                                                        ^
                                                                                ^
&id <id>-                                                                       ^
              (:read only)                                                      ^
&name <name>-                                                                   ^
              (:name)                                                           ^
&AdminContact-                                                                  ^
              (:Admin contact information)                                      ^
                                                                                ^
@3600~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <sysls>.                                                          }^
{    Is used to configure up to 3 Syslog Servers to which the Tenor will send  }^
{    alarm events when they happen. You may also configure the syslog servers  }^
{    poll your Tenor for alarms on a scheduled basis if your syslog servers    }^
{    supports this.                                                            }^
{    The syslog server is a third party software and is not provided by Quintum}^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <SYSLogServer>.                                                     ^
     Is used to configure up to 3 Syslog Servers to which the Tenor will send   ^
     alarm events when they happen. You may also configure the syslog servers   ^
     poll your Tenor for alarms on a scheduled basis if your syslog servers     ^
     supports this.                                                             ^
     The syslog server is a third party software and is not provided by Quintum.^
                                                                                ^
@3603~{------------------------------------------------------------------------}^
{Set sysls <parameter><value>                                                  }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{id <id>-                       (:read only)                                   }^
{name <name>-                   (:name)                                        }^
{SysLogPort <slp>-              (:Syslog Server IP port)                       }^
{SysLogIP <slip>-               (:Syslog Server IP address)                    }^
{SysLogFacility <slf>-          (:Syslog Server facility code.)                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %SYSLogServer <parameter><value>                                            ^
   where <parameter> is:                                                        ^
                                                                                ^
&id <id>-                                                                       ^
              (:read only)                                                      ^
&name <name>-                                                                   ^
              (:name)                                                           ^
&SysLogPort-                                                                    ^
              (514:Syslog Server IP port, default)                              ^
                                                                                ^
&SysLogIP-                                                                      ^
              (:Syslog Server IP address)                                       ^
                                                                                ^
&SysLogFacility-                                                                ^
              (16:Syslog Server facility code, default)                         ^
                                                                                ^
@3700~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <cdrs>.                                                           }^
{    The Call Detail record Server is used to set up CDR collection server to  }^
{    collect the CDR records from the Tenor.                                   }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <CallDetailRecordServer>.                                           ^
      The Call Detail record Server is used to set up CDR collection server to  ^
      collect the CDR records from the Tenor. A Call Detail Record <CDR>,       ^
      provides call information such as origination number, destination number, ^
      call duration, etc. This information can be used to create billing reports^
      Most third party billing systems can be tailored to read this information.^
                                                                                ^
@3703~{------------------------------------------------------------------------}^
{Set cdrs <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{CDRFormat <cdrf>-              (0:default, standard CDR)                      }^
{                               (1:standard CDR plus other)                    }^
{                               (3:CMS CDR plus other)                         }^
{                               (4:CMS CDR plus other)                         }^
{                               (99:same as 4 plus other)                      }^
{                               (100:standard plus session id)                 }^
{                               (101:standard CDR plus other)                  }^
{                               (103:CMS CDR plus other)                       }^
{                               (104:CMS CDR plus other)                       }^
{                               (199:same as 99 plus other)                    }^
{CDRServerPort <cdrsp>-         (:9002 or 9003 (or 9004 or 9005 for CMS))      }^
{CDRServerIPAddr <cdrsipa>-     (:0.0.0.0-255.255.255.255)                     }^
{CDRPassword <cdrp>-            (:CDR password.)                               }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %CDRServer <parameter><value>                                               ^
   where <parameter> is:                                                        ^
                                                                                ^
&CDRFormat-                                                                     ^
             (0:default, standard CDR)                                          ^
             (1:standard CDR plus other)                                        ^
             (3:CMS CDR plus other)                                             ^
             (4:CMS CDR plus other)                                             ^
             (99:same as 4 plus other)                                          ^
             (100:standard plus session id)                                     ^
             (101:standard CDR plus other)                                      ^
             (103:CMS CDR plus other)                                           ^
             (104:CMS CDR plus other)                                           ^
             (199:same as 99 plus other)                                        ^
                                                                                ^
&CDRServerPort-                                                                 ^
             (9002:default)                                                     ^
                                                                                ^
&CDRServerIPAddr-                                                               ^
             (:0.0.0.0-255.255.255.255)                                         ^
             (0.0.0.0:default)                                                  ^
                                                                                ^
&CDRPassWord-                                                                   ^
             (:Alphanumeric String)                                             ^
                                                                                ^
@3800~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <ipdp>.                                                           }^
{    Configuration for IpDialPlan is located under the site. Used to configure }^
{    the incoming and outgoing calls for IP dial plan.                         }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <IPDialPlan>.                                                       ^
     Configuration for IpDialPlan is located under the site. Used to configure  ^
     the incoming and outgoing calls for IP dial plan.                          ^
                                                                                ^
@3803~{------------------------------------------------------------------------}^
{Set ipdp <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{INcomingDelDigits <indd>-      (:0-15,Incoming Del Digits)                    }^
{OUTgoingDelDigits <outdd>-     (:0-15,Outgoing Del Digits)                    }^
{INcomingPrefix <inp>-          (:Numeric string)                              }^
{OUTgoingPrefix <outp>-         (:Numeric string)                              }^
{OUTgoingTechPrefix <outtp>-    (:Numeric string)                              }^
{INcomingTechPrefix <intp>-     (:Numeric string)                              }^
{PrefixTrunkID <ptid>-          (:Numeric string)                              }^
--------------------------------------------------------------------------------^
Set %IPDialPlan <parameter><value>                                              ^
   where <parameter> is:                                                        ^
                                                                                ^
&INcomingDelDigits-                                                             ^
             (0:0-15: default)                                                  ^
                                                                                ^
&OUTgoingDelDigits-                                                             ^
             (0:0-15; default)                                                  ^
                                                                                ^
&INcomingPrefix-                                                                ^
             (:Numeric string)                                                  ^
                                                                                ^
&OUTgoingPrefix-                                                                ^
             (:Numeric string)                                                  ^
                                                                                ^
&OUTgoingTechPrefix-                                                            ^
             (:Numeric string)                                                  ^
                                                                                ^
&INcomingTechPrefix-                                                            ^
             (:Numeric string)                                                  ^
                                                                                ^
&PrefixTrunkID-                                                                 ^
             (0:Diabled;Default)  (1:Enabled)                                   ^
                                                                                ^
                                                                                ^
@3900~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <dp>.                                                             }^
{    Configuration for Dial plan is located under site. The dial plan defines  }^
{    how user shall dial at the site by a user or the system.                  }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <DialPlan>.                                                         ^
     Configuration for Dial plan is located under site. The dial plan defines   ^
     how user shall dial at the site by a user or the system.                   ^
                                                                                ^
@3903~{------------------------------------------------------------------------}^
{Set dp  <parameter><value>                                                    }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{10DigitlocalDial <10dd>-       (0:No; default), (1:Yes)                       }^
{MINDNlength <mindn>-           (1 to max DN length:MINDNlength)               }^
{MAXDNlength <maxdn>-           (:max DN length)                               }^
{LongDistancePrefix <ldp>-      (:Numeric string)                              }^
{CarrierPrefixPattern <cpp>-    (:101xxx;x, 0-9)                               }^
{                                                                              }^
{INTernationaLPrefix <intlp>-   (:numeric string)                              }^
{                                                                              }^
{IntercomEnable <ie>-           (0:No; default), (1:Yes)                       }^
{IPRoutePrefix <iprp>-          (:digit, 0-9,#)                                }^
{PSTNRoutePrefix <pstnrp>-      (:digit, 0-9,#)                                }^
{MultipathPrefix <mp>-          (:digit, 0-9,#)                                }^
{IntercomPrefix <ip>-           (:digit, 0-9,#)                                }^
{CentrexPrefix <cp>-            (:digit, 0-9,#)                                }^
{InterDigitTimeout <idt>-       (4:secs, default)                              }^
{UserProgramDialPlanEnabled <updpe>-                                           }^
{                               (0:disabled;default)                           }^
{                               (1:enabled)                                    }^
{ProgressToneCountry <ptc>-     (0:US)                                         }^
{                               (1:China)                                      }^
{                               (2:Taiwan)                                     }^
{                               (3:Japan)                                      }^
{                               (4:Poland)                                     }^
{                               (5:Yugoslavia)                                 }^
{                               (6:UK)                                         }^
{                               (7:Australia)                                  }^
{                               (8:Korea)                                      }^
{                               (9:South Africa)                               }^
{                               (10:Israel)                                    }^
{                               (11:Brazil)                                    }^
{                               (12:India)                                     }^
{                               (13:Czech/Slovak)                              }^
{CountryCode <cc>-              (:digits 1 to 7)                               }^
{AreaCode <ac>-                 (:area or city code)                           }^
{DialPlanCountry <dpc>-         (0:Generic CCITT)                              }^
{                               (1:US,NANPA,7digit)                            }^
{                               (2:US,NANPA,10digit)                           }^
{                               (3:China)                                      }^
{                               (4:Taiwan)                                     }^
{                               (5:UK)                                         }^
{                               (6:Australia)                                  }^
{                               (99:Custom,UPDP)                               }^
{                               (255:No dial plan)                             }^
{AllowUnmatchedNumbers<aun>-    (0:disable,default)                            }^
{                               (1:enable)                                     }^
--------------------------------------------------------------------------------^
Set %DialPlan <parameter><value>                                                ^
   where <parameter> is:                                                        ^
                                                                                ^
&10DigitlocalDial-                                                              ^
             (0:No; default)                                                    ^
             (1:Yes).                                                           ^
                                                                                ^
&MINDNlength-                                                                   ^
             (1 to max DN length:min DN length)                                 ^
                                                                                ^
&MAXDNlength-                                                                   ^
             (:max DN length)                                                   ^
                                                                                ^
&LongDistancePrefix-                                                            ^
             (1:default)                                                        ^
             (:Numeric string)                                                  ^
                                                                                ^
&CarrierPrefixPattern-                                                          ^
             (101xxxx:x is 0 to 9)                                              ^
             (:101xxxx;x is 0 to 9)                                             ^
                                                                                ^
&INTernationaLPrefix-                                                           ^
             (:Numeric string)                                                  ^
                                                                                ^
&IntercomEnable-                                                                ^
             (0:No; default)                                                    ^
             (1:Yes)                                                            ^
                                                                                ^
&IPRoutePrefix-                                                                 ^
             (:digit, 0-9,#)                                                    ^
                                                                                ^
&PSTNRoutePrefix-                                                               ^
             (:digit, 0-9,#)                                                    ^
                                                                                ^
&MultipathPrefix-                                                               ^
             (:digit, 0-9,#)                                                    ^
                                                                                ^
&IntercomPrefix-                                                                ^
             (:digit, 0-9,#)                                                    ^
                                                                                ^
&CentrexPrefix-                                                                 ^
             (:digit, 0-9,#)                                                    ^
                                                                                ^
&InterDigitTimeout-                                                             ^
             (:secs)                                                            ^
             (4:secs; default)                                                  ^
                                                                                ^
&UserProgramDialPlanEnabled-                                                    ^
             (0:disabled;default)                                               ^
             (1:enabled)                                                        ^
                                                                                ^
&ProgressToneCountry-                                                           ^
                                (0:US)                                          ^
                                (1:China)                                       ^
                                (2:Taiwan)                                      ^
                                (3:Japan)                                       ^
                                (4:Poland)                                      ^
                                (5:Yugoslavia)                                  ^
                                (6:UK)                                          ^
                                (7:Australia)                                   ^
                                (8:Korea)                                       ^
                                (9:South Africa)                                ^
                                (10:Israel)                                     ^
                                (11:Brazil)                                     ^
                                (12:India)                                      ^
                                (13:Czech/Slovak)                               ^
&CountryCode-                                                                   ^
              (:digits 1 to 7)                                                  ^
                                                                                ^
&AreaCode-                                                                      ^
              (:Numeric String)                                                 ^
                                                                                ^
&DialPlanCountry-               (0:Generic CCITT)                               ^
                                (1:US,NANPA,7digit)                             ^
                                (2:US,NANPA,10digit)                            ^
                                (3:China)                                       ^
                                (4:Taiwan)                                      ^
                                (5:UK)                                          ^
                                (6:Australia)                                   ^
                                (99:Custom,UPDP)                                ^
                                (255:No dial plan,default)                      ^
&AllowUnmatchedNumbers-         (0:disable,default)                             ^
                                (1:enable)                                      ^
 @4000~{Current Level                                                          }^
{------------------------------------------------------------------------------}^
{Level Name: <privnp>.                                                         }^
{    The Private Numbering Plan is used to enable the end of both Public and   }^
{    Private Dial Plan Numbers within one Tenor site. By default, the Tenor    }^
{    will use a public dial plan.                                              }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <PRIVateNumberingPlan>.                                             ^
     The Private Numbering Plan is used to enable the end of both Public and    ^
     Private Dial Plan Numbers within one Tenor site. By default, the Tenor     ^
     will use a public dial plan.                                               ^
@4003~{------------------------------------------------------------------------}^
{Set privnp <parameter><value>                                                 }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{PRIVateDNEnabled <privdne>-    (0:No; default), (1:Yes)                       }^
{PRIVateDNLength <privdnl>-     (:Only shown if PrivDNEnabled=1)               }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %PRIVateNumberingPlan <parameter><value>                                    ^
   where <parameter> is:                                                        ^
                                                                                ^
&PRIVateDNEnabled-                                                              ^
             (0:No; default)                                                    ^
             (1:Yes)                                                            ^
                                                                                ^
&PRIVateDNLength-                                                               ^
             (:1-32;if PrivDNEnabled=1)                                         ^
             (3:default length)                                                 ^
                                                                                ^
@4100~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <pubnp>.                                                          }^
{    The PublicNumberingPlan is used to define the Numbering Plan structure    }^
{    that will be set to when sending Public Dial Plan call out of this Site.  }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <PUBlicNumberingPlan>.                                              ^
     The PublicNumberingPlan is used to define the Numbering Plan structure     ^
     that will be set to when sending Public Dial Plan call out of this Site.   ^
                                                                                ^
@4103~{------------------------------------------------------------------------}^
{Set pubnp <parameter><value>                                                  }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %PUBlicNumberingPlan <parameter><value>                                     ^
   where <parameter> is:                                                        ^
                                                                                ^
                                                                                ^
@4200~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <fp>.                                                             }^
{    Fax profile is located under Gateway, which is used to configure the      }^
{    parameters for fax function.                                              }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <FaxProfile>.                                                       ^
     Fax profile is located under Gateway, which is used to configure the       ^
     parameters for fax function.                                               ^
                                                                                ^
@4203~{------------------------------------------------------------------------}^
{Set fp <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{FaxMaxRate <fmr>-              (24:2400 bps)      (48:4800 bps)               }^
{                               (72:7200 bps)      (96:9600 bps)               }^
{                               (120:12000 bps)    (144:14400 bps)             }^
{                                                                              }^
{FaxNominalDelay <fnd>-         (:ms,default 200 ms)                           }^
{                                                                              }^
{FaxInactivityTimeOut <fito>-   (:no activity timeout <in seconds> values are  }^
{                                 in the range of 10-32000 sec)                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %FaxProfile <parameter><value>                                              ^
   where <parameter> is:                                                        ^
                                                                                ^
&FaxMaxRate-                                                                    ^
              (24:2400 bps)      (48:4800 bps)                                  ^
              (72:7200 bps)      (96:9600 bps)                                  ^
              (120:12000 bps)    (144:14400 bps)                                ^
                                                                                ^
&FaxNominalDelay-                                                               ^
             (:ms,default 200ms)                                                ^
                                                                                ^
&FaxInactivityTimeOut-                                                          ^
              (:Secs; Range 10-32000)                                           ^
              (20:20 seconds)                                                   ^
                                                                                ^
@4300~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <iprg>.                                                           }^
{    IPRoutingGroup is located under Gateway, Which is used to configure the   }^
{    voice codec profile and voice activity, transmit and receive the gain for }^
{    voice signal.                                                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <IPRoutingGroup>.                                                   ^
     IPRoutingGroup is an located under Gateway, Which is used to configure the ^
     voice codec profile and voice activity, transmit and receive gain the voice^
     signal.                                                                    ^
                                                                                ^
@4303~{------------------------------------------------------------------------}^
{Set iprg <parameter><value>                                                   }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{VADEnable <vade>-              (0:Disable silence suppression)                }^
{                               (1:Enable silence suppression)                 }^
{IdleNoiseLevel <inl>-          (:Idle noise level x 0.01 dbm)                 }^
{                                                                              }^
{RxGain <rg>-                                                                  }^
{             (-14 - +14:db)                                                   }^
{                                                                              }^
{                                                                              }^
{TxGain <tg>-                                                                  }^
{             (-14 - +14:db)                                                   }^
{                                                                              }^
{                                                                              }^
{DigitRelayH323 <drh323>-      (0:in-band DTMF)                                }^
{                              (1:out-of-band H245 Alpha)                      }^
{                              (2:out-of-band H245 Signal)                     }^
{                              (3:out-of-band RFC 2833)                        }^
{                                                                              }^
{DigitRelaySIP- <drsip>-        (0:in-band tones)                              }^
{                               (3:out-of-band RFC 2833)                       }^
{                               (5:SIP INFO)                                   }^
{PacketSaverEnabled <pse>-      (0:Disable Packet saver)                       }^
{                               (1:Enable Packet saver).                       }^
{                                                                              }^
{MaxIncomingCallsAllowed <mica>-(:Limit the number of incoming calls)          }^
{                               (-1:Unlimted number of incoming calls allowed) }^
{                                                                              }^
{EnableExternalRouting <eer>-   (0:Disable)                                    }^
{                               (1:Enable, See ri-RoutingServer)               }^
{                                                                              }^
{MaxOutgoingCallsAllowed <moca>-(:Limit the number of outgoing calls)          }^
{                               (-1:Unlimted number of outgoing calls allowed) }^
{                                                                              }^
{MaxTalkTime <mtt>-             (:Mins)                                        }^
{CodecProfileAttached <cpa>-    (:Codec Profile ID)                            }^
{                                                                              }^
{IPDialPlanAttached <IPDPA>-    (:IPDialPlan ID)                               }^
{                                                                              }^
{InBoundAccessLevel <ibal>-                                                    }^
{                               (:Access level between 0 and 127)              }^
{                                                                              }^
{OutBoundAccessLevel <obal> -                                                  }^
{                               (:Access level between 0 and 127)              }^
{StopAcctID <said>-                                                            }^
{                               (0:IP Addr, default)                           }^
{                               (1:TrunkID of IC RG)                           }^
{                               (2:DNIS)                                       }^
{                               (3:Remote Signaling IP)                        }^
{                               (4:Term Signaling IP)                          }^
{                               (5:ANI)                                        }^
{ForceProgIEAlert <fpiea> -                                                    }^
{                               (0:No, default) (1:Yes)                        }^
{RelayANI <rani>-                                                              }^
{                               (0:No Relay ANI)                               }^
{                               (1:Relay ANI)                                  }^
{                               (2:Relay ANI with TON,NPI)                     }^
{DefaultANI <dani>-                                                            }^
{                               (:Calling Party Number)                        }^
{T303 <t303>-                   (:seconds; default 4)                          }^
{TCPConnectTime <tcpct>-        (:seconds; default 3)                          }^
{IVRType <ivrt>-                (0:Disabled)                                   }^
{                               (9:Provides single-stage pass-through)         }^
{                                authentication)                               }^
{IVRAuthType <ivrat>-           (0:ANI)                                        }^
{                               (1:IP Address)                                 }^
{                               (2:MAC Address)                                }^
{                               (3:H323 ID)                                    }^
{                               (4:MAC Address,ANI)                            }^
{                               (5:MAC,DN,PIN)                                 }^
{IgnoreTonNpi <itn>-            (0:Observe TON and NPI)                        }^
{                               (128:Ignore TON and NPI)                       }^
{                               (145:Treated as TON of International, NPI of   }^
{                               ISDN)                                          }^
{MediaQOSType <mqost>-          (0:TOS)                                        }^
{                               (1:Diffserv)                                   }^
{MediaQOSValue <mqosv>-         (:0x00-0xFE)                                   }^
{InbandTone <it>-               (0:no)                                         }^
{                               (1:yes; default)                               }^
{FaxRelay <fr>-                 (0:Disabled)                                   }^
{                               (1:T.38 w/o Fallback - Default)                }^
{                               (2:G.711 Mu-Law)                                }^
{                               (3:G.711-aLaw)                                 }^
{                               (4:T.38 with G.711-uLaw fallback)              }^
{                               (5:T.38 with G.711-aLaw fallback)              }^
{T38HSDataRedundancy <t38hsdr>- (0:default)                                    }^
{                               (:number of packets)                           }^
{T38LSDataRedundancy <t38lsdr>- (0:default)                                    }^
{                               (:number of packets)                           }^
{TCFHandlingMethod <tcfhm>-     (1:local)                                      }^
{                               (2:network)                                    }^
{ECM <ecm>-                     (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{AllowMRPageCompression <amrpc>-(0:disabled)                                   }^
{                               (1:enabled)                                    }^
{FaxModemCoding <fmc>-          (0:disabled;default)                           }^
{                               {8:G.711 A-Aaw)                                }^
{                               (9:G.711 Mu-Law)                               }^
{                               (10:ADPCM at 16kbps)                           }^
{                               (11:ADPCM at 24kbps)                           }^
{                               (12:ADPCM at 32kbps)                           }^
{                               (13:ADPCM at 40kbps)                           }^
{                               (100:Clear channel)                            }^
{DefaultANITON <daniton>-       (0:unknown,default)                            }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (3:Network Specific)                           }^
{                               (4:Subscriber)                                 }^
{                               (6:Abbreviated)                                }^
{DefaultANINPI <daninpi>-       (0:unknown,default)                            }^
{                               (1:ISDN/Telephony)                             }^
{                               (3:Data Numbering)                             }^
{                               (4:Telex Numbering)                            }^
{                               (8:National Standard Numbering)                }^
{                               (9:Private)                                    }^
{TCPOutboundConnectTimer <tcpoct>-  (:seconds,default 3)                       }^
{TCPInboundConnectTimer <tcpict>-  (:seconds,2-10)                             }^
{DisableFS <dfs>-               (0:FastStartEnabled,default)                   }^
{                               (1:FastStartDisabled)                          }^
{SIPDigitRelayPayloadType <sipdrpt>-                                           }^
{                               (:numeric,default 101)                         }^
{EnableSignalingOnly <eso>-     (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{DefaultANIScreenInd <danisi>-  (0:passthrough received)                       }^
{                               (1:user-provided)                              }^
{                               (2:user-provided,passed)                       }^
{                               (3:user-provided,failed)                       }^
{                               (4:network provided)                           }^
{RelayCallingNAMe <rcnam>-      (0:do not relay)                               }^
{                               (1:relay CNAM in INVITE)                       }^
{                               (3:relay default CNAM)                         }^
{DefaultCallingNAMe <dcnam>-    (:calling name,31 alphanum)                    }^
{DefaultANIPresentationInd <danipi>-   (0:relay ANI)                           }^
{                                      (1:No ANI,set CLIR)                     }^
{                                      (2:Always set CLIR and Relay ANI)       }^
{T310 <t310>-                          (:numeric,default 30)                   }^
{RejCallNoANi <rcnani>-		(0:Accept all calls)                           }^
{                               (1:Reject no/short ANI calls)                  }^
{CauseRejNoANI <crnani>-        (:cause value when rejecting no ANI calls)     }^
{MinimumANILength <manil>-      (:minimum acceptable value of ANI)             }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %IPRoutingGroup <parameter><value>                                          ^
   where <parameter> is:                                                        ^
                                                                                ^
&VADEnable-                                                                     ^
              (0:Disable silence suppression)                                   ^
              (1:Enable silence suppression)                                    ^
                                                                                ^
&IdleNoiseLevel-                                                                ^
              (:times 0.01 dbm)                                                 ^
                                                                                ^
&RxGain-                                                                        ^
               (-14 - +14:db)                                                   ^
                                                                                ^
&TxGain-                                                                        ^
               (-14 - +14:db)                                                   ^
                                                                                ^
&DigitRelayH323-                                                                ^
              (0:in-band DTMF)                                                  ^
              (1:out-of-band H245 Alpha)                                        ^
              (2:out-of-band H245 Signal)                                       ^
              (3:out-of-band RFC2833)                                           ^
                                                                                ^
&DigitRelaySIP-                                                                 ^
              (0:in-band tones)                                                 ^
              (3:out-of-band RFC2833)                                           ^
              (5:SIP INFO)                                                      ^
&PacketSaverEnabled-                                                            ^
              (0:Disable Packet saver)                                          ^
              (1:Enable Packet saver).                                          ^
                                                                                ^
&MaxIncomingCallsAllowed-                                                       ^
              (:InComing calls allowed)                                         ^
              (-1:UnLimited)                                                    ^
                                                                                ^
&EnableExternalRouting-                                                         ^
              (0:Default; Disabled)                                             ^
              (1:Enabled)                                                       ^
                                                                                ^
&MaxOutgoingCallsAllowed-                                                       ^
              (:OutGoing calls allowed)                                         ^
              (-1:UnLimited)                                                    ^
                                                                                ^
&MaxTalkTime-                                                                   ^
        (:Mins)                                                                 ^
                                                                                ^
                                                                                ^
&InBoundAccessLevel-                                                            ^
                                (:Access level, 0 to 127)                       ^
                                (:Access level between 0 and 127)               ^
                                                                                ^
&OutBoundAccessLevel-                                                           ^
                                (:Access level, 0 to 127)                       ^
                                                                                ^
&StopAcctID-                                                                    ^
            (0:IP Addr; Default)                                                ^
            (1:TrunkID of IC RG)                                                ^
            (2:DNIS)                                                            ^
            (3:Remote Signaling IP)                                             ^
            (4:Term Signaling IP)                                               ^
            (5:ANI)                                                             ^
                                                                                ^
&ForceProgIEAlert-                                                              ^
              (0:No;Default),                                                   ^
              (1:Yes)                                                           ^
                                                                                ^
&RelayANI-                                                                      ^
              (0:No Relay ANI)                                                  ^
              (1:Relay ANI)                                                     ^
              (2:Relay ANI with TON,NPI)                                        ^
                                                                                ^
&DefaultANI-                                                                    ^
             (:Calling party number for out bound calls)                        ^
                                                                                ^
&T303-                                                                          ^
             (:seconds; default 4)                                              ^
                                                                                ^
&TCPConnectTimer-                                                               ^
             (:seconds; default 3)                                              ^
                                                                                ^
&IVRType-                                                                       ^
             (0:Disabled)                                                       ^
             (9:Provides single-stage pass-through authentication)              ^
                                                                                ^
&IVRAuthType-                                                                   ^
             (0:ANI)                                                            ^
             (1:IP Address)                                                     ^
             (2:MAC Address)                                                    ^
             (3:H323 ID)                                                        ^
             (4:MAC Address,ANI)                                                ^
             (5:MAC,DN,PIN)                                                     ^
                                                                                ^
&IgnoreTonNpi-                                                                  ^
             (0:Observe TON and NPI)                                            ^
             (128:Ignore TON and NPI)                                           ^
             (145:Treated as TON of International, NPI of ISDN)                 ^
                                                                                ^
&MediaQOSType-                                                                  ^
             (0:TOS)                                                            ^
             (1:Diffserv)                                                       ^
                                                                                ^
&MediaQOSValue-                                                                 ^
             (:0x00-0xFE)                                                       ^
                                                                                ^
&InbandTone-                                                                    ^
             (0:no)                                                             ^
             (1:yes; default)                                                   ^
                                                                                ^
&CodecProfileAttached-                                                          ^
             (:Codec Profile ID)                                                ^
                                                                                ^
&IPDialPlanAttached-                                                            ^
             (:IP Dial Plan ID)                                                 ^
                                                                                ^
&FaxRelay-                                                                      ^
              (0:Disabled)                                                      ^
              (1:T.38 W/O Fallback - Default)                                   ^
              (2:G.711 Mu-Law)                                                  ^
              (3:G.711-aLaw)                                                    ^
              (4:T.38 with G.711-uLaw Fallback)                                 ^
              (5:T.38 with G.711-aLaw Fallback)                                 ^
                                                                                ^
&T38HSDataRedundancy-  (0:default)                                              ^
                       (:number of packets)                                     ^
                                                                                ^
&T38LSDataRedundancy-  (0:default)                                              ^
                       (:number of packets)                                     ^
                                                                                ^
&TCFHandlingMethod-    (1:local)                                                ^
                       (2:network)                                              ^
                                                                                ^
&ECM-                  (0:disabled)                                             ^
                       (1:enabled)                                              ^
                                                                                ^
&AllowMRPageCompression- (0:disabled)                                           ^
                         (1:enabled)                                            ^
                                                                                ^
&FaxModemCoding-                                                                ^
              (0:disabled;default)                                              ^
              (8:G.711 A-Aaw)                                                   ^
              (9:G.711 Mu-Law)                                                  ^
              (10:ADPCM at 16kbps)                                              ^
              (11:ADPCM at 24kbps)                                              ^
              (12:ADPCM at 32kbps)                                              ^
              (13:ADPCM at 40kbps)                                              ^
              (100:Clear channel)                                               ^
                                                                                ^
                                                                                ^
&DefaultANITON-                 (0:unknown,default)                             ^
                                (1:International)                               ^
                                (2:National)                                    ^
                                (3:Network Specific)                            ^
                                (4:Subscriber)                                  ^
                                (6:Abbreviated)                                 ^
                                                                                ^
&DefaultANINPI-                 (0:unknown,default)                             ^
                                (1:ISDN/Telephony)                              ^
                                (3:Data Numbering)                              ^
                                (4:Telex Numbering)                             ^
                                (8:National Standard Numbering)                 ^
                                (9:Private)                                     ^
                                                                                ^
&TCPOutboundConnectTimer-       (:seconds,default 3)                            ^
                                                                                ^
&TCPInboundConnectTimer-        (:seconds,2-10)                                 ^
                                                                                ^
&DisableFS-                     (0:FastStartEnabled,default)                    ^
                                (1:FastStartDisabled)                           ^
&SIPDigitRelayPayloadType-      (:numeric,default 101)                          ^
&EnableSignalingOnly-           (0:disabled)                                    ^
                                (1:enabled)                                     ^
&DefaultANIScreenInd-           (0:passthrough received)                        ^
                                (1:user-provided)                               ^
                                (2:user-provided,passed)                        ^
                                (3:user-provided,failed)                        ^
                                (4:network provided)                            ^
&RelayCallingNAMe-              (0:do not relay)                                ^
                                (1:relay CNAM in INVITE)                        ^
                                (3:relay default CNAM)                          ^
&DefaultCallingNAMe-            (:calling name,31 alphanum)                     ^
&DefaultANIPresentationInd-            (0:relay ANI)                            ^
                                       (1:No ANI,set CLIR)                      ^
                                       (2:Always set CLIR and Relay ANI)        ^
&T310-                                 (:numeric,default 30)                    ^
&RejCallNoANI-                                                                  ^
             (1:Yes) (0:No)                                                     ^
                                                                                ^
&CauseRejNoANI-                                                                 ^
             (:cause code value)                                                ^
                                                                                ^
&MinimumANILength-								^
             (:minimum acceptable value of ANI)	        	      		^						
										^
@4400~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <di>.                                                             }^
{    Digital Interface consists of either T1 or E1 WAN interface card. This    }^
{    card provides 8 T1 or E1 span line density to a single chassis slot. The  }^
{    individual span lines are switchable to provide either a trunk-side <PSTN>}^
{    or line-side <PBX> interface.                                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <DigitalInterface>.                                                 ^
     Digital Interface consists of either T1 or E1 WAN interface card. This     ^
     card provides 8 T1 or 8 E1 span line density to a single chassis slot. The ^
     individual span lines are switchable to provide either a trunk-side <PSTN> ^
     or line-side <PBX> interface.                                              ^
                                                                                ^
@4403~{------------------------------------------------------------------------}^
{Set di <parameter><value>                                                     }^
{    where <parameter> is:                                                     }^
{                                                                              }^
{Port Number <Read Only>-       (:read only)                                   }^
{LineType <Read Only>-          (0:T1), (1:E1)                                 }^
{DS0IdleCode <dsic>-            (127:0x7f), (255:0xff)                         }^
{Law <law>-                     (0:muLaw), (1:aLaw)                            }^
{                                                                              }^
{LineCode <lc>-                 (0:B8ZS, used for T1 only)                     }^
{                               (1:AMI, used for both T1 and E1)               }^
{                               (2:HDB3, used for E1 only)                     }^
{                                                                              }^
{CRC <crc>-                     E1(0:Disable CRC)                              }^
{                               E1(1:Enable CRC)                               }^
{                                                                              }^
{FramingFormat <ff>-            T1(0:D4)                                       }^
{                               T1(1:ESF)                                      }^
{                                                                              }^
{DS1orDSX <ds1dsx>-             (0:Short haul, DSX-default)                    }^
{                               (1:Long haul, DS1)                             }^
{                                                                              }^
{BuildOut <bo>-                 (0:0dBm)                                       }^
{                               (1:-7.5dBm)                                    }^
{                               (2:-15dBm)                                     }^
{                               (3:-22.5dBm)                                   }^
{                                                                              }^
{LENgth <len>-                  (0:0-133 ft)                                   }^
{                               (1:133-266 ft)                                 }^
{                               (2:266-399 ft)                                 }^
{                               (3:399-533 ft)                                 }^
{                               (4:533-655 ft)                                 }^
{                                                                              }^
{ChannelIndex <ci>-             1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,  }^
{                               19,20,21,22,23,24,25,26,27,28,29,30,31         }^
{                               (:channels)                                    }^
{Termination <t>-               (0:off)                                        }^
{                               (1:on,default)                                 }^
{StaticChannelConnection <scc>- (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %DigitalInterface <parameter><value>                                        ^
    where <parameter> is:                                                       ^
                                                                                ^
&PortNumber-   (:read only)                                                     ^
                                                                                ^
&LineType-                                                                      ^
              (0:T1)                                                            ^
              (1:E1)                                                            ^
                                                                                ^
&DS0IdleCode-                                                                   ^
              (127:0x7f),                                                       ^
              (255:0xff)                                                        ^
                                                                                ^
&Law-                                                                           ^
              (0:muLaw)                                                         ^
              (1:aLaw)                                                          ^
                                                                                ^
&LineCode-                                                                      ^
              (0:B8ZS, for T1 only)                                             ^
              (1:AMI,  both T1 and E1)                                          ^
              (2:HDB3, for E1 only)                                             ^
                                                                                ^
&CRC-                                                                           ^
              (0:Disable CRC)                                                   ^
              (1:Enable CRC)                                                    ^
                                                                                ^
&FramingFormat-                                                                 ^
             (0:D4)                                                             ^
             (1:ESF; default)                                                   ^
                                                                                ^
&DS1orDSX-                                                                      ^
              (0:DSX-ShortHaul; default)                                        ^
              (1:Long haul, DS1)                                                ^
                                                                                ^
&BuildOut-                                                                      ^
              (0:0dBm)                                                          ^
              (1:-7.5dBm)                                                       ^
              (2:-15dBm)                                                        ^
              (3:-22.5dBm)                                                      ^
                                                                                ^
&LENgth-                                                                        ^
              (0:0-133 ft)                                                      ^
              (1:133-266 ft)                                                    ^
              (2:266-399 ft)                                                    ^
              (3:399-533 ft)                                                    ^
              (4:533-655 ft)                                                    ^
                                                                                ^
&ChannelIndex-                                                                  ^
              (:channels)                                                       ^
                                                                                ^
&Termination-                                                                   ^
              (0:off)                                                           ^
              (1:on,default)                                                    ^
&StaticChannelConnection-       (0:disabled)                                    ^
                                (1:enabled)                                     ^
                                                                                ^
@4404~{------------------------------------------------------------------------}^
{map (or mapchannel)    - A config command at DigitalInterface/AnalogInterface }^
{                         level used for two purposes:                         }^
{                         1). Map channels into a ChannelGroup,                }^
{                         2). Set port mapping for the IP Extension feature.   }^
{                                                                              }^
--------------------------------------------------------------------------------^
map                     - A config command at DigitalInterface/AnalogInterface  ^
                          level used for two purposes:                          ^
                          1). Map channels into a ChannelGroup,                 ^
                          2). Set port mapping for the IP Extension feature.    ^
                                                                                ^
     Syntax for mapping channels into a ChannelGroup:                           ^
         map <channels> cg <id>                                                 ^
     where <channels> specify the channels to map,                              ^
           <id> is the ChannelGroup ID.                                         ^
                                                                                ^
     Example 1: map 3..6,12,15..20 cg myCG                                      ^
     Example 2: map +13..14 cg myCG                                             ^
     Example 3: map -12 cg myCG                                                 ^
                                                                                ^
     Example 1 shows how to map channels 3 to 6, 12 and 15 to 20 into CG-myCG.  ^
     Example 2 shows how to add channels 13 to 14 into CG-myCG.                 ^
     Example 3 shows how to remove channels 12 from CG-myCG.                    ^
                                                                                ^
                                                                                ^
     Syntax for setting port mapping:                                           ^
         map <channels> rip <ipAddr> rsl <slot> rsp <span> rch <chan> dnis <dn> ^
     where <channels> specify the channels to map,                              ^
           <ipAddr> is the IP address of the remote Tenor,                      ^
           <slot> is the slot number of the remote Tenor,                       ^
           <span> is the span number of the remote Tenor,                       ^
           <chan> is the channel number of the remote Tenor,                    ^
                                                                                ^
     Example 4: map 3..6 rip 192.168.1.1                                        ^
     Example 5: map 3 rch 22                                                    ^
     Example 6: map 4 rip                                                       ^
                                                                                ^
     Example 4 shows how to map channels 3 to 6 to a remote Tenor.              ^
     Example 5 shows how to map channel 3 to channel 22 of the remote Tenor.    ^
     Example 6 shows how to unmap channel 4 from the remote Tenor.              ^
                                                                                ^
                                                                                ^
     Note 1: You must go to a DigitalInterface/AnalogInterface to initiate this ^
             command, e.g., di SL2DV1DI1, or ai phone                           ^
     Note 2: In order to set port mapping, the IPExtension field of that        ^
             DigitalInterface/AnalogInterface must be set to 1.                 ^
                                                                                ^
@5000~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <RI>.                                                             }^
{    Is used to configure up to 2 Radius Servers IP addresses. You can also    }^
{    assign accounting port and authentication port to which the Tenor will    }^
{    send AAA Requests. Other configurable items include: retry count, timeout }^
{    interval, accounting type and shared secret                               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <RadiusInfo>.                                                       ^
     Is used to configure 3 Radius Servers IP address, accounting port,         ^
     and authentication port to which the Tenor will send AAA Requests.         ^
     retry count, timeout interval, accounting type and shared secret.          ^
     The three RIs are UserServer, EndpointServer and RoutingServer.            ^
                                                                                ^
     UserServer is mainly for calling card application/IVR                      ^
                                                                                ^
     EndpointServer is mainly for simple call authorization                     ^
     See also setting EPRadiusAuthorization in GateKeeperParam.                 ^
                                                                                ^
     RoutingServer is mainly for external routing. Make this settings when the  ^
     Tenor is used in conjunction with Quintum Routing Server.                  ^
                                                                                ^
@5003~{------------------------------------------------------------------------}^
{Set ri <parameter><value>                                                     }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{PrimaryAuthenticationPort <pap>- (:Auth. Port;1812, default)                  }^
{                                 (1812:default)                               }^
{PrimaryServerIPAddr <psipa>-     (:IP Address)                                }^
{PrimaryACcountingPort <pacp>-    (:Acco.Port;1813, default)                   }^
{                                 (:1813,default)                              }^
{SecondaryAuthenticationPort <sap>-                                            }^
{                                 (:Auth.Port,1812, default)                   }^
{                                 (1812:default)                               }^
{SecondaryServerIPAddr <psipa>-   (:IP Address)                                }^
{SecondaryACcountingPort <pacp>-  (:Acc.Port;1813, default)                    }^
{                                 (1813:default)                               }^
{RetryCount <rc>-                 (:Retry Count)                               }^
{Timeout <t>-                     (:Time Out in seconds)                       }^
{AccountingType <at>-             (0:no acct.msgs)                             }^
{                                 (1:1 stop per call)                          }^
{                                 (2:1 stop per leg)                           }^
{                                 (3:1 stop,1 start)                           }^
{                                 (4:1 stop,1 start per leg)                   }^
[                                 (5:1 stop per inc/out leg)                   }^
{SharedSecret <ss>-               (:Up to 63 Chars)                            }^
{IDType <idt>-                    (0:IP Address, default)                      }^
{                                 (1:H323 ID)                                  }^
{                                 (2:Serial Number)                            }^
{                                 (3:Trunk ID)                                 }^
{PasswordType <pt>                (0:IP Address, default)                      }^
{                                 (1:H323 ID)                                  }^
{                                 (2:Serial Number)                            }^
{                                 (3:Trunk ID)                                 }^
{GateWayID <gwid>-                (:an integer)                                }^
{BillingVendor <bv>-              (0:support Cisco;default)                    }^
{                                 (1:support SysMaster)                        }^
{                                 (2:support IVR Type 9)                       }^
{                                 (3:support PortaBilling)                     }^
{                                 (4:disable authenticator)                    }^
{UpdateAccountingInterval <uai>-  (:minutes,default 3)                         }^
{UpdateAccountingType <uat>-      (0:disabled,default)                         }^
{                                 (1:Outgoing Leg only)                        }^
{                                 (2:Incoming&Outgoing Leg)                    }^
{                                 (3:Outgoing Leg,disconnect)                  }^
{UseModifiedDN <umdn>-            (0:disable)                                  }^
{                                 (1:enable)                                   }^
{LocalRoutingFallback <lrf>-      (0:no response from RS)                      }^
{                                 (1:local RS if no response)                  }^
{                                 (2:local RS if no route)                     }^
{FailoverRetryInterval <fri>-     (0 - 5000:calls,default 0)                   }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %RadiusInfo <parameter><value>                                              ^
   where <parameter> is:                                                        ^
                                                                                ^
&PrimaryAuthenticationPort-                                                     ^
             (:Auth.Port;1812, default)                                         ^
             (1812:default)                                                     ^
                                                                                ^
&PrimaryServerIPAddr-                                                           ^
             (:IP Address)                                                      ^
                                                                                ^
&PrimaryACcountingPort-                                                         ^
             (:Acc. Port'1813, defaul)                                          ^
             (1813:default)                                                     ^
                                                                                ^
&SecondaryAuthenticationPort-                                                   ^
             (:Authen.port;1812,default)                                        ^
             (1812:default)                                                     ^
                                                                                ^
&SecondaryServerIPAddr-                                                         ^
             (:IP Address)                                                      ^
                                                                                ^
&SecondaryACcountingPort-                                                       ^
             (:Acco.Port;1813, default)                                         ^
             (1813:default)                                                     ^
                                                                                ^
&RetryCount-                                                                    ^
             (:Retry Count)                                                     ^
             (3:Retry Count,default)                                            ^
&Timeout-                                                                       ^
             (:Time Out in seconds)                                             ^
                                                                                ^
&AccountingType-                                                                ^
             (0:no acct.msgs)                                                   ^
             (1:1 stop per call)                                                ^
             (2:1 stop per leg)                                                 ^
             (3:1 stop,1 start)                                                 ^
             (4:1 stop,1 start per leg)                                         ^
             (5:1 stop per inc/out leg)                                         ^
                                                                                ^
&SharedSecret-                                                                  ^
             (:Up to 63 chars)                                                  ^
                                                                                ^
&IDType-                                                                        ^
             (0:IP Address, default)                                            ^
             (1:H323 ID)                                                        ^
             (2:Serial Number)                                                  ^
             (3:Trunk ID)                                                       ^
                                                                                ^
&PasswordType-                                                                  ^
             (0:IP Address, default)                                            ^
             (1:H323 ID)                                                        ^
             (2:Serial Number)                                                  ^
             (3:Trunk ID)                                                       ^
                                                                                ^
&GateWayID-                                                                     ^
             (:an integer)                                                      ^
                                                                                ^
&BillingVendor-                                                                 ^
             (0:support Cisco;default)                                          ^
             (1:support SysMaster)                                              ^
             (2:support IVR Type 9)                                             ^
             (3:support PortaBilling)                                           ^
             (4:disable authenticator)                                          ^
                                                                                ^
&UpdateAccountingInterval-        (:minutes,default 3)                          ^
&UpdateAccountingType-            (0:disabled,default)                          ^
                                  (1:Outgoing Leg only)                         ^
                                  (2:Incoming&Outgoing Leg)                     ^
                                  (3:Outgoing Leg,disconnect)                   ^
                                  (4:On Connect only)                           ^
&UseModifiedDN-                   (0:disable)                                   ^
                                  (1:enable)                                    ^
&LocalRoutingFallback-            (0:no response from RS)                       ^
                                  (1:fallback to local RS)                      ^
                                  (1:local RS if no response)                   ^
                                  (2:local RS if no route)                      ^
&FailoverRetryInterval-           (0 - 5000:calls,default 0)                    ^
@5100~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <fipd>.                                                           }^
{    FilterIPDir prompt acts as some sort of a firewall by creating an allow   }^
{    list of IP addresses and networks that are permitted to make ANY sort of  }^
{    communication with this Tenor e.g. Ping, Telnet, RADIUS Servers and       }^
{    SNMP Servers. The filter IP directory must have class C ONLY IP network   }^
{    addresses.                                                                }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <FilterIPDir>.                                                      ^
     FilterIPDir prompt acts as some sort of a firewall by creating an allow    ^
     list of IP addresses and networks that are permitted to make ANY sort of   ^
     communication with this Tenor e.g. Ping, Telnet, RADIUS Servers,and SNMP   ^
     Servers. The filter IP directory must have class C ONLY IP network         ^
     addresses.                                                                 ^
                                                                                ^
@5104~{------------------------------------------------------------------------}^
{Change                        -a config command used to change settings in    }^
{                               FilterIPTable                                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change settings in     ^
                                FilterIPTable.                                  ^
                                                                                ^
     Example one shows how to change a destination in the FilterIP Table        ^
             Example 1: config-FilterIPDir-1# change 2 d 213.123.43.121         ^
                                                                                ^
@5105~{------------------------------------------------------------------------}^
{Add                           -a config command used to add an ip address to  }^
{                               FilterIPTable.                                 }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                            -a config command used to add a IP endpoint to   ^
                                FilterIP Table.                                 ^
                                                                                ^
     Example one shows how to add an IP endpoint to FilterIP Table              ^
          Example 1: config-FilterIPDir-1# add 121.122.122.131 nm 255.255.255.0 ^
                                                                                ^
@5106~{------------------------------------------------------------------------}^
{rem                           -a config command used to remove a IP endpoint  }^
{                               from FilterIP Table.                           }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                         -a config command used to remove a IP endpoint to^
                                FilterIP Table.                                 ^
                                                                                ^
@5200~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <ai>.                                                             }^
{    Analog Interface consists of two interfaces: phone (PBX) or line          }^
{    (PSTN). The phone interface is associated with an LCRG, and the line      }^
{    interface is associated with a TCRG.                                      }^
{                                                                              }^
Current Level                                                                  }^
--------------------------------------------------------------------------------^
Level Name: <Analog Interface>.                                                 ^
     Analog Interface consists of two interfaces: phone <PBX> or line           ^
     <PSTN>. The phone interface is associated with an LCRG, and the line       ^
     interface is associated with a TCRG.                                       ^
                                                                                ^
@5203~{------------------------------------------------------------------------}^
{Set ai <parameter><value>                                                     }^
{    where <parameter> is:                                                     }^
{                                                                              }^
{name (name)-                   (:up to 32 Chars)                              }^
{                                                                              }^
{Type <type>-                   (0:phone)                                      }^
{                               (1:line)                                       }^
{                                                                              }^
{PortNumber <pn>-               (:read only; defines port number)              }^
{                                                                              }^
{Channels <channels>-           (:Available Channels)                          }^
{                                                                              }^
{IPExtension <ipe>-             (0:Disabled; default)                          }^
{                               (1:Enabled)                                    }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %AnalogInterface <parameter><value>                                         ^
    where <parameter> is:                                                       ^
                                                                                ^
&name-                                                                          ^
              (:Up to 32 Chars)                                                 ^
                                                                                ^
&Type-                                                                          ^
              (0:phone)                                                         ^
              (1:line)                                                          ^
&PortNumber-                                                                    ^
              (:read only; defines port number),                                ^
                                                                                ^
&Channels-                                                                      ^
              (:Available Channels)                                             ^
                                                                                ^
&IPExtension-                                                                   ^
              (0:Disabled; default),                                            ^
              (1:Enabled)                                                       ^
                                                                                ^
@5300~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <updp>.                                                           }^
{  User Programmable Dial Plan.Enables you to customize the way                }^
{  the Tenor interprets the sequences of digits you enter.                     }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <UserProgramDialPlan>                                               ^
    User Programmable Dial Plan.Enables you to customize the way                ^
    the Tenor interprets the sequences of digits you enter.                     ^
                                                                                ^
@5303~{------------------------------------------------------------------------}^
{Add                           -a config command used to add a pattern to the  }^
{                               UserProgramDialPlanENtry Table.                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                            -a config command used to add a pattern to       ^
                                UserProgramDialPlanENtry Table.                 ^
                                                                                ^
     The table below includes various patterns, types and dial strings used in  ^
     the UserProgramDialPlanENtry Table. For example, in Index 1, to add a      ^
     national pattern with a 10 digit dial string, enter                        ^
     config-UPDP-1# add 7 t 2 mind 10 maxd 10. In the table, the dashes should  ^
     be replaced with tilde marks.                                              ^
                                                                                ^
            UserProgramDialPlanENtry Table                                      ^
              index Pattern                  Type MINDigit MAXDigit PrefixLen   ^
              ----- ------------------------ ---- -------- -------- ---------   ^
              1     7                        2    10       10       255         ^
              2     2-9                      4     7        7       255         ^
              3     12-9                     2    11       11       255         ^
              4     0112-9                   1    10       18       3           ^
              5     2-911                    5     0        0       255         ^
@5304~{------------------------------------------------------------------------}^
{Change                        -a config command used to change settings in    }^
{                               UserProgramDialPlanENtry Table.                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change settings in     ^
                                UserProgramDialPlanENtry Table.                 ^
                                                                                ^
     Example one shows how to change the type of Index 1 to type 4 in the       ^
     UserProgramDialPlanENtry Table.                                            ^
             Example 1: config-UPDP-1# change 1 t 4                             ^
     Example two shows how to change minimun and maximum digits of Index 2 to   ^
     11 in the UserProgramDialPlanENtry Table                                   ^
             Example 2: config-UPDP-1# change 2 mind 10 maxd 10                 ^
                                                                                ^
           UserProgramDialPlanENtry Table                                       ^
             index Pattern                  Type MINDigit MAXDigit PrefixLen    ^
             ----- ------------------------ ---- -------- -------- ---------    ^
              1     7                        4    10       10        255        ^
              2     2-9                      2    10       10        255        ^
                                                                                ^
@5400~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <updpen>.                                                         }^
{  User Programmable Dial Plan Entry Table. Available under                    }^
{  the UserProgramDialPlan prompt. Enables you to customize the way the Tenor  }^
{  interprets the sequences of digits you enter.                               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <UserProgramDialPlanENtry Table>                                    ^
    User Programmable Dial Plan Entry Table. Available under                    ^
    the UserProgramDialPlan prompt. Enables you to customize the way            ^
    the Tenor interprets the sequences of digits you enter.                     ^
                                                                                ^
@5305~{------------------------------------------------------------------------}^
{Set UserProgramDialPlanENtry Table                                            }^
{Use Add, Change and Remove to modify the UserProgramDialPlanENtry Table       }^
{values.                                                                       }^
{                                                                              }^
{Type <type>-                   (0:None)                                       }^
{                               (1:International)                              }^
{                               (2:National)                                   }^
{                               (3:Carrier Selection)                          }^
{                               (4:Local)                                      }^
{                               (5:Special Service)                            }^
{                               (6:Supplementary Code 1)                       }^
{                               (7:Private)                                    }^
{                               (8: Supplementary Code 2)                      }^
{				(14:Local Prefix)			       }^
{				(90:Support second dialtone)                   }^
{				(100:Allow AddPrefix for non-Nortel            }^
{				(101-120:Support Nortel nummber types)         }^
{Pattern <p>-                   (:0-9,*,# or tilde for special ranging)        }^
{MINDigit<mind>                 (0 to 32:Minimum Digits)                       }^
{MAXDigit <maxd>                (0 to 32:Maximum Digits)                       }^
{PrefixLen <pl>                 (:pattern length)                              }^
{AddPrefix <ap>			(:add prefix for Nortel compatibility) 	       }^
--------------------------------------------------------------------------------^
Set %UserProgramDialPlanENtry <parameter><value>                                ^
Use Add, Change and Remove to modify the table values.                          ^
   where <parameter> is:                                                        ^
                                                                                ^
&Type-                                                                          ^
                 (0:None;default)                                               ^
                 (1:International)                                              ^
                 (2:National)                                                   ^
                 (3:Carrier Selection)                                          ^
                 (4:Local)                                                      ^
                 (5:Special Service)                                            ^
                 (6:Supplementary Code 1)                                       ^
                 (7:Private)                                                    ^
		 (8:Supplementary Code 2)                                       ^
		 (14:Local Prefix)						^
		 (90:Support second dialtone)					^
		 (100:Allow AddPrefix for non-Nortel)				^
		 (101-120:Support Nortel number types				^
&Pattern-                                                                       ^
                 (:0-9,*,# or tilde)                                            ^
&MINDigit-                                                                      ^
                 (0 to 32:Minimum Digits)                                       ^
&MAXDigit-                                                                      ^
                 (0 to 32:Maximum Digits)                                       ^
&PrefixLen-                                                                     ^
                 (:pattern length)                                              ^
                                                                                ^
&AddPrefix-	 (:add prefix for Nortel compatibility)				^
									       }^
@5500~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <natipd>.                                                         }^
{    NATIPDir prompt contains essential parameters that pertain to Quintum's   }^
{    NATAccess technology, which allows the Tenor units to route VoIP calls    }^
{    through a NAT server. The addresses configured here will contain the      }^
{    Private <Internal> IP addresses <and Subnet Masks>  of other Tenor        }^
{    units that reside on the same side of the NAT server as this Tenor.       }^
{                                                                              }^
{                                                                              }^
{    Configurable fields:                                                      }^
{                                                                              }^
{    Destination <d> Destination IP address.                                   }^
{    Subnet Mask <nm> Subnet Mask address used to differentiate the network    }^
{    portion of the IP address from the host portion of the IP address.        }^
{                                                                              }^
Current Level                                                                  }^
--------------------------------------------------------------------------------^
Level Name: <NATIPDir>.                                                         ^
     NATIPDir prompt contains essential parameters that pertain to Quintum's    ^
     NATAccess technology, which allows the Tenor units to route VoIP calls     ^
     through a NAT server. The addresses configured here will contain the       ^
     private <Internal> IP addresses <and Subnet Masks> of other Tenor          ^
     units that reside on the same side of the NAT server as this Tenor.        ^
                                                                                ^
     Configurable fields:                                                       ^
     Destination <d> Destination IP address.                                    ^
     Subnet Mask <nm> Subnet Mask address used to differentiate the network     ^
     portion of the IP address from the host portion of the IP address.         ^
                                                                                ^
@5504~{------------------------------------------------------------------------}^
{Change                        -a config command used to change settings in    }^
{                               NATIPDir table.                                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change settings in     ^
                                NATIPDir table.                                 ^
                                                                                ^
     Example one shows how to change a Destination in the NATIPDir table        ^
             Example 1: config-NATIPDir-1# change 1 d 192.168.1.3               ^
                                                                                ^
     Example two shows how to change a NetMask in the NATIPDir table            ^
             Example 2: config-NATIPDir-1# change 1 nm 255.255.255.0            ^
                                                                                ^
@5505~{------------------------------------------------------------------------}^
{Add                           -a config command used to add a Destination to  }^
{                               the NATIPDir table.                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                            -a config command used to add a Destination to   ^
                                the NATIPDir Table.                             ^
                                                                                ^
     Example one shows how to add a Destination to the NATIPDir table           ^
             Example 1: config-NATIPDir-1# add 192.168.55.3                     ^
                                                                                ^
@5506~{------------------------------------------------------------------------}^
{rem                           -a config command used to remove an entry from  }^
{                               the NATIIPDir table                            }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                         -a config command used to remove an entry from   ^
                                the NATIPDir table.                             ^
                                                                                ^
     Example one shows how to remove an entry from the NATIPDir table           ^
             Example 1: config-NATIPDir-1# rem 1 <index number>                 ^
                                                                                ^
@5600~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <siprd>.                                                          }^
{    StaticIPRouteDir contains essential parameters that pertain to Ethernet   }^
{    Interfaces.                                                               }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <StaticIProuteDir>.                                                 ^
     StaticIPRouteDir contains essential parameters that pertain to Ethernet    ^
     Interfaces.                                                                ^
     Configurable fields:                                                       ^
                                                                                ^
     Destination <d> Destination IP address.                                    ^
                                                                                ^
     NetMask <nm> Netmask IP address. Indicates how many bits of the            ^
     destination IP are significant in routing.                                 ^
                                                                                ^
     Gateway <g>. Gateway IP address. used by the Tenor to forward packets to   ^
     another network, subnet or device.                                         ^
                                                                                ^
     EIAttached <eia>. The slot/device and ethernet port to which this route    ^
     information applies.                                                       ^
                                                                                ^
     Metric <m>. The hop-count <in the range of 1 to 16> to the <endpoint>      ^
     host whose IP address is configured.                                       ^
                                                                                ^
@5604~{------------------------------------------------------------------------}^
{Change                        -a config command used to change settings in    }^
{                               StaticIPRouteDir table.                        }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                         -a config command used to change settings in     ^
                                StaticIPRouteDir table.                         ^
                                                                                ^
     Example one shows how to change a Destination in the SIPRD table           ^
             Example 1: config-StaticIPRouteDir-1# change 1 d 0.0.0.0           ^
                                                                                ^
     Example two shows how to change a NetMask in the SIPRD table               ^
             Example 2: config-StaticIPRouteDir-1# change 1 nm 0.0.0.0          ^
                                                                                ^
     Example three shows how to change a Gateway in the SIPRD table             ^
             Example 3: config-StaticIPRouteDir-1# change 1 g 192.168.2.1       ^
                                                                                ^
     Example four shows how to change a EIAttached in the SIPRD table           ^
             Example 4: config-StaticIPRouteDir-1# change 1 eia EI-SL1V1ET1     ^
                                                                                ^
     Example five shows how to change a Metric example in the SIPRD table       ^
             Example 3: config-StaticIPRouteDir-1# change 1 m 0                 ^
                                                                                ^
@5605~{------------------------------------------------------------------------}^
{Add                           -a config command used to add a new entry to    }^
{                               the SIPRD table.                               }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add                            -a config command used to add a new entry to     ^
                                the SIPRD table.                                ^
                                                                                ^
     Example one shows how to add a Destination to the SIPRD table              ^
             Example 1: config-SIPRD-1# add 0.0.0.0                             ^
                                                                                ^
@5606~{------------------------------------------------------------------------}^
{rem                           -a config command used to remove an entry from  }^
{                               the SIDPRD table                               }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                         -a config command used to remove an entry from   ^
                                the SIPRD table.                                ^
                                                                                ^
     Example one shows how to remove an entry from the SIDPRD table             ^
             Example 1: config-SIDPRD-1# rem 1 <index number>                   ^
                                                                                ^
@5700~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <sipsg>.                                                          }^
{    IPRoutingGroup is located under Gateway, Which is used to configure the   }^
{    voice codec profile and voice activity, transmit and receive the gain for }^
{    voice signal.                                                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <sipsg>.                                                            ^
     IPRoutingGroup is an located under Gateway, Which is used to configure the ^
     voice codec profile and voice activity, transmit and receive gain the voice^
     signal.                                                                    ^
                                                                                ^
@5704~{------------------------------------------------------------------------}^
{Set sipsg <parameter><value>                                                  }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{SIPListenPort <siplp>-        (:port number,def 5060)                         }^
{                                                                              }^
{PrimarySIPServerPort <psipsp>-       (:portnumber,def 5060)                   }^
{                                                                              }^
{PrimarySIPServer <psips>-                                                     }^
{                              (:IP address)                                   }^
{SecondarySIPServer <ssips>-                                                   }^
{                              (:IP address)                                   }^
{OBPrimaryUseLocalSurvivableGW <obpulsgw>-  (0:disabled)                       }^
{                                           (1:enabled)                        }^
{OB2ndaryUseLocalSurvivableGW  <ob2ulsgw>-  (0:disabled)                       }^
{                                           (1:enabled)                        }^
{SecondarySIPServerPort <ssipsp>-                                              }^
{                              (:port number,def 5060)                         }^
{OutboundPrimaryServerPort <opsp>-   (:port number,def 5060)                   }^
{OutboundPrimaryServer <ops>-   (:IP address)                                  }^
{OutboundSecondaryServerPort <ossp>-   (:port number,def 5060)                 }^
{OutboundSecondaryServer <oss>-   (:IP address)                                }^
{RegisterExpiryTime <ret>-          (:seconds,def 300)                         }^
{                                   (0:seconds,def 300)                        }^
{UserNameInContact <unic>-          (0:default,contact info not sent)          }^
{                                   (1:contact info sent)                      }^
{Contacts <c>-                      (:contact,alphanumeric, 1-4)               }^
{SDPin180Ringing <sdp180r>-         (0:disabled)                               }^
{                                   (1:send SDP)                               }^
{OutboundPrimaryProxyIPAddresses   <oppipa>- (:IP address,default 0.0.0.0)     }^
{OutboundSecondaryProxyIPAddresses <ospipa>- (:IP address,default 0.0.0.0)     }^
{OutboundPrimaryProxyPort <oppp>- (:IP address,default 0.0.0.0)                }^
{OutboundSecondaryProxyPort <ospp>- (:IP address,default 0.0.0)                }^
{SIPServerInFromHdr <sipsifh>-      (0:use Tenor IP)                           }^
{                                   (1:use SIP Server IP)                      }^
{MaxForwards <mf>-         (+1 - +255:default 70)                              }^
{IncludeQuintumHeader <iqh>-  (0:disable)                                      }^
{                             (1:enable,default)                               }^
{UserNameAsURI <unauri>-      (0:disable,default)                              }^
{                             (1:enable)                                       }^
{RequestReTransmitCount <rrtc>- (+3 - +18:default 11)                          }^
{SDPin183Progress <sdp183p>-    (0:no)                                         }^
{                               (1:yes,default)                                }^
{AllowOnlyProxyCalls <aopc>-    (0:all calls)                                  }^
{                               (1:from proxy,default)                         }^
{Send180Ringing <s180r>-        (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{Send183Progress <s183p>-       (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{SipPstnInterworking <spi>-     (0:disabled)                                   }^
{                               (1:enabled)                                    }^
{ForceAlertOn183 <fao183>-	(0:disabled)				       }^
{				(1:enabled)				       }^
{PRACKMethod <prackm>-          (0:disabled)                                   }^
{                               (1:supported)                                  }^
{                               (2:required)                                   }^
{SessionTimer <st>-             (0:disabled)                                   }^
{                               (1:supported)                                  }^
{                               (2:required)                                   }^
{SessionTimerMinSE <stmse>-     (300-65535:seconds,def 600)                    }^
{SessionTimerExpires <ste>-      (300 - 65535:seconds,def 3600)                }^
{MWIServer <mwis>-               (:IP address)                                 }^
{MWIServerPort <mwisp>-          (:Numeric,default 5060)                       }^
{MWISubscribeDuration <mwisd>-   (0 - 65535:minutes,def 60)                    }^
{MWIFailureRetryDelay <mwifrd>-  (0 - 65535:minutes,def 30)                    }^
{UserAgentHeader <uah>-          (:0-31 char,def Quintum1.0.0)                 }^
{SIPNoConnectTimeout <sipnct>-   (32 - 3600:seconds,def 180)                   }^
{ProxyFailoverBehavior <pfb>-    (0:no fail over)                              }^
{                                (1:fail over)                                 }^
{SIPInfoFormat <sipif>-          (0:Nortel,default)                            }^
{                                (1:Cisco)                                     }^
{CLIHeaderType <cliht>-          (0:disabled)                                  }^
{                                (1:Send Remote-Party-Id)                      }^
{                                (2:Q.1912.5 as TEL URI)                       }^
{                                (3:Q.1912.5 as SIP URI)                       }^
{                                (4:Ppreferred tel URI)                        }^
{                                (5:Ppreferred sip URI)                        }^
{UseFromContact <ufc>            (0:DN)                                        }^
(                                (1:Alias Name)                                }^
{RPIDDefaultPrivacy <rpiddp>-    (0:disabled)                                  }^
{                                (1:off)                                       }^
{                                (2:URI)                                       }^
{                                (3:Name)                                      }^
{                                (4:Full)                                      }^
{UseFromContact <ufc>-		 (0:Use DN)				       }^
				 (1:Use Alias Name)			       }^
{SIPTelephoneEvents <siptc>-	 (0:Don't append "/1" to SDP attribute)	       }^
				 (1:Append "/1" to SDP attribute)	       }^
{SIPUseDNinRegister <sipudnr>-	 (0:Use PrimaryUser in Register)	       }^
				 (1:Use DN from channel map in Register)       }^
{ConferenceFactoryName <cfn>-    (:0-31 charac,name)                           }^
{ConferenceFactoryPort <cfp>-    (:port number,def 5060)                       }^
{ConferenceFactoryServer <cfs>-  (:server name)                                }^
{DirectGWRouting <dgwr>-         (0:disable)                                   }^
{                                (1:enable)                                    }^
{GKBusyOut <gkbo>-               (0:disable)                                   }^
{                                (1:enable)                                    }^
{SIPRegisterOnBootup <siprob>-   (0:disable)                                   }^
{                                (1:enable)                                    }^
{SDPinInvite <sdpi>-             (0:disabled)                                  }^
{                                (1:send SDP)                                  }^
--------------------------------------------------------------------------------^
Set %SIPSignalingGroup <parameter><value>                                       ^
   where <parameter> is:                                                        ^
                                                                                ^
&SIPListenPort-                                                                 ^
              (:port number,def 5060)                                           ^
                                                                                ^
&PrimarySIPServerPort-       (:portnumber,def 5060)                             ^
                                                                                ^
&PrimarySIPServer-                                                              ^
                             (:IP address)                                      ^
&SecondarySIPServer-                                                            ^
                              (:IP address)                                     ^
&SecondarySIPServerPort-                                                        ^
                              (:port number,def 5060)                           ^
&OBPrimaryUseLocalSurvivableGW-  (0:disabled)                                   ^
                                 (1:enabled)                                    ^
&OB2ndaryUseLocalSurvivableGW-   (0:disabled)                                   ^
                                 (1:enabled)                                    ^
&OutboundPrimaryServerPort-   (:port number,def 5060)                           ^
&OutboundPrimaryServer-       (:IP address)                                     ^
&OutboundSecondaryServerPort-   (:port number,def 5060)                         ^
&OutboundSecondaryServer-     (:IP address)                                     ^
&RegisterExpiryTime-                (:seconds,def 300)                          ^
                                    (0:seconds,def 300)                         ^
&UserNameInContact-                 (0:default,contact info not sent)           ^
                                    (1:contact info sent)                       ^
&Contacts-                          (:contact,alphanumeric, 1-4)                ^
&SDPin180Ringing-                   (0:disabled)                                ^
                                    (1:send SDP)                                ^
&OutboundPrimaryProxyIPAddresses-  (:IP address,default 0.0.0.0)                ^
&OutboundSecondaryProxyIPAddresses- (:IP address,default 0.0.0.0)               ^
&OutboundPrimaryProxyPort-  (:IP address,default 0.0.0.0)                       ^
&OutboundSecondaryProxyPort- (:IP address,default 0.0.0)                        ^
&SIPServerInFromHdr-                (0:use Tenor IP)                            ^
                                    (1:use SIP Server IP)                       ^
&MaxForwards-                       (+1 - +255:default 70)                      ^
                                                                                ^
&IncludeQuintumHeader-              (0:disable)                                 ^
                                    (1:enable,default)                          ^
&UserNameAsURI-                     (0:disable,default)                         ^
                                    (1:enable)                                  ^
&RequestReTransmitCount-            (+3 - +18:default 11)                       ^
&SDPin183Progress-                  (0:no)                                      ^
                                    (1:yes,default)                             ^
&AllowOnlyProxyCalls-               (0:all calls)                               ^
                                    (1:from proxy,default)                      ^
&Send180Ringing-                    (0:disabled)                                ^
                                    (1:enabled)                                 ^
&Send183Progress-                   (0:disabled)                                ^
                                    (1:enabled)                                 ^
&SipPstnInterworking-               (0:disabled)                                ^
                                    (1:enabled)                                 ^
&ForceAlertOn183-		    (0:disabled)				^
				    (1:enabled)					^
&PRACKMethod-                       (0:disabled)                                ^
                                    (1:supported)                               ^
                                    (2:required)                                ^
&SessionTimer-                      (0:disabled)                                ^
                                    (1:supported)                               ^
                                    (2:required)                                ^
&SessionTimerMinSE-                 (300-65535:seconds,def 600)                 ^
&SessionTimerExpires-                (300-65535:seconds,def 3600)               ^
&MWIServer-                         (:IP address)                               ^
&MWIServerPort-                     (:Numeric,default 5060)                     ^
&MWISubscribeDuration-              (0 - 65535:minutes,def 60)                  ^
&MWIFailureRetryDelay-              (0 - 65535:minutes,def 30)                  ^
&UserAgentHeader-                   (:0-31 char,def Quintum1.0.0)               ^
&SIPNoConnectTimeout-               (32 - 3600:seconds,def 180)                 ^
&ProxyFailoverBehavior-             (0:no fail over)                            ^
                                    (1:fail over)                               ^
&SIPInfoFormat-                     (0:Nortel,default)                          ^
                                    (1:Cisco)                                   ^
&CLIHeaderType-                     (0:disabled)                                ^
                                    (1:Send Remote-Party-Id)                    ^
                                    (2:Q.1912.5 as TEL URI)                     ^
                                    (3:Q.1912.5 as SIP URI)                     ^
                                    (4:Ppreferred tel URI)                      ^
                                    (5:Ppreferred sip URI)                      ^
&UseFromContact-                    (0:DN)                                      ^
                                    (1:Alias Name)                              ^
&RPIDDefaultPrivacy-                (0:disabled)                                ^
                                    (1:off)                                     ^
                                    (2:URI)                                     ^
                                    (3:Name)                                    ^
                                    (4:Full)                                    ^
&UseFromContaact-		    (0:Use DN)					^
				    (1:Use Alias Name				^
&SIPTelephoneEvents-		    (0:Don't append "/1" to SDP attribute)	^
				    (1:Append "/1" to SDP attribute)		^
&SIPUseDNinRegister-		    (0:Use PrimaryUser in Register)		^
				    (1:Use DN from channel map in Register)	^
&ConferenceFactoryName-             (:0-31 charac,name)                         ^
&ConferenceFactoryPort-             (:port num, def 5060)                       ^
&ConferenceFactoryServer-             (:server name)                            ^
&DirectGWRouting-                   (0:disable)                                 ^
                                    (1:enable)                                  ^
&GKBusyOut-                         (0:disable)                                 ^
                                    (1:enable)                                  ^
&SIPRegisterOnBootup-            (0:disable)                                    ^
                                 (1:enable)                                     ^
&SDPinInvite-                    (0:disabled)                                   ^
                                 (1:send SDP)                                   ^
@5800~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <ss7sg>.                                                          }^
{    IPRoutingGroup is located under Gateway, Which is used to configure the   }^
{    voice codec profile and voice activity, transmit and receive the gain for }^
{    voice signal.                                                             }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <ss7sg>.                                                            ^
     IPRoutingGroup is an located under Gateway, Which is used to configure the ^
     voice codec profile and voice activity, transmit and receive gain the voice^
     signal.                                                                    ^
                                                                                ^
@5804~{------------------------------------------------------------------------}^
{Set ss7sg <parameter><value>                                                  }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{name <name>-        (:up to 31 char)                                          }^
{                                                                              }^
{DelayACM <dacm>-       (0:Do not wait for alerting)                           }^
{                       (1:Wait for alerting)                                  }^
{                                                                              }^
{OutBndBearerCap <obbc>- (0:3.1KHz)                                            }^
{                        (1:Speech,default)                                    }^
{DefaultANI <dani>-                                                            }^
{                       (:Phone number)                                        }^
{                                                                              }^
{DefaultANITON <daniton>-                                                      }^
{                       (0:Unknown,default)                                    }^
{                       (1:International)                                      }^
{                       (2:National)                                           }^
{                       (4:Subscriber)                                         }^
{DefaultANINPI <daninpi>-                                                      }^
{                       (1:ISDN/Telephony,default)                             }^
{                       (3:Data Numbering)                                     }^
{                       (4:Telex Numbering)                                    }^
{                                                                              }^
{CallingCategory <cc>-                                                         }^
{                       (10:Ordinary subscriber,default)                       }^
{                       (12:Data Call,voice band data)                         }^
{                       (13:Test Call)                                         }^
{IgnoreTONNPI <itnpi>-                                                         }^
{                       (0:TON and NPI)                                        }^
{                       (1:Ignore TON and NPI)                                 }^
{                       (128:Ignore TON and NPI)                               }^
{                       (145:Treat Int TON,ISDN NPI)                           }^
{PROTocol <prot>-       (1:ITU ISUP 1992)                                      }^
{                       (4:ISUP R,Russian ISUP)                                }^
{.......................(5:Hong Kong)                                          }
{DefaultANIScreenInd <danisi>-  (0:passthrough received)                       }^
{                               (1:user-provided)                              }^
{                               (2:user-provided,passed)                       }^
{                               (3:user-provided,failed)                       }^
{                               (4:network provided)                           }^
{DefaultANIPresentationInd <danipi>-   (0:relay ANI)                           }^
{                                      (1:No ANI,set CLIR)                     }^
{                                      (2:Always set CLIR and Relay ANI)       }^
{RElayANI <reani>-              (0:No Relay ANI)                               }^
{                               (1:Relay ANI)                                  }^
{                               (2:Relay ANI with TON,NPI)                     }^
{RejCallNoANI <rcnani>-         (0:Accept all calls)                           }^
{                               (1:Reject no/short ANI calls)                  }^
{ 				(2:Route no/short ANI calls to IVR             }^
{CauseRejNoANI <crnani>-        (:cause value when rejecting no ANI calls)     }^
{MinimumANILength <manil>-      (:minimum acceptable value of ANI)             }^
--------------------------------------------------------------------------------^
Set %SS7SignalingGroup <parameter><value>                                       ^
   where <parameter> is:                                                        ^
                                                                                ^
&name-                                                                          ^
                        (:up to 31 char)                                        ^
                                                                                ^
&DelayACM-                                                                      ^
                        (0:Do not wait for alerting)                            ^
                        (1:Wait for alerting)                                   ^
                                                                                ^
&OutBndBearerCap-        (0:3.1KHz)                                             ^
                         (1:Speech,default)                                     ^
&DefaultANI-                                                                    ^
                        (:Phone number)                                         ^
                                                                                ^
&DefaultANITON-                                                                 ^
                        (0:Unknown,default)                                     ^
                        (1:International)                                       ^
                        (2:National)                                            ^
                        (4:Subscriber)                                          ^
&DefaultANINPI-                                                                 ^
                        (1:ISDN/Telephony,default)                              ^
                        (3:Data Numbering)                                      ^
                        (4:Telex Numbering)                                     ^
                                                                                ^
&CallingCategory-                                                               ^
                        (10:Ordinary subscriber,default)                        ^
                        (12:Data Call,voice band data)                          ^
                        (13:Test Call)                                          ^
&IgnoreTONNPI-                                                                  ^
                        (0:TON and NPI)                                         ^
                        (1:Ignore TON and NPI)                                  ^
                        (128:Ignore TON and NPI)                                ^
                        (145:Treat Int TON,ISDN NPI)                            ^
&PROTocol-              (1:ITU ISUP 1992)                                       ^
                        (4:ISUP R,Russian ISUP)                                 ^
                        (5:Hong Kong)                                           ^
&DefaultANIScreenInd-           (0:passthrough received)                        ^
                                (1:user-provided)                               ^
                                (2:user-provided,passed)                        ^
                                (3:user-provided,failed)                        ^
                                (4:network provided)                            ^
&DefaultANIPresentationInd-            (0:relay ANI)                            ^
                                       (1:No ANI,set CLIR)                      ^
                                       (2:Always set CLIR and Relay ANI)        ^
&RElayANI-                                                                      ^
             (0:No Relay ANI)                                                   ^
             (1:Relay ANI)                                                      ^
             (2:Relay ANI with TON,NPI)                                         ^
{RejCallNoANi <rcnani>-		(0:Accept all calls)                           }^
{                               (1:Reject no/short ANI calls)                  }^
{				(2:Route no/short ANI calls to IVR)	       }^
{CauseRejNoANI <crnani>-        (:cause value when rejecting no ANI calls)     }^
{MinimumANILength <manil>-      (:minimum acceptable value of ANI)             }^
									       }^
@5900~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <ss7g>.                                                           }^
{    SS7Gateway protocol                                                       }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <ss7g>.                                                             ^
     SS7Gateway protocol                                                        ^
                                                                                ^
@5904~{------------------------------------------------------------------------}^
{Set ss7gateway <parameter><value>                                             }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Name <name>-           (:up to 31 characters)                                 }^

{LocalID <lid>-         (:numeric)                                             }^
{PrimaryGatewayIPAddr <pgipa>-  (:IP address)                                  }^
{                                                                              }^
{SecondaryGatewayIPAddr <sgipa>-  (:IP address)                                }^
{                                                                              }^
{PrimaryGatewayPort <pgp>-     (:port number,default 6767)                     }^
{SecondaryGatewayPort <sgp>-   (:port number,default 2525)                     }^
{                                                                              }^
{PrimaryGatewayID <pgid>-                                                      }^
{              (:1-255)                                                        }^
{SecondaryGatewayID <sgid>-                                                    }^
{              (:1-255)                                                        }^
{                                                                              }^
{PrimaryGatewayPassWord <pgpw>-       (:password,alphanumeric)                 }^
{SecondaryGatewayPassWord <sgpw>-     (:password,alphanumeric)                 }^
--------------------------------------------------------------------------------^
Set %SS7Gateway <parameter><value>                                              ^
   where <parameter> is:                                                        ^
                                                                                ^
&Name-           (:up to 31 characters)                                         ^
&LocalID-        (:numeric)                                                     ^
&PrimaryGatewayIPAddr-  (:IP address)                                           ^
&SecondaryGatewayIPAddr- (:IP address)                                          ^
&PrimaryGatewayPort-     (:port number,default 6767)                            ^
&SecondaryGatewayPort-   (:port number,default 2525)                            ^
&PrimaryGatewayID-                                                              ^
              (:1-255)                                                          ^
&SecondaryGatewayID-                                                            ^
               (:1-255)                                                         ^
                                                                                ^
&PrimaryGatewayPassWord-       (:password,alphanumeric)                         ^
&SecondaryGatewayPassWord-     (:password,alphanumeric)                         ^
@5900~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <rtmi>.                                                           }^
{    Tunnel Server Info                                                        }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <rtmi>.                                                             ^
     RemoteTenorManagerInfo                                                     ^
                                                                                ^
@6000~{------------------------------------------------------------------------}^
{Set RemoteTenorManagerInfo <parameter><value>                                 }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{ConnectTimer <ct>-       (:seconds)                                           }^
{                                                                              }^
{Udp <u>-   (0:no udp)                                                         }^
{           (1:use udp)                                                        }^
{                                                                              }^
{PrimaryServerPort <psp>-  (:port number,default 2525)                         }^
{                                                                              }^
{PrimaryServer <ps>-  (:IP address)                                            }^
{                                                                              }^
{SecondaryServerPort <ssp>-       (:port number,default 2525)                  }^
{SecondaryServer <ss>-   (:IP address)                                         }^
--------------------------------------------------------------------------------^
Set %RemoteTenorManagerInfo <parameter><value>                                  ^
   where <parameter> is:                                                        ^
                                                                                ^
&ConnectTimer- (:seconds)                                                       ^
                                                                                ^
&Udp- (0:no udp)                                                                ^
      (1:use udp)                                                               ^
&PrimaryServerPort-  (:port number,default 2525)                                ^
                                                                                ^
&PrimaryServer-  (:IP address)                                                  ^
                                                                                ^
&SecondaryServerPort-     (:port number,default 2525)                           ^
&SecondaryServer-   (:IP address)                                               ^
@6100~{------------------------------------------------------------------------}^
{Set DNSServer <parameter><value>                                              }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{UseConfiguredDNSServers <ucdnss>-  (0:disabled,default)                       }^
{                                   (1:enabled)                                }^
{PrimaryServerIPAddr <psipa>-       (:IP address)                              }^
{SecondaryServerIPAddr <ssipa>-     (:IP address)                              }^
{                                                                              }^
--------------------------------------------------------------------------------^
Set %DNSServer <parameter><value>                                               ^
   where <parameter> is:                                                        ^
                                                                                ^
&UseConfiguredDNSServers-  (0:disabled)                                         ^
                           (1:enabled,default)                                  ^
&PrimaryServerIPAddr-      (:IP address)                                        ^
&SecondaryServerIPAddr-    (:IP address)                                        ^
                                                                                ^
@6200~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <dnshe>.                                                          }^
{    DNSHosts table.                                                           }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <DNSHostEntry>.                                                     ^
     DNSHosts table.                                                            ^
                                                                                ^
@6203~{------------------------------------------------------------------------}^
{Add, Change and Remove command can be used with DNSHost tables, also the      }^
{following commands are used to                                                }^
{set DNSHostEntry table.                                                       }^
{                                                                              }^
{IPAddress <ipa>-               (:DNS Host IP)                                 }^
{HostName <hn>-                 (:URL,DNS host)                                }^
{Priority <p>-                  (:Numeric priority of DNS host)                }^
{                                                                              }^
--------------------------------------------------------------------------------^
Add, Change and Remove command can be used with DNSHosts tables, also the       ^
following commands are used to:                                                 ^
                                                                                ^
Set %DNSHostEntry <param> <value>:                                              ^
                                                                                ^
&IPAddress-                     (:DNS Host IP)                                  ^
&HostName-                      (:URL,DNS host)                                 ^
&Priority-                      (:Numeric priority of DNS host)                 ^
                                                                                ^
@6204~{------------------------------------------------------------------------}^
{Change               - a config command used to change table values by the    }^
{                       index                                                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                -a config command used to change table values by the      ^
                       index                                                    ^
                                                                                ^
                                                                                ^
@6206~{------------------------------------------------------------------------}^
{rem                   -a config command used to remove entry from the tables. }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                  -a config command used to remove entry from the tables. ^
                                                                                ^
@6300~{Current Level                                                           }^
{------------------------------------------------------------------------------}^
{Level Name: <idnisx>                                                          }^
{    InboundDNISXlation table.                                                 }^
{                                                                              }^
Current Level                                                                   ^
--------------------------------------------------------------------------------^
Level Name: <InboundDNISXlation>.                                               ^
     InboundDNISXlation table.                                                  ^
                                                                                ^
@6303~{------------------------------------------------------------------------}^
{Add, Change and Remove command can be used with DNSHost tables, also the      }^
{following commands are used to                                                }^
{set InboundDNISXlation table.                                                 }^
{                                                                              }^
{Pattern <p>-              (:Set number pattern)                               }^
{Replacement <r>-          (:Added digits PSTN requires)                       }^
{TON <ton>-                (:Type of Number)                                   }^
{NPI <npi>-                (:Number Plan ID)                                   }^
--------------------------------------------------------------------------------^
Add, Change and Remove command can be used with Inbound tables, also the        ^
following commands are used to:                                                 ^
                                                                                ^
Set %InboundDNISXlation <param> <value>:                                        ^
                                                                                ^
&Pattern-                  (:Set number pattern)                                ^
&Replacement-              (:Added digits PSTN requires)                        ^
&TON-                      (:Type of Number)                                    ^
&NPI-                      (:Number Plan ID)                                    ^
                                                                                ^
@6304~{------------------------------------------------------------------------}^
{Change               - a config command used to change table values by the    }^
{                       index                                                  }^
{                                                                              }^
--------------------------------------------------------------------------------^
Change                -a config command used to change table values by the      ^
                       index                                                    ^
                                                                                ^
                                                                                ^
@6306~{------------------------------------------------------------------------}^
{rem                   -a config command used to remove entry from the tables. }^
{                                                                              }^
--------------------------------------------------------------------------------^
Remove                  -a config command used to remove entry from the tables. ^
                                                                                ^
@6400~{------------------------------------------------------------------------}^
{Set SurvivabilityParameters <parameter><value>                                }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{ListeningPort <lp>-  (:port number,def 5060)                                  }^
{UseLocalGateway <ulg>-  (0:disabled)                                          }^
{                     (1:enabled)                                              }^
{DefaultRouteIPAddress <dripa>- (:IP Address)                                  }^
{DefaultRoutePort <drp>-      (:port number,def 5061)                          }^
--------------------------------------------------------------------------------^
Set %SurvivabilityParameters <parameter><value>                                 ^
   where <parameter> is:                                                        ^
                                                                                ^
&ListeningPort-  (:port number,def 5060)                                        ^
&UseLocalGateway-   (0:disabled)                                                ^
                    (1:enabled)                                                 ^
&DefaultRouteIPAddress- (:IP Address)                                           ^
&DefaultRoutePort-      (:port number,def 5061)                                 ^
                                                                                ^
@6500~{------------------------------------------------------------------------}^
{Set FlexibleIVRServer <parameter><value>                                      }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{SChedulerInterval <si>-  (0:disabled)                                         }^
{                         (1 - 240:seconds,max 240)                            }^
{ListenPort <lp>-  (:port,default 9999)                                        }^
{KeepAliveInterval <kai>-   (:0-6000,def 30)                                   }^
(PrimaryServerPort <psp>- (:port,default 9999)                                 }^
(PrimaryServerIPAddr <psipa>-  (:IP address)                                   }^
(SecondaryServerPort <ssp>-  (:port,default 9999)                              }^
(SecondaryServerIPAddr <ssipa>-  (:IP address)                                 }^
--------------------------------------------------------------------------------^
Set %FlexibleIVRServer <parameter><value>                                       ^
   where <parameter> is:                                                        ^
                                                                                ^
&SChedulerInterval-  (0:disabled)                                               ^
                     (1 - 240:seconds,max 240)                                  ^
&ListenPort-  (:port,default 9999)                                              ^
&KeepAliveInterval-   (:0-6000, def 30)                                         ^
&PrimaryServerPort- (:port,default 9999)                                        ^
&PrimaryServerIPAddr-  (:IP address)                                            ^
&SecondaryServerPort-  (:port,default 9999)                                     ^
&SecondaryServerIPAddr-  (:IP address)                                          ^
@6600~{------------------------------------------------------------------------}^
{Set AutoProvisioning <parameter><value>                                       }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Enabled <e>-  (0:disabled)                                                    }^
{              (1:enabled)                                                     }^
{ProvisionEnable <pe>-   (0: enable,default)                                   }^
{                        (1:upload,reset)                                      }^
{                        (2:upload,possible reset)                             }^
{                        (3:upload on curr dbase)                              }^
{ProvisionErrorPolicy <pep>-    (0:no errors)                                  }^
{                               (1:min errors)                                 }^
{                               (2:max errors)                                 }^
{ResyncOnReset <ror>-           (0:disable)                                    }^
{                               (1:enable,default)                             }^
{ResyncRandomDelay <rdr>-       (:seconds,def 15)                              }^
{ResyncPeriodic <rp>-           (:seconds,def 86400)                           }^
{ResyncErrorRetryDelay <rerd>-    (:seconds,def 360)                           }^
{ProfileRuLe <prl>- (:url of config file)                                      }^
{ConnectTimeout <ct>- (:seconds,def 30)                                        }^
{TransferTimeout <tt>- (:seconds,def 3600)                                     }^
{ResyncNewCallsAllowed <rnca>-  (0:disable)                                    }^
{                               (1:enable)                                     }^
{ResyncAfterUpgradeAttempt <raua>-  (0:disable)                                }^
{                                   (1:enable)                                 }^
{ForcedResyncDelay <frd>- (:seconds,def 120)                                   }^
{UpgradeEnable.<ue>-      (0:disable)                                          }^
{                         (1:enable)                                           }^
{UpgradeRule <ur>-        (:URL of new code)                                   }^
{UpgradeRElease. <ure>-  (:firmware version)                                   }^
{UpgradeErrorRetryDelay <uerd>-  (:seconds,def 3600)                           }^
{ProvisionLog <pl>-  (:log output )                                            }^
{ResyncTimeofDay<rtd>- (:hh,mm)                                                }^
{TFTPServer <tftps>- (:internal use)                                           }^
{Status <s>- (:internal use)                                                   }^
--------------------------------------------------------------------------------^
Set %AutoProvisioning <parameter><value>                                        ^
   where <parameter> is:                                                        ^
                                                                                ^
&Enabled-  (0:disabled)                                                         ^
           (1:enabled)                                                          ^
&ProvisionEnable-       (0:enable,default)                                      ^
                        (1:upload,reset)                                        ^
                        (2:upload,possible reset)                               ^
                        (3:upload on curr dbase)                                ^
&ProvisionErrorPolicy-    (0:no errors)                                         ^
                          (1:min errors)                                        ^
                          (2:max errors)                                        ^
&ResyncOnReset-          (0:disable)                                            ^
                         (1:enable,default)                                     ^
&ResyncRandomDelay-       (:seconds,def 15)                                     ^
&ResyncPeriodic-          (:seconds,def 86400)                                  ^
&ResyncErrorRetryDelay-    (:seconds,def 360)                                   ^
&ProfileRuLe-           (:url of Tenor config file)                             ^
&ConnectTimeout- (:seconds,def 30)                                              ^
&TransferTimeout- (:seconds,def 3600)                                           ^
&ResyncNewCallsAllowed-    (0:disable)                                          ^
                          (1:enable)                                            ^
&ResyncAfterUpgradeAttempt-  (0:disable)                                        ^
                             (1:enable)                                         ^
&ForcedResyncDelay- (:seconds,def 120)                                          ^
&UpgradeEnable-      (0:disable)                                                ^
                     (1:enable)                                                 ^
&UpgradeRule-       (:URL of new code)                                          ^
&UpgradeRElease-  (:firmware version)                                           ^
&UpgradeErrorRetryDelay-  (:seconds,def 3600)                                   ^
&ProvisionLog- (0:0x0000 log bits)                                              ^
               (1:0x0001 log bits)                                              ^
               (2:0x0010 log bits)                                              ^
               (3:0x0011 log bits)                                              ^
               (4:0x0100 log bits)                                              ^
               (5:0x0101 log bits)                                              ^
               (6:0x0110 log bits)                                              ^
               (7:0x0111 log bits)                                              ^
               (8:0x1000 log bits)                                              ^
               (9:0x1001 log bits)                                              ^
               (10:0x1010 log bits)                                             ^
               (11:0x1011 log bits)                                             ^
               (12:0x1100 log bits)                                             ^
               (13:0x1101 log bits)                                             ^
               (14:0x1110 log bits)                                             ^
               (15:0x1111 log bits)                                             ^
               (@:Provisioning Log bits:)                                       ^
 (Bit 3:Print connection status in RS-232 console)                              ^
 (Bit 2:Log the configuration file received from the Provisioning Server)       ^
 (Bit 1:Log parsing result of the received configuration file)                  ^
 (Bit 0:Log execution result of the received configuration file)                ^
&ProvisionMask- (:encrypt/mask SIP UA)                                          ^
&ResyncTimeofDay- (:in hh:mm)                                                   ^
&TFTPServer- (:internal use)                                                    ^
&Status- (:internal use)                                                        ^
@6700~{------------------------------------------------------------------------}^
{Set UserAgent <parameter><value>                                              }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{Enabled <e>-  (0:disabled)                                                    }^
{              (1:enabled)                                                     }^
{ListenPort <lp>-  (:port,default 5060)                                        }^
{PrimaryUser <pu>-           (:username)                                       }^
{PrimaryPassword <pp>-       (:up to 31 char)                                  }^
{SecondaryUser <su>-           (:username)                                     }^
{SecondaryPassword <sp>-       (:up to 31 char)                                }^
{Contacts <c>-       (:contact,alphanumeric,1-4)                               }^
{MWIUserName <mwiun>-      (:name,15 char)                                     }^
{MWIPassword.<mwip>-       (:password,15 char)                                 }^
--------------------------------------------------------------------------------^
Set %UserAgent <parameter><value>                                               ^
   where <parameter> is:                                                        ^
                                                                                ^
&Enabled-  (0:disabled)                                                         ^
           (1:enabled)                                                          ^
&ListenPort-  (:port,default 5060)                                              ^
&PrimaryUser-    (:username)                                                    ^
&PrimaryPassword-       (:up to 31 char)                                        ^
&SecondaryUser-           (:username)                                           ^
&SecondaryPassword-      (:up to 31 char)                                       ^
&Contacts-                          (:contact,alphanumeric,1-4)                 ^
&MWIUserName-      (:name,15 char)                                              ^
&MWIPassword-       (:password,15 char)                                         ^
@6800~{------------------------------------------------------------------------}^
{Set DNChannelMapEntry <parameter><value>                                      }^
{   where <parameter> is:                                                      }^
{                                                                              }^
{PublicDN <pdn>-   .  (0:disabled)                                             }^
{                     (1:enabled)                                              }^
{AliasName<an>-                 (:name,31 char)                                }^
{SPan <sp>-               (:span,0-255),                                       }^
{CHannel <ch>-                  (:channel,0-255).                              }^
{CallingNAMe <cnam>-       (:name,15 char)                                     }^
{RegisterDN<rdn>-     (0:disabled)                                             }^
{                     (1:enabled)                                              }^
{DN<dn>-              (:31 char string)                                        }^
--------------------------------------------------------------------------------^
Set %DNChannelMapEntry <parameter><value>                                       ^
   where <parameter> is:                                                        ^
                                                                                ^
&PublicDN-   .  (0:disabled)                                                    ^
                (1:enabled)                                                     ^
&AliasName-     (:name,31 char)                                                 ^
&SPan-               (:span,0-255),                                             ^
&CHannel-                  (:channel,0-255).                                    ^
&CallingNAMe-       (:name,15 char)                                             ^
&RegisterDN-   (0:disabled)                                                     ^
               (1:enabled)                                                      ^
&DN-              (:31 char string)                                             ^
\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\\^

