;***********************************************************************
;
; NETPRISM.INF
;
;   This installation script supports Windows 95,98,Me&2000 for the
;   Wireless LAN Card.
;
;   Copyright (c) 2003
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer = 04/10/2003, 3.0.4
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
CatalogFile         = PRISMNIC.cat
 

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = VID_2001&PID_3700
 
[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %PRISM_USB1_STR%    = PRISM_USB1,    USB\VID_2001&PID_3700

;==========================================
[PRISM_USB1]            ; Win9x
 AddReg         = PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy 

[PRISM_USB1.NT]         ; Win2k
 AddReg         = PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 15     ; USB
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_USB1.NT.Services]
 AddService     = PRISM_USB, 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_USB1.reg]
 HKR,Ndi        ,DeviceID,0,"USB\VID_2001&PID_3700"
 HKR,           ,PlatformId,0,"0"
 HKR,           ,VendorDesc,0,%USB_DESC_STR%
 HKR,           ,LoadFirmware,0,"1"
 ;HKR, NDI\params\LoadFirmware,,0,"1"

;==========================================


[PRISM_USB_DRIVER.Service]
 DisplayName    = %PRISM_USB_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMUSB.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_USB.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_USB"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"15"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMUSB.sys"

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,"1"
 ;HKR,NDI\params\PSMode,,0,"1"
 HKR,Ndi\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,"enum"
 HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,"1"
 
[COMMON_NDIS.reg.NT]
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,"1"
 ;HKR,NDI\params\PSMode,,0,"1"
 HKR,Ndi\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,"enum"
 HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,"1"
 
[COMMON.reg]
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,"3"
 ;HKR,NDI\params\ListenInterval,,0,"3"
 HKR,Ndi\params\ListenInterval,default,0,"3"
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,"int"
 HKR,NDI\params\ListenInterval,flag,1,"30","00","00","00"
 HKR,NDI\params\ListenInterval,min,0,"0"
 HKR,NDI\params\ListenInterval,max,0,"77"
 HKR,NDI\params\ListenInterval,step,0,"1"
 HKR,NDI\params\ListenInterval,optional,0,"1"
 
 HKR,defaults,RTSThresh,0,"2432"
 ;HKR,NDI\params\RTSThresh,,0,"2432"
 HKR,Ndi\params\RTSThresh,default,0,"2432"
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,"int"
 HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
 HKR,NDI\params\RTSThresh,min,0,"0"
 HKR,NDI\params\RTSThresh,max,0,"2432"
 HKR,NDI\params\RTSThresh,step,0,"64"
 HKR,NDI\params\RTSThresh,optional,0,"1"
 
 HKR,defaults,FragThresh,0,"2432"
 ;HKR,NDI\params\FragThresh,,0,"2432"
 HKR,Ndi\params\FragThresh,default,0,"2432"
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,"int"
 HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
 HKR,NDI\params\FragThresh,min,0,"256"
 HKR,NDI\params\FragThresh,max,0,"2432"
 HKR,NDI\params\FragThresh,step,0,"128"
 HKR,NDI\params\FragThresh,optional,0,"1"
 
 HKR,defaults,PreambleMode,0,"1"
 ;HKR,NDI\params\PreambleMode,,0,"1"
 HKR,Ndi\params\PreambleMode,default,0,"1"
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,"enum"
 HKR,NDI\params\PreambleMode,flag,1,"30","00","00","00"
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,"1"
 
 HKR,defaults,AuthentAlg,0,"65535"
 ;HKR,NDI\params\AuthentAlg,,0,"65535"
 HKR,NDI\params\AuthentAlg,default,0,"65535"
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,"enum"
 HKR,NDI\params\AuthentAlg,flag,1,"30","00","00","00"
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,"1"
 
 HKR,defaults,AdhocDemoMode,0,"0"
 ;HKR,NDI\params\AdhocDemoMode,,0,"0"
 ;HKR,Ndi\params\AdhocDemoMode,default,0,"0"
 ;HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 ;HKR,NDI\params\AdhocDemoMode,type,,"enum"
 ;HKR,NDI\params\AdhocDemoMode,flag,1,"30","00","00","00"
 ;HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 ;HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 ;HKR,NDI\params\AdhocDemoMode,optional,0,"1"
 

;
; Channel
; 
 HKR,defaults,DSChannel,0,"10"
 ;HKR,NDI\params\Channel,ParamDesc,,"Channel"
 ;HKR,NDI\params\Channel,type,,"enum"
 ;HKR,NDI\params\Channel,default,0,"10"
 ;HKR,NDI\params\Channel,flag,1,"30","00","00","00"
 ;HKR,NDI\params\Channel\enum,0,,"Channel  1"
 ;HKR,NDI\params\Channel\enum,1,,"Channel  2"
 ;HKR,NDI\params\Channel\enum,2,,"Channel  3"
 ;HKR,NDI\params\Channel\enum,3,,"Channel  4"
 ;HKR,NDI\params\Channel\enum,4,,"Channel  5"
 ;HKR,NDI\params\Channel\enum,5,,"Channel  6"
 ;HKR,NDI\params\Channel\enum,6,,"Channel  7"
 ;HKR,NDI\params\Channel\enum,7,,"Channel  8"
 ;HKR,NDI\params\Channel\enum,8,,"Channel  9"
 ;HKR,NDI\params\Channel\enum,9,,"Channel 10"
 ;HKR,NDI\params\Channel\enum,10,,"Channel 11"
 ;HKR,NDI\params\Channel\enum,11,,"Channel 12"
 ;HKR,NDI\params\Channel\enum,12,,"Channel 13"
 ;HKR,NDI\params\Channel\enum,13,,"Channel 14"
 
 HKR,defaults,LoadFirmware,0,"1"
 ;HKR,NDI\params\LoadFirmware,,0,"1" ; Moved to device specific entry
 HKR,Ndi\params\LoadFirmware,default,0,"1"
 HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
 HKR,NDI\params\LoadFirmware,type,,"enum"
 HKR,NDI\params\LoadFirmware,flag,1,"30","00","00","00"
 HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
 HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
 HKR,NDI\params\LoadFirmware,optional,0,"1"
 
 HKR,defaults,PDwellTime,0,"120"
 ;HKR,NDI\params\PDwellTime,,0,"120"
 HKR,Ndi\params\PDwellTime,default,0,"120"
 HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
 HKR,NDI\params\PDwellTime,type,0,"int"
 HKR,NDI\params\PDwellTime,flag,1,"20","00","00","00"
 HKR,NDI\params\PDwellTime,min,0,"0"
 HKR,NDI\params\PDwellTime,max,0,"1000"
 HKR,NDI\params\PDwellTime,step,0,"10"
 HKR,NDI\params\PDwellTime,optional,0,"1"
 
 HKR,defaults,11dMode,0,"0"
 ;HKR,NDI\params\11dMode,,0,"0"
 HKR,Ndi\params\11dMode,default,0,"0"
 HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
 HKR,NDI\params\11dMode,type,,"enum"
 HKR,NDI\params\11dMode,flag,1,"30","00","00","00"
 HKR,NDI\params\11dMode\enum,0,,"None"
 HKR,NDI\params\11dMode\enum,1,,"Strict"
 HKR,NDI\params\11dMode\enum,2,,"Flexible"
 HKR,NDI\params\11dMode,optional,0,"1"

 
;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[PRISM_DRIVER.copy]
 PRISMUSB.sys

[PRISM_DRIVER.copy.NT]
 PRISMUSB.sys

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 PRISMUSB.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 PRISMUSB.sys           = 1

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "D-Link"
 VER_VENDOR_NAME_STR    = "D-Link"

 PRISM_USB1_STR         = "D-Link Air DWL-122 Wireless USB Adapter"

 PRISM_USB_SERVICE_DISPLAY  = "D-Link Air DWL-122 Wireless USB Adapter Driver"
 INSTALL_DISK_STR       = "D-Link Air DWL-122 Wireless USB Adapter Install Disk"

 ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save"
 PDWELL_STR             = "Passive Scan Dwell Time"

 LOAD_FIRMWARE_STR      = "Firmware Download"

 USB_DESC_STR           = "D-Link Air DWL-122 Wireless USB Adapter"
 MDC_CONTROL_STR        = "802.11D Control"