;
;          Copyright (c) 1998-1999 Harris Semiconductor
;          All Rights Reserved.
;
;    $Logfile:  $
;    $Revision:  $
;    $Date:  $
;    $Author:  $
;
;
[version]
LayoutFile=layout.inf
signature="$CHICAGO$"
Class=Net
Provider=%HARRIS_STR%

[DestinationDirs]
DefaultDestDir				=11 ; LDID_SYS
PRISM.ndis3.CopyFiles			=11 ; LDID_SYS
PRISM.inf.CopyFiles			=17 ; LDID_INF
PRISM.exe.CopyFiles			=10 ; LDID_EXE

[Manufacturer]
%HARRIS_STR%=GT11

[GT11]
%HARRIS_PCMCIA_PRISM3_STR%=PRISM_PCMCIA_PRISM3.ndi, PCMCIA\D-Link_DWL-650_11Mbps_WLAN_Card-F360

[PRISM_PCMCIA_PRISM3.ndi]
;DelReg=PRISM.reg.del
AddReg=PRISM_PCMCIA_PRISM3.ndi.reg,PRISM.reg,PRISM_PCMCIA.reg
MaxInstance=1

[PRISM_PCMCIA_PRISM3.ndi.reg]
HKR,Ndi,DeviceID,,"PCMCIA\D-Link_DWL-650_11Mbps_WLAN_Card-F360"
HKR,,BusType,,8

[PRISM.reg]
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,gt11.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

;
; NDIS Info
;
HKR,NDIS,LogDriverName,,"gt11"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A

;
; Interfaces
;
HKR,NDI\Interfaces,DefUpper,,"ndis3"
HKR,NDI\Interfaces,DefLower,,"ethernet"
HKR,NDI\Interfaces,UpperRange,,"ndis3"
HKR,NDI\Interfaces,LowerRange,,"ethernet"

;
; Install sections
;
HKR,NDI\Install,ndis3,,"PRISM.ndis3"

;
; Vendor Description
;
HKR,,VendorDesc,0,"D-Link DWL-650 11Mbps WLAN Adapter"

;
; AP Density
;
;HKR,,APDensity,,1
;HKR,defaults,APDensity,,1

;
; StationName
;
;HKR,,StationName,,"Client"
;HKR,defaults,StationName,,"Client"

;
; SSID
; 
HKR,,SSID,,%SSID_DEF_STR%
;HKR,defaults,SSID,,%SSID_DEF_STR%
HKR,NDI\params\SSID,ParamDesc,,"SSID"
HKR,NDI\params\SSID,type,,edit
HKR,NDI\params\SSID,limitText,,32
HKR,NDI\params\SSID,default,,%SSID_DEF_STR%
HKR,NDI\params\SSID,flag,1,30,00,00,00

HKR,,ATIMWindow,0,0
;HKR,defaults,ATIMWindow,0,0
;HKR,NDI\params\ATIMWindow,,0,0
;HKR,NDI\params\ATIMWindow,ParamDesc,,%ATIMWINDOW_STR%
;HKR,NDI\params\ATIMWindow,flag,1,30,00,00,00
;HKR,NDI\params\ATIMWindow,type,,int
;HKR,Ndi\params\ATIMWindow,default,,0
;HKR,NDI\params\ATIMWindow,optional,0,0

HKR,,ListenInterval,0,3
;HKR,defaults,ListenInterval,0,3
;HKR,NDI\params\ListenInterval,,0,3
;HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
;HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
;HKR,NDI\params\ListenInterval,type,,int
;HKR,Ndi\params\ListenInterval,default,,3
;HKR,NDI\params\ListenInterval,min,0,0
;HKR,NDI\params\ListenInterval,max,0,77
;HKR,NDI\params\ListenInterval,step,0,1
;HKR,NDI\params\ListenInterval,optional,0,0

;
; Channel
; 
HKR,,DSChannel,,1
;HKR,defaults,DSChannel,,1
HKR,NDI\params\DSChannel,ParamDesc,,"Channel"
HKR,NDI\params\DSChannel,type,,enum
HKR,NDI\params\DSChannel,default,,6
HKR,NDI\params\DSChannel,flag,1,30,00,00,00
HKR,NDI\params\DSChannel\enum,1,,"Channel  1"
HKR,NDI\params\DSChannel\enum,2,,"Channel  2"
HKR,NDI\params\DSChannel\enum,3,,"Channel  3"
HKR,NDI\params\DSChannel\enum,4,,"Channel  4"
HKR,NDI\params\DSChannel\enum,5,,"Channel  5"
HKR,NDI\params\DSChannel\enum,6,,"Channel  6"
HKR,NDI\params\DSChannel\enum,7,,"Channel  7"
HKR,NDI\params\DSChannel\enum,8,,"Channel  8"
HKR,NDI\params\DSChannel\enum,9,,"Channel  9"
HKR,NDI\params\DSChannel\enum,10,,"Channel 10"
HKR,NDI\params\DSChannel\enum,11,,"Channel 11"
HKR,NDI\params\DSChannel\enum,12,,"Channel 12"
;HKR,NDI\params\DSChannel\enum,13,,"Channel 13"
;HKR,NDI\params\DSChannel\enum,14,,"Channel 14"

;
; Encapsultion (i.e. Ethernet Translation)
;0-encapsul, 1 -rfc1042 2-802.1h
HKR,,Encapsulation,,1
;HKR,defaults,Encapsulation,,2

;
; TxRate
;
HKR,,TxRate,,15
;HKR,defaults,TxRate,,3
HKR,NDI\params\TxRate,ParamDesc,,"Transmit Rate"
HKR,NDI\params\TxRate,type,,enum
HKR,NDI\params\TxRate,default,,15
HKR,NDI\params\TxRate,flag,1,30,00,00,00
HKR,NDI\params\TxRate\enum,1,,"Fixed 1 Mb/s"
HKR,NDI\params\TxRate\enum,2,,"Fixed 2 Mb/s"
HKR,NDI\params\TxRate\enum,3,,"Auto Select 1 or 2"
HKR,NDI\params\TxRate\enum,4,,"Fixed 5.5 Mb/s"
HKR,NDI\params\TxRate\enum,8,,"Fixed 11 Mb/s"
HKR,NDI\params\TxRate\enum,15,,"Fully Auto"

;
; RTS Threshold
;
HKR,,RTSThresh,0,2432
;HKR,defaults,RTSThresh,0,2432
;HKR,NDI\params\RTSThresh,,0,2432
;HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
;HKR,NDI\params\RTSThresh,type,0,int
;HKR,Ndi\params\RTSThresh,default,0,2432
;HKR,NDI\params\RTSThresh,min,0,128
;HKR,NDI\params\RTSThresh,max,0,2432
;HKR,NDI\params\RTSThresh,step,0,128
;HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
;HKR,NDI\params\RTSThresh,optional,0,0

HKR,,FragThresh,0,2500
;HKR,defaults,FragThresh,0,2500
;HKR,NDI\params\FragThresh,,0,2500
;HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
;HKR,NDI\params\FragThresh,type,0,int
;HKR,Ndi\params\FragThresh,default,0,2500
;HKR,NDI\params\FragThresh,min,0,256
;HKR,NDI\params\FragThresh,max,0,2500
;HKR,NDI\params\FragThresh,step,0,128
;HKR,NDI\params\FragThresh,flag,1,20,00,00,00
;HKR,NDI\params\FragThresh,optional,0,0

;
; Network Type
;
HKR,,NetworkType,,1
;HKR,defaults,NetworkType,,1
HKR,NDI\params\NetworkType,ParamDesc,,"Network Type"
HKR,NDI\params\NetworkType,type,,enum
HKR,NDI\params\NetworkType,default,,1
HKR,NDI\params\NetworkType,flag,1,30,00,00,00
HKR,NDI\params\NetworkType\enum,1,,"Infrastructure"
HKR,NDI\params\NetworkType\enum,3,,"Ad hoc"

;
; PS Mode
;
HKR,,PSMode,,1
;HKR,defaults,PSMode,,1
HKR,NDI\params\PSMode,ParamDesc,,"Power Save Mode"
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,default,,1
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disabled"
HKR,NDI\params\PSMode\enum,2,,"Enabled"

HKR,,PSLevel,,0
;HKR,defaults,PSLevel,,0
HKR,NDI\params\PSLevel,ParamDesc,,"Power Save Level"
HKR,NDI\params\PSLevel,type,,enum
HKR,NDI\params\PSLevel,default,,0
HKR,NDI\params\PSLevel,flag,1,30,00,00,00
HKR,NDI\params\PSLevel\enum,0,,"Normal"
HKR,NDI\params\PSLevel\enum,1,,"Enhanced"


;
;	Wep Required
;
HKR,,WepReq,0,0
;HKR,defaults,WepReq,0,0
;HKR,NDI\params\WepReq,,0,0
;HKR,NDI\params\WepReq,ParamDesc,,%WEPREQ_STR%
;HKR,NDI\params\WepReq,flag,1,30,00,00,00
;HKR,NDI\params\WepReq,type,,enum
;HKR,Ndi\params\WepReq,default,,0
;HKR,NDI\params\WepReq\enum,0,,"Disabled"
;HKR,NDI\params\WepReq\enum,2,,"Mandatory"
;HKR,NDI\params\WepReq,optional,0,0


;
; Install NDIS3 miniport driver
;
[PRISM.ndis3]
CopyFiles=PRISM.ndis3.CopyFiles,PRISM.inf.CopyFiles,PRISM.exe.CopyFiles

[PRISM.ndis3.CopyFiles]
gt11.sys

[PRISM.inf.CopyFiles]
;netCW10.inf

[PRISM.exe.CopyFiles]
;gtutil.exe

;
; other general sections
;
[PRISM_PCMCIA.reg]
HKR,NDI,CardType,,"PCMCIA"

;
; All resources are dynamically configured
;
HKR,,IOBaseAddress,1,02,00,00,00
HKR,,InterruptNumber,1,04,00,00,00
;HKR,,PCCARDAttributeMemoryAddress,1,01,00,00,00
;HKR,,PCCARDAttributeMemorySize,,1000

;
; Localizable Strings
;
[strings]
;HARRIS_STR="Harris Semiconductor"
HARRIS_STR="D-Link"
HARRIS_PCMCIA_PRISM3_STR="D-Link DWL-650 11Mbps WLAN Adapter"

ATIMWINDOW_STR="Adhoc STA - Atim Window"
LISTENINTERVAL_STR="Infrastructure STA - Listen Interval"

RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
WEPREQ_STR="Use Wep"

SSID_DEF_STR="default"
