2.0

1. Add site survey for P2P, AP Client mode under SNMP.
2. Add SSID broadcasting.
3. Add STA association table.
4. Enhance SNMP AP search function.
5. The fixed data rate is mean max. date rate.
6. SNMP utility follow rule that use read/write community string.
7. The USB password same as SNMP write community string.