
        D-Link DL10050-based FAST Ethernet Adapter
	D-Link DFE-550TX FAST Ethernet 10/100 Adapter
	D-Link DFE-550FX 100Mbps Fiber-optics Adapter
	D-Link DFE-580TX 4 Port Server Adapter
	D-Link DFE-530TXS PCI Fast Ethernet Adapter 

 	Installation for SUN PC-NFS V5.0


 Getting Started
 ---------------
    Please read all methods below and choose the one that matches your
    configuration.


    Packet Driver
    -------------
    When using PC-NFS independently, select the "OTHER" option from the
    PC-NFS installation screen.  This option works with the PACKET driver
    included in the provided driver diskette.  Copy the files listed
    below into the \NFS directory of your hard disk. These files will be
    used in the installation.

       File                     Description
    ------------     -------------------------------------
    PDNFS.SYS        PC-NFS driver program
    DLH5X.SYS       Packet driver program

    The following lists the contents of the configuration files:

    CONFIG.SYS                             AUTOEXEC.BAT
    ----------                             ------------
    SWITCHES=/F                            SET TZ=EST5EDT
    DEVICE=C:\HIMEM.SYS                    C:\DOS\SMARTDRV.EXE
    DEVICE=C:\EMM386.EXE NOEMS RAM         @PROMPT $p$g
    DOS=HIGH,UMB                           PATH=C:\NFS;C:\WINDOWS;C:\DOS;
    BUFFERS=10,0                           SET TEMP=C:\DOS
    FILES=40                               SET NFSDRIVE=C
    STACKS=0,0                             SET NFSPATH=C:\NFS
    LASTDRIVE=G                            SET TN_DIR=C:\NFS\TELNET
    SHELL=C:\DOS\COMMAND.COM C:\DOS /P     C:\NFS\PRT *
    DEVICE=C:\NFS\PCNFS.SYS /l40           C:\NFS\NET INIT
    DEVICE=C:\NFS\SOCKDRV.SYS
    DEVICE=C:\NFS\DLH5X.SYS
    DEVICE=C:\NFS\PDNFS.SYS

