;***********************************************************************
;
; OEMSETUP.INF
;
;       D-Link DWL-650 11Mbps WLAN Card .INF file
;
;***********************************************************************

;-----------------------------------------------------------------------
; OPTION TYPE
; -----------
; This identifies the Option type we are dealing with.  The different
; possible types are:
;
; COMPUTER, DISPLAY, MOUSE, KEYBOARD, LAYOUT, SCSI, PRINTER, ...
;
;  Types specific to networking:
;
; NetAdapter,        a netcard / adapter combination or just a netcard
; NetDriver,         just a netcard driver
; NetTransport,      a complete NDIS-compliant TDI transport stack
; NetService,        an NT networking service
; NetWork,           a complete network ensemble.
; NetProvider        a complete network which supports NT MPR protocol
;-----------------------------------------------------------------------

[Identification]
    OptionType = NetAdapter

;-----------------------------------------------------------------------
; PlatformsSupported
; ------------------
; This identifies the platforms supported by the adapter card.
; Possible types are:
;
; ISA, EISA, MCA and PCMCIA
;-----------------------------------------------------------------------

[PlatformsSupported]
    ISA
;    EISA
;    PCI
    PCMCIA

;-----------------------------------------------------------------------
; OPTION LIST
; -----------
; This section lists the OEM Option key names.  These keys are locale
; independent and used to represent the option in a locale independent
; manner.
;
;-----------------------------------------------------------------------

[Options]
    GTWLAN11

;***********************************************************************
; CONSTANTS FOR USING DIALOGS
;***********************************************************************

[FileConstants]
    GenericAdapterName = "D-Link DWL-650 11Mbps WLAN Card"
    GenericDriverName  = "D-Link DWL-650 11Mbps WLAN Card driver"
    GenericSysName     = "gt11.sys"
    GenericName        = "GT11"

    ;
    ;  File names, etc.
    ;
    UtilityInf      = "UTILITY.INF"
    ParamInf        = "NCPARAM.INF"
    subroutineinf   = "SUBROUTN.INF"
    SoftwareType    = "driver"
    Exit_Code       = 0

    ;
    ; EventLog Message File
    ;
    NetEventDLL     = "%SystemRoot%\System32\netevent.dll"
    IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"

    ;
    ; Product Info
    ;
    Manufacturer    = "INTERSIL"
    ProductMajorVersion     = "1"
    ProductMinorVersion     = "00"
    ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)

    ;
    ; Software
    ;
    ProductSoftwareName         = "GT11"
    ProductSoftwareImagePath    = "\SystemRoot\System32\drivers\"$(GenericSysName)
    NetRuleSoftwareType         = "gt11Sys ndisDriver gt11Driver"

    NetRuleSoftwareUse          = $(SoftwareType)
    NetRuleSoftwareBindForm     = """gt11Sys"" yes no container"

    NetRuleSoftwareClass        = {"gt11Driver basic"}
    NetRuleSoftwareBindable     = {"gt11Driver gt11Adapter non exclusive 100"}
    ;
    ; Hardware
    ;
    ProductHardwareName         = "GT11"
    NetRuleHardwareType         = "gt11 gt11Adapter"
    NetRuleHardwareBindForm     = " yes yes container"
    NetRuleHardwareClass        = {"gt11Adapter basic"}

    ;
    ; Registry Key
    ;
    ProductKeyName          = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
    ParamKeyName            = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
    PcmciaDataBaseKeyName   = $(!NTN_ServiceBase)"\Pcmcia\Database"

[GeneralConstants]
    ;
    ;  Program flow control variables.
    ;
    from      = ""
    to        = ""
    ;
    ;  Return codes; Exit_Code is set to one of these
    ;
    ExitCodeOk     = 0
    ExitCodeCancel = 1
    ExitCodeFatal  = 2

    KeyNull             = ""
    MAXIMUM_ALLOWED     = 33554432
    RegistryErrorIndex  = NO_ERROR
    KeyProduct          = ""
    KeyParameters       = ""

    TRUE    = 1
    FALSE   = 0
    NoTitle = 0

    ExitState           = "Active"
    OldVersionExisted   = $(FALSE)

    DriverPath = $(!STF_NTPATH)\drivers

[date]
    ; Now is a list which contains { Sec from 1-1-1970, Year, Month, Day, Hour,
    ; Minute, Second }
    Now = {} ? $(!LIBHANDLE) GetSystemDate


;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    ;
    ;
    read-syms Identification

    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    ;
    ;
    set Status        = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
	;
	; Check if the platforms requested is supported
	;
	ifstr(i) $($1) == ""
	    goto returnoptions
	endif

	set PlatformList = ^(PlatformsSupported, 1)
	Ifcontains(i) $($1) in $(PlatformList)
	    goto returnoptions
	else
	    set Status = STATUS_NOTSUPPORTED
	    goto finish_ReturnOptions
	endif
    else
	set Status = STATUS_NOLANGUAGE
	goto finish_ReturnOptions
    endif

    ;
    ; form a list of all the options and another of the text representing
    ;

returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL

finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]
    ;
    ; Set default values for
    ;
    set Status   = STATUS_FAILED
    ;
    ; extract parameters
    ;
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)
    Set !DebugOutputControl = 0

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
	Return STATUS_NOLANGUAGE
    endif

    set-subst LF = "\n"

    read-syms GeneralConstants
    read-syms FileConstants

    read-syms DialogConstants$(!STF_LANGUAGE)
    ifstr(i) $(!NTN_Origination) == "NCPA"
	set Continue = $(OK)
    endif
    read-syms FileConstants$(!STF_LANGUAGE)

    detect date

    set-title  $(FunctionTitle)

    set to   = Begin
    set from = Begin
    ;
    ;  Assume all is well.
    ;
    set CommonStatus = STATUS_SUCCESSFUL

    EndWait

    ;
    ;   Set up the operation-mode-based variables and gaily welcome
    ;   the user.  If the "install mode" variable is improperly set,
    ;   assume this is a new installation.
    ;

Begin = +
    Set ActivateDetection = FALSE

    Ifstr(i) $(!NTN_InstallMode) == deinstall
	set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
	set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
	set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
;        set ActivateDetection = TRUE
	set StartLabel = configureadapter
	;
	;   You cannot config the software component
	;
	Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
            Debug-Output "Cannot configure the D-Link driver software."
	    Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		Debug-Output "ShellCode error: cannot get an error string."
		goto ShellCodeError
	    endif
	    set Error = $($R0)
	    set from = end
	    set to = end
	    goto nonfatalinfo
	endif
    else
;        set ActivateDetection = TRUE
	set StartLabel = installadapter
	set OEM_ABANDON_OPTIONS = {}
	set OEM_ABANDON_SOFTWARE = FALSE
	set OEM_ABANDON_ON = TRUE
    endif

    ;****************************
    ;  set the default values

    ; I/O Base Address              = 0x300
	set IOBaseAddrUIVal		= "300"

	; IRQ Level = 9
	set IRQValueUIVal		= "10"

	; PcmciaValue = 0/1
	set PcmciaValue			= 1
	set Chk1 				= "ON"

	; Ethernet conversion mode = "Encapsulated"/"RFC1042"/"802.1h"
;	set EthConvValue		= "802.1h"
	set EthConvValue		= 2

	; Station Mode related default values
	set PSLevelValue		= 0;

	; Power Save Mode = "Disabled"/"Basic"/"Enhanced"
	set PSModeList			= $(STA_PSModeList)
	set PSModeValues		= $(STA_PSModeValues)
	set PSModeUIVal			= "Disabled"

	; configure as infrastructure station
	set NetTypeList			= $(STA_NetTypeList)
	set NetTypeValues		= $(STA_NetTypeValues)
	set NetTypeUIVal		= "Infrastructure Station"

	; configure for 2 Mb/s default
	set TxRateList			= $(STA_TxRateList)
	set TxRateValues		= $(STA_TxRateValues)
	set TxRateUIVal			= "Fully Auto"

	; configure for ATIM Window Disabled
	set ATIMWindowList			= $(STA_ATIMWindowList)
	set ATIMWindowValues		= $(STA_ATIMWindowValues)
	set ATIMWindowUIVal			= "Disabled"

	; configure for Listen interval at MAX
	set ListenIntervalList			= $(STA_ListenIntervalList)
	set ListenIntervalValues		= $(STA_ListenIntervalValues)
	set ListenIntervalUIVal			= "Maximum"

	; configure for RTS/CTS disabled
	set RTSThreshList		= $(RTSThreshList)
	set RTSThreshValues		= $(RTSThreshValues)
	set RTSThreshUIVal		= "Disabled"

	; configure for Fragmentation disabled
	set FragThreshList		= $(FragThreshList)
	set FragThreshValues	= $(FragThreshValues)
	set FragThreshUIVal		= "Disabled"

	; configure for WEP Disabled
	set WepReqList			= $(WepReqList)
	set WepReqValues		= $(WepReqValues)
	set WepReqUIVal			= "Disabled"

	; PHY parameters DS
	set PHYParmName			= "DSChannel";
	set PHYParmList			= $(DSChanList)
	set PHYParmValues		= $(DSChanValues)
	set PHYParmUIVal		= 6
	set PHYParmLabel		= "DS Channel:"

	; default SSID - to be customized by OEM customer
        set SSIDValue                   = "default"

    Set from = $(fatal)
    Set to = $(fatal)
    Goto $(StartLabel)

;-----------------------------------------------
; Installation Section
;-----------------------------------------------

installadapter = +
    ;
    ; Create/recreate the Registry's PCMCIA database entry for the PCnet-Mobile.
    ;

    set KeyPcmciaDataBase = ""
    OpenRegKey $(!REG_H_LOCAL) "" $(PcmciaDataBaseKeyName) $(MAXIMUM_ALLOWED) KeyPcmciaDataBase
    Shell "" ExCreateRegKey $(KeyPcmciaDataBase) "D\Link DWL-650 11Mbps WLAN Card"
    OpenRegKey $(!REG_H_LOCAL) "" $(PcmciaDataBaseKeyName)"\D\Link DWL-650 11Mbps WLAN Card" $(MAXIMUM_ALLOWED) KeyTemp
    SetRegValue $(KeyTemp) {Driver,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)}
    CloseRegKey $(KeyTemp)
    CloseRegKey $(KeyPcmciaDataBase)

    ;
    ; Check whether the same version of the software exists
    ;

    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

    Ifstr $(KeyProduct) != $(KeyNull)
	;
	; Same version already existed in the local machine
	; Popup the dialog and ask the user whether he wants to continue
	;
	CloseRegKey $(KeyProduct)

	ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
	   ;
	   ; Cannot Install the same software again
	   ;
	   Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
	       $(ProductVersion)
	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif

	   goto end
	else
	   ;
	   ; Add a new adapter card?
	   ;
	   Shell $(UtilityInf), CardExistedDlg

	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif

	   ifstr(i) $($R1) != "OK"
	       goto end
	   endif
	   set OldVersionExisted = $(TRUE)
	endif
    endif

;
;  dll load addition
;
    Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) NO

    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Goto ShellCodeError
    Else-Ifstr(i) $($R0) == STATUS_FAILED
	Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
	Goto fatal
    Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
	Goto successful
    Endif

    Set SrcDir = $($R1)

    install "Install-Dll"

    goto adaptersetup

;-----------------------------------------------
; Configuration Section
;-----------------------------------------------
;
;   Get the current values of all the parameters
;
configureadapter = +
    Ifstr $(KeyProduct) == $(KeyNull)
	OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
	Ifstr $(KeyProduct) == $(KeyNull)
	    set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	    Debug-Output "Cannot find component product key"
	    goto fatalregistry
	Endif
    Endif

    ;
    ; Get the other parameters;  they're attached to the service parameters key
    ;
    Debug-Output "INF: Shelling to FindService"
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "INF: FindService shell failure"
	Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
	Debug-Output "INF: FindService Shell error: "$($R0)
	Goto fatalregistry
    endif

    Set KeyParameters = $($R2)

    ;
    ;  We don't need the services key, so close it.
    ;
    CloseRegKey $($R1)

    Ifstr $(KeyParameters) == $(KeyNull)
	set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	Debug-Output "Cannot find component service"
	goto fatalregistry
    endif

    set OldVersionExisted = $(TRUE)

    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}

    ;
    ; Get the old values
    ;
    EnumRegValue $(KeyParameters) ValueList

	ForListDo $(ValueList)
		set ValueItem	= $($)
		set ValueName	= *($(ValueItem),1)
		set ValueData	= *($(ValueItem),4)
  ; resources
		ifstr(i) $(ValueName) == "IoBaseAddress"
			set IOBaseAddrItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "InterruptNumber"
			set IRQValueItem = $(ValueData)
  ; general - combo
		else-ifstr(i) $(ValueName) == "DSChannel"
			set PHYParmItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "NetworkType"
			set NetTypeItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "TxRate"
			set TxRateItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "ATIMWindow"
			set ATIMWindowItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "ListenInterval"
			set ListenIntervalItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "RTSThresh"
			set RTSThreshItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "FragThresh"
			set FragThreshItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "PSMode"
			set PSModeItem = $(ValueData)
		else-ifstr(i) $(ValueName) == "WepReq"
			set WepReqItem = $(ValueData)
  ; checkbox
		else-ifstr(i) $(ValueName) == "Pcmcia"
			set PcmciaValue = $(ValueData)
  ; edit
		else-ifstr(i) $(ValueName) == "SSID"
			set SSIDValue = $(ValueData)

		endif

	EndForListDo


	ifint $(PcmciaValue) == 1
		set Chk1 = "ON"
	else
		set Chk1 = "OFF"
	endif

	set IOBaseAddrUIVal = *($(IOBaseAddrList), ~($(IOBaseAddrValues),$(IOBaseAddrItem)))
	ifstr(i) $(IOBaseAddrUIVal) == ""
		set IOBaseAddrUIVal = *($(IOBaseAddrList), 1)
	endif

	set IRQValueUIVal = *($(IRQList), ~($(IRQValues),$(IRQValueItem)))
	ifstr(i) $(IRQValueUIVal) == ""
		set IRQValueUIVal = *($(IRQList), 6)
	endif

	set PHYParmUIVal = *($(PHYParmList), ~($(PHYParmValues),$(PHYParmItem)))
	ifstr(i) $(PHYParmUIVal) == ""
		set PHYParmUIVal = *($(PHYParmList), 1)
	endif

	set NetTypeUIVal = *($(NetTypeList), ~($(NetTypeValues),$(NetTypeItem)))
	ifstr(i) $(NetTypeUIVal) == ""
		set NetTypeUIVal = *($(NetTypeList), 1)
	endif

	set TxRateUIVal = *($(TxRateList), ~($(TxRateValues),$(TxRateItem)))
	ifstr(i) $(TxRateUIVal) == ""
		set TxRateUIVal = *($(TxRateList), 1)
	endif

	set ATIMWindowUIVal = *($(ATIMWindowList), ~($(ATIMWindowValues),$(ATIMWindowItem)))
	ifstr(i) $(ATIMWindowUIVal) == ""
		set ATIMWindowUIVal = *($(ATIMWindowList), 1)
	endif

	set ListenIntervalUIVal = *($(ListenIntervalList), ~($(ListenIntervalValues),$(ListenIntervalItem)))
	ifstr(i) $(ListenIntervalUIVal) == ""
		set ListenIntervalUIVal = *($(ListenIntervalList), 6)
	endif

	set RTSThreshUIVal = *($(RTSThreshList), ~($(RTSThreshValues),$(RTSThreshItem)))
	ifstr(i) $(RTSThreshUIVal) == ""
		set RTSThreshUIVal = *($(RTSThreshList), 6)
	endif

	set FragThreshUIVal = *($(FragThreshList), ~($(FragThreshValues),$(FragThreshItem)))
	ifstr(i) $(FragThreshUIVal) == ""
		set FragThreshUIVal = *($(FragThreshList), 6)
	endif

	set PSModeUIVal = *($(PSModeList), ~($(PSModeValues),$(PSModeItem)))
	ifstr(i) $(PSModeUIVal) == ""
		set PSModeUIVal = *($(PSModeList), 1)
	endif

	set WepReqUIVal = *($(WepReqList), ~($(WepReqValues),$(WepReqItem)))
	ifstr(i) $(WepReqUIVal) == ""
		set WepReqUIVal = *($(WepReqList), 1)
        endif

;  Save the settings as they were read from the Registry.

;    Shell $(ParamInf) Param_SaveValues
;    Set CurrParamSettings = $($R0)
;
;   Put up the adapter configuration dialog if necessary.
;
;   Note that $(CurrParamSettings) has the old known parameter values.
;
adaptersetup = +

;    Shell "" DebugConfiguration "before displaying dialog"

    Set from = adapteroptions


adapteroptions = +

    LoadLibrary "Disk 1" $(DialogDllName) hLib

    read-syms FileDependentDlg$(!STF_LANGUAGE)

    ui start "InputDlg"  $(hLib)

    set ExitButton  = $(ButtonPressed)

    Debug-Output " ButtonPressed "$(ButtonPressed)

    FreeLibrary $(hLib)

    ifstr(i) $(DLGEVENT) == "CONTINUE"
        set IOBaseAddrUIVal             = $(Combo1Out)
        set IRQValueUIVal               = $(Combo2Out)
        set TxRateUIVal                 = $(Combo3Out)
        set PHYParmUIVal                = $(Combo4Out)
        set NetTypeUIVal                = $(Combo5Out)
        set RTSThreshUIVal              = $(Combo6Out)
        set FragThreshUIVal             = $(Combo7Out)
        set PSModeUIVal                 = $(Combo8Out)
        set WepReqUIVal                 = $(Combo9Out)
        set ATIMWindowUIVal             = $(Combo10Out)
        set ListenIntervalUIVal = $(Combo11Out)

        set SSIDValue                   = *($(EditTextOut),1)

        Set Chk = *($(CheckItemsOut), 1)
        Ifstr(i) $(Chk) == "ON"
                Set PcmciaValue = 1
                set Chk1 = "ON"
        Else
                Set PcmciaValue = 0
                set Chk1 = "OFF"
        Endif
	set ExitButton          = $(ButtonPressed)

	ui pop 1
;        goto nextstep
    else-ifstr(i) $(DLGEVENT) == "EXIT"
	set CommonStatus = STATUS_USERCANCEL
	Debug-Output "Action: exit. Bye."
	ui pop 1
	goto end
    else
	;
	; Unknow command
	;
	ui pop 1

	Debug-Output "Action: unknown. Bye."
	goto end
    endif

    Debug-Output " Combo list out "$(ComboListItemsOut)

;
;   If installing, go create the necessary keys;
;   if configuring, they're already open.
;
skipoptions =+

    ifint $(OldVersionExisted) == $(TRUE)
	ifstr(i) $(!NTN_InstallMode) == configure
	    goto writeparameters
	endif
    endif
    StartWait
    ;
    ; Add Software Component
    ;
    ifint $(OldVersionExisted) == $(FALSE)

	ifstr(i) $(!NTN_InstallMode) == "install"
	   Ifstr(i) $(DoCopy) == "YES"

	      Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES

	      Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		  Goto ShellCodeError
	      Else-Ifstr(i) $($R0) == STATUS_FAILED
		  Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		  ifint $($ShellCode) != $(!SHELL_CODE_OK)
		      goto ShellCodeError
		  endif
		  set Error = $($R0)
		  Goto fatal
	      Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		  Goto successful
	      Endif

	      Set SrcDir = $($R1)

	   Endif

	   install "Install-Option"

	   ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
	      Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
	      ifint $($ShellCode) != $(!SHELL_CODE_OK)
		  goto ShellCodeError
	      endif
	      set Error = $($R0)
	      goto fatal
	   endif
	endif



	Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
	    $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
	    $(NetEventDLL)

	Set OEM_ABANDON_SOFTWARE = TRUE

	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	;
	;   At this point:
	;     $R1 contains the product version key handle;
	;     $R2 contains the NetRules subkey handle;
	;     $R3 contains the new Services key handle; and
	;     $R4 contains the Parameters key
	;     $R5 contains the Linkage Key
	;
	set RegistryErrorIndex = $($R0)
	set KeyProduct      = $($R1)
	Set SoftNetRulesKey = $($R2)
	CloseRegKey $($R3)
	CloseRegKey $($R4)
	CloseRegKey $($R5)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add software components"
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif

	set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
			   {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
			   {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
			   {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
			   {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
			   {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
			   {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

	Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add value list."
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif

	set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
			    {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
			    {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
			    {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
			    {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
			    {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

	Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	CloseRegKey $(KeyProduct)
	CloseRegKey $(SoftNetRulesKey)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Resgitry error: add value list."
	    goto fatalregistry
	endif
    endif
;
;   Create the HARDWARE\Netcard region and its corresponding service
;
    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)

    ifint $($R4) != -1
	Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
    endif

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "Cannot add hardware component"
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	EndWait
	Debug-Output "Registry error: add hardware component"
	CloseRegKey $($R1)
	CloseRegKey $($R2)
	CloseRegKey $($R3)
	goto fatalregistry
    endif

;
;   At this point:
;     $R1  Registry key variable for HARDWARE\Netcard\(n)
;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
;     $R3  Registry key handle for <service>\Parameters key
;     $R4  Adapter number assigned to adapter
;     $R5  Service name generated by combining svc name with adapter number
;
    set KeyParameters = $($R3)
    set KeyAdapterRules = $($R2)
    set AdapterNumber = $($R4)

    set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
                       {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardwareTitle)},+
                       {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareDescription)},+
		       {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
		       {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
		       {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

    Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error"
	goto ShellCodeError
    endif

    CloseRegKey $($R1)

    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)

    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
			{bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
			{class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
			{InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

    Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	EndWait
	Debug-Output "Resgitry error: add value list."
	CloseRegKey $(KeyParameters)
	CloseRegKey $(KeyAdapterRules)
	goto fatalregistry
    endif

    CloseRegKey $(KeyAdapterRules)

    goto writeparameters
;
;   REQUIRED:   $(KeyParameters) contains service Parameters key handle
;
writeparameters = +
    Shell $(UtilityInf), GetBusTypeNum

;	set BusTypeNum = $($R1)
; the above was not working so hard coding the bus type to 1 which represents
;			NdisInterfaceIsa
	set BusTypeNum		= 1
	set BusNumber		= 0

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

;
;   Add the rest of the parameters to the Services area
;
        set IOBaseAddrValue     = *($(IOBaseAddrValues), ~($(IOBaseAddrList),$(IOBaseAddrUIVal)))
        set IRQValue            = *($(IRQValues), ~($(IRQList),$(IRQValueUIVal)))
        set PHYParmValue        = *($(PHYParmValues), ~($(PHYParmList),$(PHYParmUIVal)))
        set NetTypeValue        = *($(NetTypeValues), ~($(NetTypeList),$(NetTypeUIVal)))
        set TxRateValue         = *($(TxRateValues), ~($(TxRateList),$(TxRateUIVal)))
        set ATIMWindowValue     = *($(ATIMWindowValues), ~($(ATIMWindowList),$(ATIMWindowUIVal)))
	set ListenIntervalValue	= *($(ListenIntervalValues), ~($(ListenIntervalList),$(ListenIntervalUIVal)))
        set RTSThreshValue      = *($(RTSThreshValues), ~($(RTSThreshList),$(RTSThreshUIVal)))
        set FragThreshValue     = *($(FragThreshValues), ~($(FragThreshList),$(FragThreshUIVal)))
        set PSModeValue         = *($(PSModeValues), ~($(PSModeList),$(PSModeUIVal)))
        set WepReqValue         = *($(WepReqValues), ~($(WepReqList),$(WepReqUIVal)))

        set NewValueList = {+
                {MediaType,       $(NoTitle),$(!REG_VT_DWORD),1},+
                {BusNumber,       $(NoTitle),$(!REG_VT_DWORD),$(BusNumber)},+
                {BusType,         $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
                {IoBaseAddress,   $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
                {IoLength,        $(NoTitle),$(!REG_VT_DWORD),64},+
                {InterruptNumber, $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
                {Pcmcia,          $(NoTitle),$(!REG_VT_DWORD),$(PcmciaValue)},+
                {MajorVersion,    $(NoTitle),$(!REG_VT_SZ),2},+
                {MinorVersion,    $(NoTitle),$(!REG_VT_SZ),0},+
                {SSID,            $(NoTitle),$(!REG_VT_SZ),   $(SSIDValue)},+
                {RTSThresh,       $(NoTitle),$(!REG_VT_DWORD),$(RTSThreshValue)},+
                {FragThresh,      $(NoTitle),$(!REG_VT_DWORD),$(FragThreshValue)},+
                {Encapsulation,   $(NoTitle),$(!REG_VT_DWORD),$(EthConvValue)},+
                {TxRate,          $(NoTitle),$(!REG_VT_DWORD),$(TxRateValue)},+
                {WepReq,          $(NoTitle),$(!REG_VT_DWORD),$(WepReqValue)},+
                {ATIMWindow,      $(NoTitle),$(!REG_VT_DWORD),$(ATIMWindowValue)},+
                {ListenInterval,  $(NoTitle),$(!REG_VT_DWORD),$(ListenIntervalValue)},+
                {NetworkType,     $(NoTitle),$(!REG_VT_DWORD),$(NetTypeValue)},+
                {PSMode,          $(NoTitle),$(!REG_VT_DWORD),$(PSModeValue)},+
                {PSLevel,         $(NoTitle),$(!REG_VT_DWORD),$(PSLevelValue)},+
                {DSChannel,       $(NoTitle),$(!REG_VT_DWORD),$(PHYParmValue)},+
        }

    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)

    CloseRegKey $(KeyParameters)

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	Debug-Output "Registry error: Add value list"
	goto fatalregistry
    endif

    EndWait

    goto successful

;-----------------------------------------------
; Binding section
;-----------------------------------------------
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal

;-----------------------------------------------
; Removeadapter section
;-----------------------------------------------

removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	; Remove Software Component
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    else
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $(!NTN_RegBase)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif

    goto end

;-----------------------------------------------
; Upgrade Software section
;-----------------------------------------------

UpgradeSoftware = +
    ;
    ; First determine whether we want to do upgrade or update for software
    ; or hardware component. Then we will determine whether the Mode is
    ; update or upgrade.
    ;
    ; If the same version of the product existed in the registry, we do
    ; update. Otherwise, we will do a upgrade
    ;
    ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	; Upgrade software component
	;
	; see whether the same version exist or not
	;
	OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

	Ifstr $(KeyProduct) != $(KeyNull)
	    GetRegValue $(KeyProduct),"MajorVersion", VersionInfo
	    set Version = *($(VersionInfo), 4)

	    ;
	    ; Update the binaries
	    ;
	    Shell $(UtilityInf), GetInfFileNameFromRegistry, $(KeyProduct)

	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		Debug-Output "ShellCode error"
		goto ShellCodeError
	    endif

	    set !UG_Filename = $($R0)

	    ifstr(i) $(!UG_Filename) != ""
		install "Install-Update"
		ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
		    goto fatal
		endif
	    endif

	    ; Upgrade the version number
	    ;
	    SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
	    SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}

	    ;
	    ; do nothing for update
	    ;
	    ifint $(Version) != $(ProductVersion)
	       ;
	       ; If the major version number is not the same,
	       ; it is major upgrade. So let Upgrade the product
	       ;
	       ;
	       ; make other upgrade change if necessary
	       ;
	    endif
	    CloseRegKey $(KeyProduct)
	else
	    ;
	    ; Cannot Open software key, goto ERROR
	    ;
	    goto fatalregistry
	endif
    else
	;
	; upgrade/update hardware component
	; There is no different between upgrade and update for hardware
	; component
	;
	; 1. Get the Service Name
	; 2. Change the NetRule section if necessary
	;
	OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) +
	      $(MAXIMUM_ALLOWED) NetworkCardKey
	Ifstr(i) $(NetworkCardKey) != $(KeyNull)
	    ;
	    ; Get Service name
	    ;
	    GetRegValue $(NetworkCardKey),"ServiceName", ServiceNameInfo
	    set ServiceName = *($(ServiceNameInfo), 4)

	    ;
	    ; Change the NetRule if necessary
	    ;
	    OpenRegKey $(NetworkCardKey) "" "NetRules" +
		$(MAXIMUM_ALLOWED) NetRuleKey
	    Ifstr(i) $(NetRuleKey) != $(KeyNull)
		;
		; Make the change....
		;
	    else
		;
		; Error, cannot open net rules key
		;
		goto fatalregistry
	    endif

	    CloseRegKey $(NetRules)
	    CloseRegKey $(NetworkCardKey)
	else
	    ;
	    ; Error, cannot open network card key
	    ;
	    goto fatalregistry
	endif
	;
	; 3. Change the service section of the hardware. i.e.,
	;    ParameterName change, value change, etc.
	;
	OpenRegKey $(!REG_H_LOCAL) "" +
	      $(!NTN_ServiceBase)"\"$(ServiceName) +
	      $(MAXIMUM_ALLOWED) ServiceKey

	Ifstr(i) $(ServiceKey) != $(KeyNull)
	    ;
	    ; Get the ServiceKey to change the Start value
	    ; or Type value. Or open Parameters key to
	    ; change the hardware parameters if necessary.
	    ;
	    CloseRegKey $(ServiceKey)
	else
	    ;
	    ; Error, cannot open network card key
	    ;
	    goto fatalregistry
	endif
    endif

    goto end
    ;
    ; End of Upgrade Software
    ;

;
;  Escape hatches
;
successful = +
    goto end

abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $($)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    EndForListDo

    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
	; Remove Software Component
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), FALSE
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif

    goto end

;
; warning display
;
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
	goto $(from)
    else
	goto "end"
    endif
;
; non fatal error display
;
nonfatalinfo = +
    Set Severity = STATUS
    Set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg
nonfatal = +
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    ifstr(i) $(Error) == ""
	Set Severity = NONFATAL
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(from)
    else
	goto "end"
    endif

;
;  Registry is broken
;
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
;
;  Netcard detection failure
;
fataldetect = +
    Shell $(UtilityInf),RegistryErrorString,CANNOT_DETECT
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error: cannot get an error string."
	goto ShellCodeError
    endif
    set Error = $($R0)
    Goto fatal
;
; fatal error display
;
fatal = +
    ifstr(i) $(Error) == ""
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif

    goto setfailed

;
;  Shelling error
;
ShellCodeError = +
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed

setfailed = +
    set CommonStatus = STATUS_FAILED
    ;
    ; if OEM_ABANDON_ON == TRUE, then remove the registry entries
    ;
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
	set OEM_ABANDON_ON = FALSE
	goto abandon
    endif
    goto end

end = +
    goto term

term = +

    Return $(CommonStatus)

[DebugConfiguration]

    Set InfName = "OEMNADE2.INF"
    Debug-Output $(InfName)" **CONFIGURATION STATE: "$($0)
    Debug-Output $(InfName)" IRQ_Level is "$(!p:IRQ_Level)
    Debug-Output $(InfName)" IOBaseAddrValue is "$(!p:IOBaseAddrValue)
    Debug-Output $(InfName)" TransceiverValue is "$(!p:TransceiverValue)
    Debug-Output $(InfName)" MemBaseAddrDec is "$(!p:MemBaseAddrDec)
    Debug-Output $(InfName)" MappedValue is "$(!p:MappedValue)

    return


;***************************************************************
;  INSTALL SECTIONS
;***************************************************************
[Install-Option]
    set STF_VITAL = ""

    ifstr(i) $(AddCopy) == "YES"

	;
	; Add the files to the copy list
	;
	;  BUGBUG: eliminate the "nt2" in the next line when Sunil fixes
	;      the other INF files
	;
	AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
        AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
	AddSectionFilesToCopyList Files-exe $(SrcDir) $(!STF_WINDOWSSYSPATH)
   	AddSectionFilesToCopyList Files-exe $(SrcDir) $(!STF_WINDOWSPATH)"\Profiles\All Users\desktop"
	AddSectionFilesToCopyList Files-exe $(SrcDir) $(!STF_WINDOWSPATH)"\Profiles\All Users\Start Menu\Programs\Startup"

    endif

    ifstr(i) $(DoCopy) == "YES"
       ; Copy files in the copy list
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList
    endif

    Exit

[Install-Update]
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ;set STF_VERSION     = "YES"

   AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
   AddSectionFilesToCopyList Files-Inf $(SrcDir) $(!STF_WINDOWSSYSPATH)
   AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   AddSectionFilesToCopyList Files-exe $(SrcDir) $(!STF_WINDOWSPATH)"\Profiles\All Users\desktop"
   AddSectionFilesToCopyList Files-exe $(SrcDir) $(!STF_WINDOWSPATH)"\Profiles\All Users\Start Menu\Programs\Startup"
	
   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList

   exit

[Install-Dll]
   set STF_VITAL        = ""
   AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList
   exit

[Source Media Descriptions]
    1  = "D-Link DWL-650 11Mbps WLAN Card"

[ProductType]
    STF_PRODUCT  = Winnt
    STF_PLATFORM = I386

[Files-Inf]
    1, oemsetnt.inf, SIZE=40558, RENAME=$(!UG_Filename)

[Files-GTWLAN11]
    1, gt11.sys, SIZE=12800

[Files-Dll]
    1, gt11.dll , SIZE=7168

[Files-exe]
    

[LanguagesSupported]
    ENG

[OptionsTextENG]
    GTWLAN11 = "D-Link DWL-650 11Mbps WLAN Card"

[FileConstantsENG]
    ProCaption   = "Windows NT Setup"
    ProCancel    = "Cancel"
    ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
		   "Are you sure you want to cancel copying files?"
    ProCancelCap = "Network Setup Message"
    ProText1     = "Copying:"
    ProText2     = "To:"

    FunctionTitle   = $(GenericAdapterName)" Setup"

    ProductSoftwareDescription = $(GenericDriverName)
    ProductHardwareDescription = $(GenericAdapterName)

    ProductSoftwareTitle =       $(GenericDriverName)
    ProductHardwareTitle =       $(GenericAdapterName)

    DialogDllName   = "gt11.dll"

    IOBaseAddrList = ^(IOBaseAddrChoices, 1)
    IOBaseAddrValues = ^(IOBaseAddrChoices, 2)

    IRQList  = ^(IRQChoices, 1)
    IRQValues = ^(IRQChoices, 2)

        DSChanList              = ^(DSChanChoices, 1)
	DSChanValues		= ^(DSChanChoices, 2)

	STA_NetTypeList 	= ^(STA_NetTypeChoices, 1)
	STA_NetTypeValues	= ^(STA_NetTypeChoices, 2)

	STA_TxRateList 		= ^(STA_TxRateChoices, 1)
	STA_TxRateValues	= ^(STA_TxRateChoices, 2)

	STA_ATIMWindowList 	= ^(STA_ATIMWindowChoices, 1)
        STA_ATIMWindowValues    = ^(STA_ATIMWindowChoices, 2)

	STA_ListenIntervalList	= ^(STA_ListenIntervalChoices, 1)
	STA_ListenIntervalValues= ^(STA_ListenIntervalChoices, 2)

	RTSThreshList 		= ^(RTSThreshChoices, 1)
	RTSThreshValues		= ^(RTSThreshChoices, 2)

	FragThreshList 		= ^(FragThreshChoices, 1)
	FragThreshValues	= ^(FragThreshChoices, 2)

	STA_PSModeList 		= ^(STA_PSModeChoices, 1)
	STA_PSModeValues	= ^(STA_PSModeChoices, 2)

        WepReqList              = ^(WepReqChoices, 1)
        WepReqValues            = ^(WepReqChoices, 2)

[DialogConstantsENG]
    Help        = "&Help"
    Exit        = "Cancel"
    OK          = "OK"
    HelpContext = ""
    Continue    = "Continue"
    Cancel      = "Cancel"

[MemoryMappedChoicesENG]
    Map_1 = 1, "ON"
    Map_2 = 0, "OFF"

[FileDependentDlgENG]
        DlgText                         = "Please select values for the follwing fields:"

	DlgType				= "RadioCombination"
	DlgTemplate			= "GT11"
	Caption				= $(FunctionTitle)

	CBOptionsGreyed		= {}
	NotifyFields		= {NO, NO}
	HelpContext			= $(!IDH_DB_OEMNADE2_INS)

	Combo1Label			= "I/O Base:"
	Combo2Label			= "IRQ Level:"
	Combo3Label			= "Tx Rate:"
	Combo4Label			= $(PHYParmLabel)
	Combo5Label			= "Mode:"
	Combo6Label			= "RTS Threshold:"
	Combo7Label			= "Fragmentation Threshold"
	Combo8Label			= "Power Saving:"
	Combo9Label			= "WEP:"
	Combo10Label		= "ATIM Window:"
	Combo11Label		= "Listen Interval:"

	Edit1Label			= "SS ID:"

	CheckBox1			= "PCMCIA card"

	Combo1List			= $(IOBaseAddrList)
	Combo1Out 			= $(IOBaseAddrUIVal)

	Combo2List			= $(IRQList)
	Combo2Out 			= $(IRQValueUIVal)

	Combo3List			= $(TxRateList)
	Combo3Out 			= $(TxRateUIVal)

	Combo4List			= $(PHYParmList)
	Combo4Out 			= $(PHYParmUIVal)

	Combo5List			= $(NetTypeList)
	Combo5Out 			= $(NetTypeUIVal)

	Combo6List			= $(RTSThreshList)
	Combo6Out 			= $(RTSThreshUIVal)

	Combo7List			= $(FragThreshList)
	Combo7Out 			= $(FragThreshUIVal)

	Combo8List			= $(PSModeList)
	Combo8Out 			= $(PSModeUIVal)

	Combo9List			= $(WepReqList)
	Combo9Out 			= $(WepReqUIVal)

	Combo10List			= $(ATIMWindowList)
	Combo10Out 			= $(ATIMWindowUIVal)

	Combo11List			= $(ListenIntervalList)
	Combo11Out 			= $(ListenIntervalUIVal)

	ComboListItemsIn 	= {Combo1List,Combo2List,Combo3List,+
							Combo4List, Combo5List, Combo6List,+
							Combo7List, Combo8List, Combo9List,+
							Combo10List, Combo11List+
							}
	ComboListItemsOut	= {Combo1Out,Combo2Out,Combo3Out,+
							Combo4Out, Combo5Out, Combo6Out,+
							Combo7Out, Combo8Out, Combo9Out,+
							Combo10Out, Combo11Out+
							}

	EditTextIn			= {$(SSIDValue)}
	EditTextLim			= {"32"}

        CheckItemsIn            = {$(Chk1)}

[IOBaseAddrChoices]
	IOBase_1 			= "200",512
	IOBase_2 			= "240",576
	IOBase_3 			= "280",640
	IOBase_4 			= "2C0",714
	IOBase_5 			= "300",768
	IOBase_6			=  "340",832
	IOBase_7			=  "380",896
	IOBase_8			=  "3C0",960

[IRQChoices]
	IRQ_1				= "3",3
	IRQ_2				= "4",4
	IRQ_3				= "5",5
	IRQ_4				= "7",7
	IRQ_5				= "9",9
	IRQ_6				= "10",10
	IRQ_7				= "11",11
	IRQ_8				= "12",12
	IRQ_9				= "15",15

[DSChanChoices]
	DSCHAN_1			= "1",1
	DSCHAN_2			= "2",2
	DSCHAN_3			= "3",3
	DSCHAN_4			= "4",4
	DSCHAN_5			= "5",5
	DSCHAN_6			= "6",6
	DSCHAN_7			= "7",7
	DSCHAN_8			= "8",8
	DSCHAN_9			= "9",9
	DSCHAN_10			= "10",10
	DSCHAN_11			= "11",11

[STA_NetTypeChoices]
	NETTYPE_ADHOC		= "Pseudo-IBSS Station",3
	NETTYPE_INFRA		= "Infrastructure Station",1

[STA_TxRateChoices]
	TXRATE_1			= "1 Mb/s", 1
	TXRATE_2			= "2 Mb/s", 2
	TXRATE_1_2			= "Auto 1 or 2 Mb/s", 3
	TXRATE_55			= "5.5 Mb/s", 4
	TXRATE_11			= "11 Mb/s", 8
	TXRATE_ALL			= "Fully Auto", 15

[STA_ATIMWindowChoices]
	ATIMWIN_0			= "Disabled", 0
	ATIMWIN_10			= "10 ms", 10
	ATIMWIN_20			= "20 ms", 20
	ATIMWIN_30			= "30 ms", 30
	ATIMWIN_40			= "40 ms", 40
	ATIMWIN_50			= "50 ms", 50
	ATIMWIN_60			= "60 ms", 60
	ATIMWIN_70			= "70 ms", 70
	ATIMWIN_80			= "80 ms", 80
	ATIMWIN_90			= "90 ms", 90

[STA_ListenIntervalChoices]
	LISTENINT_1			= "1 Beacon Per", 1
	LISTENINT_2			= "2 Beacon Per", 2
	LISTENINT_3			= "3 Beacon Per", 3
	LISTENINT_4			= "4 Beacon Per", 4
	LISTENINT_5			= "5 Beacon Per", 5
	LISTENINT_M			= "Maximum", 1

[STA_PSModeChoices]
	PS_DIS				= "Disabled", 0
	PS_BASIC			= "Basic", 1
	PS_ENH				= "Enhanced", 2

[RTSThreshChoices]
	RTSTHRESH_256		= "256 Bytes", 256
	RTSTHRESH_512		= "512 Bytes", 512
	RTSTHRESH_768		= "768 Bytes", 768
	RTSTHRESH_1024		= "1024 Bytes", 1024
	RTSTHRESH_1280		= "1280 Bytes", 1280
	RTSTHRESH_DIS		= "Disabled", 2560

[FragThreshChoices]
	FRAGTHRESH_256		= "256 Bytes", 256
	FRAGTHRESH_512		= "512 Bytes", 512
	FRAGTHRESH_768		= "768 Bytes", 768
	FRAGTHRESH_1024		= "1024 Bytes", 1024
	FRAGTHRESH_1280		= "1280 Bytes", 1280
	FRAGTHRESH_DIS		= "Disabled", 2560

[WepReqChoices]
	WEP_DIS				= "Disabled", 0
	WEP_MAN				= "Mandatory", 2

[STA_List]
	"STA_HAR_PCM"
	"STA_LUC_PCM"

[DS_List]
	"STA_HAR_PCM"
        "STA_LUC_PCM"


[ExCreateRegKey]
    Debug-Output "******************Entering [ExCreateRegKey]******************"
    set ECR_Result          = NO_ERROR
    set ECR_BaseKeyHandle   = $($0)
    set ECR_NewPath         = $($1)
    set KeyNull         = ""
    set MAXIMUM_ALLOWED   = 33554432
    Debug-Output "ExCreateRegKey - ECR_BaseKeyHandle = "$(ECR_BaseKeyHandle)
    Debug-Output "                 ECR_NewPath = "$(ECR_NewPath)
    Debug-Output "                 MAXIMUM_ALLOWED = "$(MAXIMUM_ALLOWED)
    Debug-Output "                 KeyNull = "$(KeyNull)
    OpenRegKey $(ECR_BaseKeyHandle) "" $(ECR_NewPath) $(MAXIMUM_ALLOWED) +
	       ECR_BaseKey
    Debug-Output "ECR_BaseKey = "$(ECR_BaseKey)
    Debug-Output "    OpenRegKey returned "$($R0)
    Ifstr $(ECR_BaseKey) == $(KeyNull)
	Debug-Output "ECR_BaseKey == KeyNull"
    Else
	Debug-Output "ECR_BaseKey != KeyNull"
	set ECR_KeyHandle = $(ECR_BaseKey)
	goto  ECR_Return
    Endif
    set ECR_TmpPath = ""
    Split-String $(ECR_NewPath) "\" ECR_PList
    Debug-Output "ECR_PList = "$(ECR_PList)
    ForListDo $(ECR_PList)
	Ifstr(i) $($) != "\"
	    Ifint $(#) == 1
		set ECR_TmpPath = $($)
	    Else
		set ECR_TmpPath = $(ECR_TmpPath)"\"$($)
	    Endif
	    Debug-Output "Determining if "$(ECR_TmpPath)" exists"
	    OpenRegKey $(ECR_BaseKeyHandle) "" $(ECR_TmpPath) $(MAXIMUM_ALLOWED) ECR_BaseKey
	    Ifstr $(ECR_BaseKey) == $(KeyNull)
		Debug-Output "Creating "$(ECR_TmpPath)
		CreateRegKey $(ECR_BaseKeyHandle)  {$(ECR_TmpPath),0,GenericClass} "" $(MAXIMUM_ALLOWED) "" ECR_KeyHandle
		Ifstr(i) $(ECR_KeyHandle) == $(KeyNull)
		    set ECR_Result = $($R0)
		    goto ECR_Return
		Endif
	    Endif
	Endif
    EndForListDo
ECR_Return = +
    return $(ECR_Result) $(ECR_KeyHandle)
